<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="HDLCompilers" num="261" delta="new" ><arg fmt="%s" index="1">&quot;../WarpSE.v&quot; line 56 </arg>Connection to output port &apos;<arg fmt="%s" index="2">SS</arg>&apos; does not match port size
</msg>

<msg type="info" file="Xst" num="2679" delta="new" >Register &lt;<arg fmt="%s" index="1">BA&lt;1&gt;</arg>&gt; in unit &lt;<arg fmt="%s" index="2">RAM</arg>&gt; has a constant value of <arg fmt="%s" index="3">0</arg> during circuit operation. The register is replaced by logic.
</msg>

<msg type="warning" file="Xst" num="1305" delta="new" >Output &lt;<arg fmt="%s" index="1">RCLK</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="1305" delta="new" >Output &lt;<arg fmt="%s" index="1">SS&lt;2&gt;</arg>&gt; is never assigned. Tied to value <arg fmt="%s" index="2">0</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">BACT</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">CLK</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="new" >Input &lt;<arg fmt="%s" index="1">SW&lt;2&gt;</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="1426" delta="new" >The value init of the FF/Latch <arg fmt="%s" index="1">0</arg> hinder the constant cleaning in the block <arg fmt="%s" index="2">RESDone</arg>.
You should achieve better results by setting this init to <arg fmt="%i" index="3">1</arg>.
</msg>

<msg type="warning" file="Xst" num="1426" delta="new" >The value init of the FF/Latch <arg fmt="%s" index="1">0</arg> hinder the constant cleaning in the block <arg fmt="%s" index="2">Disable</arg>.
You should achieve better results by setting this init to <arg fmt="%i" index="3">1</arg>.
</msg>

<msg type="warning" file="Xst" num="1426" delta="new" >The value init of the FF/Latch <arg fmt="%s" index="1">RESDone</arg> hinder the constant cleaning in the block <arg fmt="%s" index="2">WarpSE</arg>.
You should achieve better results by setting this init to <arg fmt="%i" index="3">1</arg>.
</msg>

<msg type="warning" file="Xst" num="1426" delta="new" >The value init of the FF/Latch <arg fmt="%s" index="1">Disable</arg> hinder the constant cleaning in the block <arg fmt="%s" index="2">WarpSE</arg>.
You should achieve better results by setting this init to <arg fmt="%i" index="3">1</arg>.
</msg>

</messages>

