                           Performance Summary Report
                           --------------------------

Design:     WarpSE
Device:     XC95144XL-10-TQ100
Speed File: Version 3.0
Program:    Timing Report Generator:  version P.20131013
Date:       Mon Apr 10 20:34:36 2023

Performance Summary:

Pad to Pad (tPD)                          :         11.0ns (1 macrocell levels)
Pad 'A_FSB<23>' to Pad 'nRAS'                                     

Clock net 'FCLK' path delays:

Clock Pad to Output Pad (tCO)             :         14.5ns (2 macrocell levels)
Clock Pad 'FCLK' to Output Pad 'nRES'                                     (GCK)

Clock to Setup (tCYC)                     :         20.1ns (2 macrocell levels)
Clock to Q, net 'cnt/IS_FSM_FFd1.Q' to DFF Setup(D) at 'cnt/LTimer<0>.D'        (GCK)
Target FF drives output net 'cnt/LTimer<0>'

Setup to Clock at the Pad (tSU)           :         16.6ns (1 macrocell levels)
Data signal 'A_FSB<23>' to DFF D input Pin at 'cnt/LTimer<0>.D'
Clock pad 'FCLK'                                                          (GCK)

                          Minimum Clock Period: 20.1ns
                     Maximum Internal Clock Speed: 49.7Mhz
                            (Limited by Cycle Time)

Clock net 'C16M' path delays:

Clock Pad to Output Pad (tCO)             :         13.5ns (2 macrocell levels)
Clock Pad 'C16M' to Output Pad 'nADoutLE0'                                (GCK)

Clock to Setup (tCYC)                     :         11.0ns (1 macrocell levels)
Clock to Q, net 'iobm/IOS_FSM_FFd7.Q' to DFF Setup(D) at 'nLDS_IOB.D'        (GCK)
Target FF drives output net 'nLDS_IOB'

Setup to Clock at the Pad (tSU)           :          6.5ns (0 macrocell levels)
Data signal 'C8M' to DFF D input Pin at 'iobm/C8Mr.D'
Clock pad 'C16M'                                                          (GCK)

                          Minimum Clock Period: 11.0ns
                     Maximum Internal Clock Speed: 90.9Mhz
                            (Limited by Cycle Time)

Clock net 'C8M' path delays:

Clock Pad to Output Pad (tCO)             :          5.8ns (1 macrocell levels)
Clock Pad 'C8M' to Output Pad 'nVMA_IOB'                                  (GCK)

Clock to Setup (tCYC)                     :         10.0ns (1 macrocell levels)
Clock to Q, net 'nVMA_IOB.Q' to TFF Setup(D) at 'nVMA_IOB.D'              (GCK)
Target FF drives output net 'nVMA_IOB'

Setup to Clock at the Pad (tSU)           :          6.5ns (0 macrocell levels)
Data signal 'nBERR_IOB' to DFF D input Pin at 'IOBERR.D'
Clock pad 'C8M'                                                           (GCK)

                          Minimum Clock Period: 10.0ns
                     Maximum Internal Clock Speed: 100.0Mhz
                            (Limited by Cycle Time)

--------------------------------------------------------------------------------
                            Pad to Pad (tPD) (nsec)

\ From        A     A     A     A     A     A     A     A     A     A     A
 \            _     _     _     _     _     _     _     _     _     _     _
  \           F     F     F     F     F     F     F     F     F     F     F
   \          S     S     S     S     S     S     S     S     S     S     S
    \         B     B     B     B     B     B     B     B     B     B     B
     \        <     <     <     <     <     <     <     <     <     <     <
      \       1     1     1     1     1     1     1     1     1     1     1
       \      0     1     2     3     4     5     6     7     8     9     >
        \     >     >     >     >     >     >     >     >     >     >      
  To     \------------------------------------------------------------------

RA<0>                                                                  10.0
RA<10>                                               10.0                  
RA<11>                                                           11.0      
RA<1>      10.0                                                            
RA<2>                                          10.0                        
RA<3>                                                            10.0      
RA<4>            10.0                                                      
RA<5>                  10.0                                                
RA<6>                        10.0                                          
RA<7>                              10.0                                    
RA<8>                                                      10.0            
RA<9>                                    10.0                              
nDinOE                                                                     
nRAMLWE                                                                    
nRAMUWE                                                                    
nRAS                                                                       
nROMCS                                                                     
nROMWE                                                                     

--------------------------------------------------------------------------------
                            Pad to Pad (tPD) (nsec)

\ From        A     A     A     A     A     A     A     A     A     A     A
 \            _     _     _     _     _     _     _     _     _     _     _
  \           F     F     F     F     F     F     F     F     F     F     F
   \          S     S     S     S     S     S     S     S     S     S     S
    \         B     B     B     B     B     B     B     B     B     B     B
     \        <     <     <     <     <     <     <     <     <     <     <
      \       2     2     2     2     2     3     4     5     6     7     8
       \      0     1     2     3     >     >     >     >     >     >     >
        \     >     >     >     >                                          
  To     \------------------------------------------------------------------

RA<0>                                                                      
RA<10>                                                           10.0      
RA<11>     11.0                                                            
RA<1>                              10.0                                    
RA<2>                                                            10.0      
RA<3>      10.0                                                            
RA<4>                                    10.0                              
RA<5>                                          10.0                        
RA<6>                                                10.0                  
RA<7>                                                      10.0            
RA<8>            10.0                                                      
RA<9>                                                                  10.0
nDinOE     10.0  10.0  10.0  10.0                                          
nRAMLWE                                                                    
nRAMUWE                                                                    
nRAS                   11.0  11.0                                          
nROMCS     10.0  10.0  10.0  10.0                                          
nROMWE                                                                     

--------------------------------------------------------------------------------
                            Pad to Pad (tPD) (nsec)

\ From        A     n     n     n     n
 \            _     A     L     U     W
  \           F     S     D     D     E
   \          S     _     S     S     _
    \         B     F     _     _     F
     \        <     S     F     F     S
      \       9     B     S     S     B
       \      >           B     B      
        \                              
  To     \------------------------------

RA<0>      10.0                        
RA<10>                                 
RA<11>                                 
RA<1>                                  
RA<2>                                  
RA<3>                                  
RA<4>                                  
RA<5>                                  
RA<6>                                  
RA<7>                                  
RA<8>                                  
RA<9>                                  
nDinOE           10.0              10.0
nRAMLWE                10.0        10.0
nRAMUWE                      11.0  11.0
nRAS             11.0                  
nROMCS                                 
nROMWE           10.0              10.0

--------------------------------------------------------------------------------
                      Clock Pad to Output Pad (tCO) (nsec)

\ From         C     C     F
 \             1     8     C
  \            6     M     L
   \           M           K
    \                       
     \                      
      \                     
       \                    
        \                   
         \                  
  To      \------------------

RA<0>                   13.5
RA<10>                  13.5
RA<11>                  14.5
RA<1>                   13.5
RA<2>                   13.5
RA<3>                   13.5
RA<4>                   13.5
RA<5>                   13.5
RA<6>                   13.5
RA<7>                   13.5
RA<8>                   13.5
RA<9>                   13.5
nADoutLE0   13.5        13.5
nADoutLE1                5.8
nAS_IOB      5.8        14.5
nAoutOE                  5.8
nBERR_FSB                5.8
nBR_IOB                  5.8
nCAS                     5.8
nDTACK_FSB               5.8
nDinLE       5.8            
nDoutOE     13.5        13.5
nLDS_IOB     5.8        14.5
nOE                      5.8
nRAMLWE                 13.5
nRAMUWE                 14.5
nRAS                    14.5
nRES                    14.5
nROMCS                  13.5
nUDS_IOB     5.8        14.5
nVMA_IOB           5.8  14.5
nVPA_FSB                 5.8

--------------------------------------------------------------------------------
                   Setup to Clock at Pad (tSU or tSUF) (nsec)

\ From         C     C     F
 \             1     8     C
  \            6     M     L
   \           M           K
    \                       
     \                      
      \                     
       \                    
        \                   
         \                  
  To      \------------------

A_FSB<10>               16.6
A_FSB<11>               16.6
A_FSB<12>               16.6
A_FSB<13>               16.6
A_FSB<14>               16.6
A_FSB<15>               16.6
A_FSB<16>               16.6
A_FSB<17>               16.6
A_FSB<18>               16.6
A_FSB<19>               16.6
A_FSB<20>               16.6
A_FSB<21>               16.6
A_FSB<22>               16.6
A_FSB<23>               16.6
A_FSB<8>                16.6
A_FSB<9>                16.6
C8M          6.5            
E                  6.5   6.5
nAS_FSB                 16.6
nBERR_IOB          6.5      
nDTACK_IOB         6.5      
nIPL2                    6.5
nLDS_FSB                 6.5
nRES               6.5   6.5
nUDS_FSB                 6.5
nVPA_IOB           6.5      
nWE_FSB                 16.6

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 I     I     I     I     I     Q     R     R     R     c
 \                     O     O     O     O     O     o     A     e     e     n
  \                    L     N     R     U     W     S     M     f     f     t
   \                   0     P     D     0     R     R     R     R     U     /
    \                  .     R     R     .     R     e     e     e     r     E
     \                 Q     e     E     Q     E     a     a     q     g     r
      \                      a     Q           Q     d     d     .     .     <
       \                     d     .           .     y     y     Q     Q     0
        \                    y     Q           Q     .     .                 >
         \                   .                       Q     Q                 .
          \                  Q                                               Q
           \                                                                  
            \                                                                 
             \                                                                
              \                                                               
               \                                                              
                \                                                             
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
IOL0.D              11.0                                                      
IONPReady.D               11.0                                                
IORDREQ.D                       10.0                                          
IOU0.D                                11.0                                    
IOWRREQ.D                                   10.0                              
QoSReady.D                                        10.0                        
RAMReady.D                                                    11.0  11.0      
RefReq.CE                                                                 10.0
RefReq.D                                                                      
RefUrg.CE                                                                 10.0
RefUrg.D                                                                      
cnt/Er<1>.D                                                               10.0
cnt/IS_FSM_FFd1.D                                                         10.0
cnt/IS_FSM_FFd2.D                                                         10.0
cnt/LTimer<0>.D                                                           19.1
cnt/LTimer<10>.D                                                          10.0
cnt/LTimer<11>.D                                                          10.0
cnt/LTimer<1>.D                                                           19.1
cnt/LTimer<2>.D                                                           10.0
cnt/LTimer<3>.D                                                           10.0
cnt/LTimer<4>.D                                                           10.0
cnt/LTimer<5>.D                                                           10.0
cnt/LTimer<6>.D                                                           10.0
cnt/LTimer<7>.D                                                           10.0
cnt/LTimer<8>.D                                                           10.0
cnt/LTimer<9>.D                                                           11.0
cnt/LTimerTC.D                                                                
cnt/Timer<0>.CE                                                           10.0
cnt/Timer<0>.D                                                            10.0
cnt/Timer<1>.CE                                                           10.0
cnt/Timer<1>.D                                                            10.0
cnt/Timer<2>.CE                                                           10.0
cnt/Timer<2>.D                                                            10.0
cnt/Timer<3>.CE                                                           10.0
cnt/Timer<3>.D                                                            10.0
cnt/TimerTC.CE                                                            10.0
cnt/TimerTC.D                                                                 
cnt/WS<0>.D                                                                   
cnt/WS<1>.D                                                                   
cnt/WS<2>.D                                                                   
cnt/WS<3>.D                                                                   
cs/nOverlay.D                                                                 
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                                  
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                                  
iobs/Sent.D                                                                   
iobs/TS_FSM_FFd1.D                                                            
iobs/TS_FSM_FFd2.D                                                            
nADoutLE1.D                                                                   
nAoutOE.D                                                                     
nBERR_FSB.D                                                                   
nBR_IOB.D                                                                     
nCAS.D                                                        11.0  11.0      
nDTACK_FSB.D              11.0                    10.0  11.0                  
nOE.D                                                                         
nRESout.D                                                                     
nVPA_FSB.D                10.0                                                
ram/BACTr.D                                                                   
ram/DTACKr.D                                                                  
ram/RASEL.D                                                                   
ram/RASEN.D                                                   11.0  11.0      
ram/RASrf.D                                                                   
ram/RASrr.D                                                         10.0      
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             
ram/RS_FSM_FFd4.D                                                             
ram/RS_FSM_FFd5.D                                                             
ram/RS_FSM_FFd6.D                                                             
ram/RS_FSM_FFd7.D                                             11.0  10.0      
ram/RS_FSM_FFd8.D                                             11.0  11.0      
ram/RefDone.D                                                 10.0  10.0      

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 c     c     c     c     c     c     c     c     c     c
 \                     n     n     n     n     n     n     n     n     n     n
  \                    t     t     t     t     t     t     t     t     t     t
   \                   /     /     /     /     /     /     /     /     /     /
    \                  E     I     I     L     L     L     L     L     L     L
     \                 r     S     S     T     T     T     T     T     T     T
      \                <     _     _     i     i     i     i     i     i     i
       \               1     F     F     m     m     m     m     m     m     m
        \              >     S     S     e     e     e     e     e     e     e
         \             .     M     M     r     r     r     r     r     r     r
          \            Q     _     _     <     <     <     <     <     <     <
           \                 F     F     0     1     1     1     2     3     4
            \                F     F     >     0     1     >     >     >     >
             \               d     d     .     >     >     .     .     .     .
              \              1     2     Q     .     .     Q     Q     Q     Q
               \             .     .           Q     Q                        
                \            Q     Q                                          
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
IOL0.D                                                                        
IONPReady.D                                                                   
IORDREQ.D                                                                     
IOU0.D                                                                        
IOWRREQ.D                                                                     
QoSReady.D                            10.0              10.0                  
RAMReady.D                                                                    
RefReq.CE           10.0                                                      
RefReq.D                                                                      
RefUrg.CE           10.0                                                      
RefUrg.D                                                                      
cnt/Er<1>.D                                                                   
cnt/IS_FSM_FFd1.D   10.0  10.0  10.0                                          
cnt/IS_FSM_FFd2.D   10.0  10.0  10.0                                          
cnt/LTimer<0>.D     19.1  20.1  20.1  19.1  19.1  19.1  19.1  19.1  19.1  19.1
cnt/LTimer<10>.D    10.0  10.0  10.0  10.0  10.0        10.0  10.0  10.0  10.0
cnt/LTimer<11>.D    10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0
cnt/LTimer<1>.D     19.1  20.1  20.1  19.1  19.1  19.1  19.1  19.1  19.1  19.1
cnt/LTimer<2>.D     10.0  10.0  10.0  10.0              10.0  10.0            
cnt/LTimer<3>.D     10.0  10.0  10.0  10.0              10.0  10.0  10.0      
cnt/LTimer<4>.D     10.0  10.0  10.0  10.0              10.0  10.0  10.0  10.0
cnt/LTimer<5>.D     10.0  10.0  10.0  10.0              10.0  10.0  10.0  10.0
cnt/LTimer<6>.D     10.0  10.0  10.0  10.0              10.0  10.0  10.0  10.0
cnt/LTimer<7>.D     10.0  10.0  10.0  10.0              10.0  10.0  10.0  10.0
cnt/LTimer<8>.D     10.0  10.0  10.0  10.0              10.0  10.0  10.0  10.0
cnt/LTimer<9>.D     11.0  10.0  11.0  11.0              11.0  11.0  11.0  11.0
cnt/LTimerTC.D                        10.0  10.0  10.0  10.0  10.0  10.0  10.0
cnt/Timer<0>.CE     10.0                                                      
cnt/Timer<0>.D      10.0                                                      
cnt/Timer<1>.CE     10.0                                                      
cnt/Timer<1>.D      10.0                                                      
cnt/Timer<2>.CE     10.0                                                      
cnt/Timer<2>.D      10.0                                                      
cnt/Timer<3>.CE     10.0                                                      
cnt/Timer<3>.D      10.0                                                      
cnt/TimerTC.CE      10.0                                                      
cnt/TimerTC.D                                                                 
cnt/WS<0>.D                                                                   
cnt/WS<1>.D                                                                   
cnt/WS<2>.D                                                                   
cnt/WS<3>.D                                                                   
cs/nOverlay.D                                                                 
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                                  
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                                  
iobs/Sent.D                                                                   
iobs/TS_FSM_FFd1.D                                                            
iobs/TS_FSM_FFd2.D                                                            
nADoutLE1.D                                                                   
nAoutOE.D                 11.0  11.0                                          
nBERR_FSB.D                                                                   
nBR_IOB.D                 10.0  10.0                                          
nCAS.D                                                                        
nDTACK_FSB.D                                                                  
nOE.D                                                                         
nRESout.D                 10.0  10.0                                          
nVPA_FSB.D                                                                    
ram/BACTr.D                                                                   
ram/DTACKr.D                                                                  
ram/RASEL.D                                                                   
ram/RASEN.D                                                                   
ram/RASrf.D                                                                   
ram/RASrr.D                                                                   
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             
ram/RS_FSM_FFd4.D                                                             
ram/RS_FSM_FFd5.D                                                             
ram/RS_FSM_FFd6.D                                                             
ram/RS_FSM_FFd7.D                                                             
ram/RS_FSM_FFd8.D                                                             
ram/RefDone.D                                                                 

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 c     c     c     c     c     c     c     c     c     c
 \                     n     n     n     n     n     n     n     n     n     n
  \                    t     t     t     t     t     t     t     t     t     t
   \                   /     /     /     /     /     /     /     /     /     /
    \                  L     L     L     L     L     L     T     T     T     T
     \                 T     T     T     T     T     T     i     i     i     i
      \                i     i     i     i     i     i     m     m     m     m
       \               m     m     m     m     m     m     e     e     e     e
        \              e     e     e     e     e     e     r     r     r     r
         \             r     r     r     r     r     r     <     <     <     <
          \            <     <     <     <     <     T     0     1     2     3
           \           5     6     7     8     9     C     >     >     >     >
            \          >     >     >     >     >     .     .     .     .     .
             \         .     .     .     .     .     Q     Q     Q     Q     Q
              \        Q     Q     Q     Q     Q                              
               \                                                              
                \                                                             
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
IOL0.D                                                                        
IONPReady.D                                                                   
IORDREQ.D                                                                     
IOU0.D                                                                        
IOWRREQ.D                                                                     
QoSReady.D                                                                    
RAMReady.D                                                                    
RefReq.CE                                                                     
RefReq.D                                                10.0  10.0  10.0  10.0
RefUrg.CE                                                                     
RefUrg.D                                                      10.0  10.0  10.0
cnt/Er<1>.D                                                                   
cnt/IS_FSM_FFd1.D                                 10.0                        
cnt/IS_FSM_FFd2.D                                 10.0                        
cnt/LTimer<0>.D     19.1  19.1  19.1  19.1  19.1                              
cnt/LTimer<10>.D    10.0  10.0  10.0  10.0  10.0                              
cnt/LTimer<11>.D    10.0  10.0  10.0  10.0  10.0                              
cnt/LTimer<1>.D     19.1  19.1  19.1  19.1  19.1                              
cnt/LTimer<2>.D                                                               
cnt/LTimer<3>.D                                                               
cnt/LTimer<4>.D                                                               
cnt/LTimer<5>.D     10.0                                                      
cnt/LTimer<6>.D     10.0  10.0                                                
cnt/LTimer<7>.D     10.0  10.0  10.0                                          
cnt/LTimer<8>.D     10.0  10.0  10.0  10.0                                    
cnt/LTimer<9>.D     11.0  11.0  11.0  11.0  10.0                              
cnt/LTimerTC.D      10.0  10.0  10.0  10.0  10.0                              
cnt/Timer<0>.CE                                                               
cnt/Timer<0>.D                                          10.0                  
cnt/Timer<1>.CE                                                               
cnt/Timer<1>.D                                          10.0  10.0            
cnt/Timer<2>.CE                                                               
cnt/Timer<2>.D                                          10.0  10.0  10.0      
cnt/Timer<3>.CE                                                               
cnt/Timer<3>.D                                          10.0  10.0  10.0  10.0
cnt/TimerTC.CE                                                                
cnt/TimerTC.D                                           10.0  10.0  10.0  10.0
cnt/WS<0>.D                                                                   
cnt/WS<1>.D                                                                   
cnt/WS<2>.D                                                                   
cnt/WS<3>.D                                                                   
cs/nOverlay.D                                                                 
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                                  
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                                  
iobs/Sent.D                                                                   
iobs/TS_FSM_FFd1.D                                                            
iobs/TS_FSM_FFd2.D                                                            
nADoutLE1.D                                                                   
nAoutOE.D                                                                     
nBERR_FSB.D                                                                   
nBR_IOB.D                                                                     
nCAS.D                                                                        
nDTACK_FSB.D                                                                  
nOE.D                                                                         
nRESout.D                                                                     
nVPA_FSB.D                                                                    
ram/BACTr.D                                                                   
ram/DTACKr.D                                                                  
ram/RASEL.D                                                                   
ram/RASEN.D                                                                   
ram/RASrf.D                                                                   
ram/RASrr.D                                                                   
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             
ram/RS_FSM_FFd4.D                                                             
ram/RS_FSM_FFd5.D                                                             
ram/RS_FSM_FFd6.D                                                             
ram/RS_FSM_FFd7.D                                                             
ram/RS_FSM_FFd8.D                                                             
ram/RefDone.D                                                                 

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 c     c     c     c     c     c     c     f     i     i
 \                     n     n     n     n     n     n     s     s     o     o
  \                    t     t     t     t     t     t     /     b     b     b
   \                   /     /     /     /     /     /     n     /     s     s
    \                  T     W     W     W     W     n     O     A     /     /
     \                 i     S     S     S     S     I     v     S     C     I
      \                m     <     <     <     <     P     e     r     l     O
       \               e     0     1     2     3     L     r     f     e     A
        \              r     >     >     >     >     2     l     .     a     C
         \             T     .     .     .     .     r     a     Q     r     T
          \            C     Q     Q     Q     Q     .     y           1     r
           \           .                             Q     .           .     .
            \          Q                                   Q           Q     Q
             \                                                                
              \                                                               
               \                                                              
                \                                                             
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
IOL0.D                                                  11.0  11.0            
IONPReady.D                                                   11.0            
IORDREQ.D                                               11.0  11.0        10.0
IOU0.D                                                  11.4  11.0            
IOWRREQ.D                                               11.0  11.0        10.0
QoSReady.D                11.4  11.4  11.4  11.4              19.1            
RAMReady.D                                                    11.0            
RefReq.CE                                                                     
RefReq.D                                                                      
RefUrg.CE                                                                     
RefUrg.D                                                                      
cnt/Er<1>.D                                                                   
cnt/IS_FSM_FFd1.D   10.0                          10.0                        
cnt/IS_FSM_FFd2.D   10.0                                                      
cnt/LTimer<0>.D     19.1                                      20.1            
cnt/LTimer<10>.D    10.0                                                      
cnt/LTimer<11>.D    10.0                                                      
cnt/LTimer<1>.D     19.1                                      20.1            
cnt/LTimer<2>.D     10.0                                                      
cnt/LTimer<3>.D     10.0                                                      
cnt/LTimer<4>.D     10.0                                                      
cnt/LTimer<5>.D     10.0                                                      
cnt/LTimer<6>.D     10.0                                                      
cnt/LTimer<7>.D     10.0                                                      
cnt/LTimer<8>.D     10.0                                                      
cnt/LTimer<9>.D     11.0                                                      
cnt/LTimerTC.D                                                                
cnt/Timer<0>.CE                                                               
cnt/Timer<0>.D      10.0                                                      
cnt/Timer<1>.CE                                                               
cnt/Timer<1>.D      10.0                                                      
cnt/Timer<2>.CE                                                               
cnt/Timer<2>.D      10.0                                                      
cnt/Timer<3>.CE                                                               
cnt/Timer<3>.D      10.0                                                      
cnt/TimerTC.CE                                                                
cnt/TimerTC.D                                                                 
cnt/WS<0>.D               10.0                                10.0            
cnt/WS<1>.D               10.0  10.0                          11.0            
cnt/WS<2>.D               10.0  10.0  10.0                    10.0            
cnt/WS<3>.D               10.0  10.0  10.0  10.0              10.0            
cs/nOverlay.D                                           10.0  10.0            
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                  11.0            
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                  11.0            
iobs/Sent.D                                             11.4  11.4            
iobs/TS_FSM_FFd1.D                                                        10.0
iobs/TS_FSM_FFd2.D                                      11.0  10.0        10.0
nADoutLE1.D                                                         10.0      
nAoutOE.D                                                                     
nBERR_FSB.D                                                   10.0            
nBR_IOB.D                                         10.0                        
nCAS.D                                                        11.0            
nDTACK_FSB.D                                                  10.0            
nOE.D                                                         11.0            
nRESout.D                                                                     
nVPA_FSB.D                                                    10.0            
ram/BACTr.D                                                   10.0            
ram/DTACKr.D                                                                  
ram/RASEL.D                                             10.0  10.0            
ram/RASEN.D                                                   11.0            
ram/RASrf.D                                                                   
ram/RASrr.D                                             10.0  10.0            
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             
ram/RS_FSM_FFd4.D                                                             
ram/RS_FSM_FFd5.D                                                             
ram/RS_FSM_FFd6.D                                       10.0  10.0            
ram/RS_FSM_FFd7.D                                             11.0            
ram/RS_FSM_FFd8.D                                       11.0  11.0            
ram/RefDone.D                                                                 

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 i     i     i     i     i     i     i     i     n     n
 \                     o     o     o     o     o     o     o     o     A     A
  \                    b     b     b     b     b     b     b     b     D     o
   \                   s     s     s     s     s     s     s     s     o     u
    \                  /     /     /     /     /     /     /     /     u     t
     \                 I     I     I     I     L     S     T     T     t     O
      \                O     O     O     O     o     e     S     S     L     E
       \               D     L     R     U     a     n     _     _     E     .
        \              O     1     W     1     d     t     F     F     1     Q
         \             N     .     1     .     1     .     S     S     .      
          \            E     Q     .     Q     .     Q     M     M     Q      
           \           r           Q           Q           _     _            
            \          .                                   F     F            
             \         Q                                   F     F            
              \                                            d     d            
               \                                           1     2            
                \                                          .     .            
                 \                                         Q     Q            
  To              \------------------------------------------------------------

ALE0S.D                                                       10.0            
IOL0.D                    11.0                    10.0  10.0  11.4  11.4      
IONPReady.D         11.0                          11.0                        
IORDREQ.D                       11.0              10.0  10.0  11.0  11.0      
IOU0.D                                11.0        10.0  10.0  11.4  11.4      
IOWRREQ.D                       10.0              11.0  11.0  11.0  11.0      
QoSReady.D                                                                    
RAMReady.D                                                                    
RefReq.CE                                                                     
RefReq.D                                                                      
RefUrg.CE                                                                     
RefUrg.D                                                                      
cnt/Er<1>.D                                                                   
cnt/IS_FSM_FFd1.D                                                             
cnt/IS_FSM_FFd2.D                                                             
cnt/LTimer<0>.D                                                               
cnt/LTimer<10>.D                                                              
cnt/LTimer<11>.D                                                              
cnt/LTimer<1>.D                                                               
cnt/LTimer<2>.D                                                               
cnt/LTimer<3>.D                                                               
cnt/LTimer<4>.D                                                               
cnt/LTimer<5>.D                                                               
cnt/LTimer<6>.D                                                               
cnt/LTimer<7>.D                                                               
cnt/LTimer<8>.D                                                               
cnt/LTimer<9>.D                                                               
cnt/LTimerTC.D                                                                
cnt/Timer<0>.CE                                                               
cnt/Timer<0>.D                                                                
cnt/Timer<1>.CE                                                               
cnt/Timer<1>.D                                                                
cnt/Timer<2>.CE                                                               
cnt/Timer<2>.D                                                                
cnt/Timer<3>.CE                                                               
cnt/Timer<3>.D                                                                
cnt/TimerTC.CE                                                                
cnt/TimerTC.D                                                                 
cnt/WS<0>.D                                                                   
cnt/WS<1>.D                                                                   
cnt/WS<2>.D                                                                   
cnt/WS<3>.D                                                                   
cs/nOverlay.D                                                                 
iobs/Clear1.D                                           10.0  10.0            
iobs/IOL1.CE                                10.0                              
iobs/IORW1.D                    11.0              11.0  11.0  11.0  11.0      
iobs/IOU1.CE                                10.0                              
iobs/Load1.D                                      11.0  11.0  11.0  11.0      
iobs/Sent.D                                       11.4  11.4  11.4  11.4      
iobs/TS_FSM_FFd1.D                                      10.0  10.0            
iobs/TS_FSM_FFd2.D                                10.0  10.0  11.0  11.0      
nADoutLE1.D                                 10.0                    10.0      
nAoutOE.D                                                                 11.0
nBERR_FSB.D                                       10.0                        
nBR_IOB.D                                                                     
nCAS.D                                                                        
nDTACK_FSB.D                                                        11.0      
nOE.D                                                                         
nRESout.D                                                                     
nVPA_FSB.D                                                                    
ram/BACTr.D                                                                   
ram/DTACKr.D                                                                  
ram/RASEL.D                                                                   
ram/RASEN.D                                                                   
ram/RASrf.D                                                                   
ram/RASrr.D                                                                   
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             
ram/RS_FSM_FFd4.D                                                             
ram/RS_FSM_FFd5.D                                                             
ram/RS_FSM_FFd6.D                                                             
ram/RS_FSM_FFd7.D                                                             
ram/RS_FSM_FFd8.D                                                             
ram/RefDone.D                                                                 

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 n     n     n     r     r     r     r     r     r     r
 \                     B     B     D     a     a     a     a     a     a     a
  \                    E     R     T     m     m     m     m     m     m     m
   \                   R     _     A     /     /     /     /     /     /     /
    \                  R     I     C     B     D     R     R     R     R     R
     \                 _     O     K     A     T     A     A     S     S     S
      \                F     B     _     C     A     S     S     _     _     _
       \               S     .     F     T     C     E     r     F     F     F
        \              B     Q     S     r     K     N     r     S     S     S
         \             .           B     .     r     .     .     M     M     M
          \            Q           .     Q     .     Q     Q     _     _     _
           \                       Q           Q                 F     F     F
            \                                                    F     F     F
             \                                                   d     d     d
              \                                                  1     2     3
               \                                                 .     .     .
                \                                                Q     Q     Q
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
IOL0.D                                                                        
IONPReady.D                                                                   
IORDREQ.D                                                                     
IOU0.D                                                                        
IOWRREQ.D                                                                     
QoSReady.D                                                                    
RAMReady.D                            11.0        10.0        11.0            
RefReq.CE                                                                     
RefReq.D                                                                      
RefUrg.CE                                                                     
RefUrg.D                                                                      
cnt/Er<1>.D                                                                   
cnt/IS_FSM_FFd1.D                                                             
cnt/IS_FSM_FFd2.D                                                             
cnt/LTimer<0>.D                                                               
cnt/LTimer<10>.D                                                              
cnt/LTimer<11>.D                                                              
cnt/LTimer<1>.D                                                               
cnt/LTimer<2>.D                                                               
cnt/LTimer<3>.D                                                               
cnt/LTimer<4>.D                                                               
cnt/LTimer<5>.D                                                               
cnt/LTimer<6>.D                                                               
cnt/LTimer<7>.D                                                               
cnt/LTimer<8>.D                                                               
cnt/LTimer<9>.D                                                               
cnt/LTimerTC.D                                                                
cnt/Timer<0>.CE                                                               
cnt/Timer<0>.D                                                                
cnt/Timer<1>.CE                                                               
cnt/Timer<1>.D                                                                
cnt/Timer<2>.CE                                                               
cnt/Timer<2>.D                                                                
cnt/Timer<3>.CE                                                               
cnt/Timer<3>.D                                                                
cnt/TimerTC.CE                                                                
cnt/TimerTC.D                                                                 
cnt/WS<0>.D                                                                   
cnt/WS<1>.D                                                                   
cnt/WS<2>.D                                                                   
cnt/WS<3>.D                                                                   
cs/nOverlay.D                                                                 
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                                  
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                                  
iobs/Sent.D                                                                   
iobs/TS_FSM_FFd1.D                                                            
iobs/TS_FSM_FFd2.D                                                            
nADoutLE1.D                                                                   
nAoutOE.D                 11.0                                                
nBERR_FSB.D         11.0                                                      
nBR_IOB.D                 10.0                                                
nCAS.D                                11.0  10.0  11.0        10.0  10.0  10.0
nDTACK_FSB.D                                                                  
nOE.D                                 11.0  11.0                              
nRESout.D                                                                     
nVPA_FSB.D                                                                    
ram/BACTr.D                                                                   
ram/DTACKr.D                    10.0                                          
ram/RASEL.D                                 10.0  10.0                        
ram/RASEN.D                           11.0        10.0        11.0            
ram/RASrf.D                                                                   
ram/RASrr.D                                       10.0                    10.0
ram/RS_FSM_FFd1.D                                       10.0        10.0      
ram/RS_FSM_FFd2.D                                       10.0        10.0  10.0
ram/RS_FSM_FFd3.D                                                             
ram/RS_FSM_FFd4.D                           10.0                              
ram/RS_FSM_FFd5.D                           10.0                              
ram/RS_FSM_FFd6.D                                 10.0                        
ram/RS_FSM_FFd7.D                     11.0        10.0                        
ram/RS_FSM_FFd8.D                     11.0        11.0        11.0            
ram/RefDone.D                                                 10.0  10.0  10.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: FCLK)

\ From                 r     r     r     r     r     r
 \                     a     a     a     a     a     a
  \                    m     m     m     m     m     m
   \                   /     /     /     /     /     /
    \                  R     R     R     R     R     R
     \                 S     S     S     S     S     e
      \                _     _     _     _     _     f
       \               F     F     F     F     F     D
        \              S     S     S     S     S     o
         \             M     M     M     M     M     n
          \            _     _     _     _     _     e
           \           F     F     F     F     F     .
            \          F     F     F     F     F     Q
             \         d     d     d     d     d      
              \        4     5     6     7     8      
               \       .     .     .     .     .      
                \      Q     Q     Q     Q     Q      
                 \                                    
  To              \------------------------------------

ALE0S.D                                               
IOL0.D                                                
IONPReady.D                                           
IORDREQ.D                                             
IOU0.D                                                
IOWRREQ.D                                             
QoSReady.D                                            
RAMReady.D          11.0  11.0  11.0        10.0  11.0
RefReq.CE                                             
RefReq.D                                              
RefUrg.CE                                             
RefUrg.D                                              
cnt/Er<1>.D                                           
cnt/IS_FSM_FFd1.D                                     
cnt/IS_FSM_FFd2.D                                     
cnt/LTimer<0>.D                                       
cnt/LTimer<10>.D                                      
cnt/LTimer<11>.D                                      
cnt/LTimer<1>.D                                       
cnt/LTimer<2>.D                                       
cnt/LTimer<3>.D                                       
cnt/LTimer<4>.D                                       
cnt/LTimer<5>.D                                       
cnt/LTimer<6>.D                                       
cnt/LTimer<7>.D                                       
cnt/LTimer<8>.D                                       
cnt/LTimer<9>.D                                       
cnt/LTimerTC.D                                        
cnt/Timer<0>.CE                                       
cnt/Timer<0>.D                                        
cnt/Timer<1>.CE                                       
cnt/Timer<1>.D                                        
cnt/Timer<2>.CE                                       
cnt/Timer<2>.D                                        
cnt/Timer<3>.CE                                       
cnt/Timer<3>.D                                        
cnt/TimerTC.CE                                        
cnt/TimerTC.D                                         
cnt/WS<0>.D                                           
cnt/WS<1>.D                                           
cnt/WS<2>.D                                           
cnt/WS<3>.D                                           
cs/nOverlay.D                                         
iobs/Clear1.D                                         
iobs/IOL1.CE                                          
iobs/IORW1.D                                          
iobs/IOU1.CE                                          
iobs/Load1.D                                          
iobs/Sent.D                                           
iobs/TS_FSM_FFd1.D                                    
iobs/TS_FSM_FFd2.D                                    
nADoutLE1.D                                           
nAoutOE.D                                             
nBERR_FSB.D                                           
nBR_IOB.D                                             
nCAS.D              11.0  10.0        11.0  11.0  11.0
nDTACK_FSB.D                                          
nOE.D                                                 
nRESout.D                                             
nVPA_FSB.D                                            
ram/BACTr.D                                           
ram/DTACKr.D                                          
ram/RASEL.D               10.0  10.0        10.0      
ram/RASEN.D         11.0                    10.0  11.0
ram/RASrf.D                     10.0                  
ram/RASrr.D         10.0              10.0  10.0  10.0
ram/RS_FSM_FFd1.D                                     
ram/RS_FSM_FFd2.D                                     
ram/RS_FSM_FFd3.D                     10.0            
ram/RS_FSM_FFd4.D         10.0                        
ram/RS_FSM_FFd5.D         10.0  10.0                  
ram/RS_FSM_FFd6.D                           10.0      
ram/RS_FSM_FFd7.D   10.0                    11.0  11.0
ram/RS_FSM_FFd8.D   11.0                    11.0  11.0
ram/RefDone.D                         10.0        10.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: C16M)

\ From                  A     I     i     i     i     i     i     i     i     i
 \                      L     O     o     o     o     o     o     o     o     o
  \                     E     A     b     b     b     b     b     b     b     b
   \                    0     C     m     m     m     m     m     m     m     m
    \                   M     T     /     /     /     /     /     /     /     /
     \                  .     .     C     D     I     I     I     I     I     I
      \                 Q     Q     8     o     O     O     O     O     O     O
       \                            M     u     R     S     S     S     S     S
        \                           r     t     D     0     _     _     _     _
         \                          .     O     R     .     F     F     F     F
          \                         Q     E     E     Q     S     S     S     S
           \                              .     Q           M     M     M     M
            \                             Q     r           _     _     _     _
             \                                  .           F     F     F     F
              \                                 Q           F     F     F     F
               \                                            d     d     d     d
                \                                           1     2     3     4
                 \                                          .     .     .     .
                  \                                         Q     Q     Q     Q
  To               \------------------------------------------------------------

ALE0M.D              10.0                    10.0        10.0  10.0  10.0  10.0
IOACT.D                    11.0  10.0        10.0        11.0  11.0  11.0  10.0
iobm/DoutOE.D                    10.0  10.0                          10.0  10.0
iobm/IOS0.D                      10.0        10.0  10.0  10.0  10.0  10.0  10.0
iobm/IOS_FSM_FFd1.D                                            10.0            
iobm/IOS_FSM_FFd2.D              10.0                                10.0      
iobm/IOS_FSM_FFd3.D              10.0                                10.0  10.0
iobm/IOS_FSM_FFd4.D                                                            
iobm/IOS_FSM_FFd5.D                                                            
iobm/IOS_FSM_FFd6.D              10.0        10.0                              
iobm/IOS_FSM_FFd7.D              10.0        10.0        10.0                  
nAS_IOB.D                        10.0        10.0                    10.0  10.0
nDinLE.D                                                             10.0  10.0
nLDS_IOB.D                       11.0        11.0                    10.0  10.0
nUDS_IOB.D                       11.0        11.0                    10.0  10.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                 (Clock: C16M)

\ From                  i     i     i     i     n     n
 \                      o     o     o     o     L     U
  \                     b     b     b     b     D     D
   \                    m     m     m     m     S     S
    \                   /     /     /     /     _     _
     \                  I     I     I     I     I     I
      \                 O     O     O     O     O     O
       \                S     S     S     W     B     B
        \               _     _     _     R     .     .
         \              F     F     F     R     Q     Q
          \             S     S     S     E            
           \            M     M     M     Q            
            \           _     _     _     r            
             \          F     F     F     .            
              \         F     F     F     Q            
               \        d     d     d                  
                \       5     6     7                  
                 \      .     .     .                  
                  \     Q     Q     Q                  
  To               \------------------------------------

ALE0M.D              10.0  10.0  10.0  10.0            
IOACT.D              10.0  10.0  11.0  11.0            
iobm/DoutOE.D        10.0  10.0  10.0  10.0            
iobm/IOS0.D          10.0  10.0  10.0  10.0            
iobm/IOS_FSM_FFd1.D                                    
iobm/IOS_FSM_FFd2.D                                    
iobm/IOS_FSM_FFd3.D                                    
iobm/IOS_FSM_FFd4.D  10.0                              
iobm/IOS_FSM_FFd5.D        10.0                        
iobm/IOS_FSM_FFd6.D              10.0  10.0            
iobm/IOS_FSM_FFd7.D              10.0  10.0            
nAS_IOB.D            10.0  10.0  10.0  10.0            
nDinLE.D                                               
nLDS_IOB.D           10.0  10.0  11.0        10.0      
nUDS_IOB.D           10.0  10.0  11.0              10.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                  (Clock: C8M)

\ From           i     i     i     i     i     i     n
 \               o     o     o     o     o     o     V
  \              b     b     b     b     b     b     M
   \             m     m     m     m     m     m     A
    \            /     /     /     /     /     /     _
     \           E     E     E     E     E     V     I
      \          S     S     S     S     r     P     O
       \         <     <     <     <     .     A     B
        \        0     1     2     3     Q     r     .
         \       >     >     >     >           .     Q
          \      .     .     .     .           Q      
           \     Q     Q     Q     Q                  
  To        \------------------------------------------

IODONE.D      10.0  10.0  10.0  10.0              10.0
iobm/ES<0>.D  10.0  10.0  10.0  10.0  10.0            
iobm/ES<1>.D  10.0  10.0  10.0  10.0  10.0            
iobm/ES<2>.D  10.0  10.0  10.0        10.0            
iobm/ES<3>.D  10.0  10.0  10.0  10.0  10.0            
nVMA_IOB.D    10.0  10.0  10.0  10.0        10.0  10.0

Path Type Definition: 

Pad to Pad (tPD) -                        Reports pad to pad paths that start 
                                          at input pads and end at output pads. 
                                          Paths are not traced through 
                                          registers. 

Clock Pad to Output Pad (tCO) -           Reports paths that start at input 
                                          pads trace through clock inputs of 
                                          registers and end at output pads. 
                                          Paths are not traced through PRE/CLR 
                                          inputs of registers. 

Setup to Clock at Pad (tSU or tSUF) -     Reports external setup time of data 
                                          to clock at pad. Data path starts at 
                                          an input pad and ends at register 
                                          (Fast Input Register for tSUF) D/T 
                                          input. Clock path starts at input pad 
                                          and ends at the register clock input. 
                                          Paths are not traced through 
                                          registers. Pin-to-pin setup 
                                          requirement is not reported or 
                                          guaranteed for product-term clocks 
                                          derived from macrocell feedback 
                                          signals. 

Clock to Setup (tCYC) -                   Register to register cycle time. 
                                          Include source register tCO and 
                                          destination register tSU. Note that 
                                          when the computed Maximum Clock Speed 
                                          is limited by tCYC it is computed 
                                          assuming that all registers are 
                                          rising-edge sensitive. 

