(export (version D)
  (design
    (source /home/dmb/atom/AtomBusMon/kicad/6502_adapter.sch)
    (date "Mon 24 Jul 2017 21:45:18 BST")
    (tool "Eeschema 4.0.6-e0-6349~53~ubuntu14.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 6502_adapter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value WD65C02)
      (footprint footprints:dip40_smt_header)
      (libsource (lib 65xx) (part WD65C02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975BF41))
    (comp (ref U4)
      (value 74LVC4245)
      (footprint footprints:SOIC-24W_7.5x15.4mm_Pitch1.27mm)
      (libsource (lib 74lvc) (part 74LVC8T245))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C5CE))
    (comp (ref P2)
      (value CONN_02X20)
      (footprint footprints:Socket_Strip_Straight_2x20_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C737))
    (comp (ref P1)
      (value CONN_02X20)
      (footprint footprints:Socket_Strip_Straight_2x20_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C7A4))
    (comp (ref U5)
      (value 74LVC4245)
      (footprint footprints:SOIC-24W_7.5x15.4mm_Pitch1.27mm)
      (libsource (lib 74lvc) (part 74LVC8T245))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C870))
    (comp (ref U2)
      (value 74LVC4245)
      (footprint footprints:SOIC-24W_7.5x15.4mm_Pitch1.27mm)
      (libsource (lib 74lvc) (part 74LVC8T245))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C8C1))
    (comp (ref U3)
      (value 74LVC4245)
      (footprint footprints:SOIC-24W_7.5x15.4mm_Pitch1.27mm)
      (libsource (lib 74lvc) (part 74LVC8T245))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C914))
    (comp (ref U6)
      (value 74LVC4245)
      (footprint footprints:SOIC-24W_7.5x15.4mm_Pitch1.27mm)
      (libsource (lib 74lvc) (part 74LVC8T245))
      (sheetpath (names /) (tstamps /))
      (tstamp 5975C957))
    (comp (ref P3)
      (value CONN_01X03)
      (footprint footprints:Pin_Header_Straight_1x03_Pitch2.00mm)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 59760CE2))
    (comp (ref P4)
      (value CONN_01X02)
      (footprint footprints:Pin_Header_Straight_1x02_Pitch2.00mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5976110F))
    (comp (ref R1)
      (value 4K7)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59761BB3))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 597620E8))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5976220A))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59762254))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59762296))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 597622DF))
    (comp (ref C7)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 597624D7))
    (comp (ref C8)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5976252A))
    (comp (ref C9)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59762588))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 597625E5))
    (comp (ref C11)
      (value 100nF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59762645))
    (comp (ref C6)
      (value 10uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part CP1_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 597630BE))
    (comp (ref C12)
      (value 10uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part CP1_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59763501)))
  (libparts
    (libpart (lib 74lvc) (part 74LVC8T245)
      (footprints
        (fp IPC_SOP65P640X120-24N))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LVC8T245))
      (pins
        (pin (num 1) (name VCCA) (type power_in))
        (pin (num 2) (name DIR) (type input))
        (pin (num 3) (name A1) (type BiDi))
        (pin (num 4) (name A2) (type BiDi))
        (pin (num 5) (name A3) (type BiDi))
        (pin (num 6) (name A4) (type BiDi))
        (pin (num 7) (name A5) (type BiDi))
        (pin (num 8) (name A6) (type BiDi))
        (pin (num 9) (name A7) (type BiDi))
        (pin (num 10) (name A8) (type BiDi))
        (pin (num 11) (name GND) (type power_in))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name B8) (type BiDi))
        (pin (num 15) (name B7) (type BiDi))
        (pin (num 16) (name B6) (type BiDi))
        (pin (num 17) (name B5) (type BiDi))
        (pin (num 18) (name B4) (type BiDi))
        (pin (num 19) (name B3) (type BiDi))
        (pin (num 20) (name B2) (type BiDi))
        (pin (num 21) (name B1) (type BiDi))
        (pin (num 22) (name OE#) (type input))
        (pin (num 23) (name VCCB) (type power_in))
        (pin (num 24) (name VCCB) (type power_in))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_02X20)
      (description "Connector 02x20")
      (footprints
        (fp Pin_Header_Straight_2X20)
        (fp Pin_Header_Angled_2X20)
        (fp Socket_Strip_Straight_2X20)
        (fp Socket_Strip_Angled_2X20))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X20))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))))
    (libpart (lib device) (part CP1_Small)
      (description "Polarised capacitor")
      (footprints
        (fp CP*)
        (fp Elko*)
        (fp TantalC*)
        (fp C*elec)
        (fp c_elec*)
        (fp SMD*_Pol))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R_Small)
      (description Resistor)
      (footprints
        (fp Resistor_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib 65xx) (part WD65C02)
      (fields
        (field (name Reference) U)
        (field (name Value) WD65C02))
      (pins
        (pin (num 1) (name ~VP) (type output))
        (pin (num 2) (name RDY) (type BiDi))
        (pin (num 3) (name PHI1out) (type output))
        (pin (num 4) (name ~IRQ) (type input))
        (pin (num 5) (name ~ML) (type output))
        (pin (num 6) (name ~NMI) (type input))
        (pin (num 7) (name SYNC) (type output))
        (pin (num 8) (name VCC) (type power_in))
        (pin (num 9) (name A0) (type output))
        (pin (num 10) (name A1) (type output))
        (pin (num 11) (name A2) (type output))
        (pin (num 12) (name A3) (type output))
        (pin (num 13) (name A4) (type output))
        (pin (num 14) (name A5) (type output))
        (pin (num 15) (name A6) (type output))
        (pin (num 16) (name A7) (type output))
        (pin (num 17) (name A8) (type output))
        (pin (num 18) (name A9) (type output))
        (pin (num 19) (name A10) (type output))
        (pin (num 20) (name A11) (type output))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name A12) (type output))
        (pin (num 23) (name A13) (type output))
        (pin (num 24) (name A14) (type output))
        (pin (num 25) (name A15) (type output))
        (pin (num 26) (name D7) (type 3state))
        (pin (num 27) (name D6) (type 3state))
        (pin (num 28) (name D5) (type 3state))
        (pin (num 29) (name D4) (type 3state))
        (pin (num 30) (name D3) (type 3state))
        (pin (num 31) (name D2) (type 3state))
        (pin (num 32) (name D1) (type 3state))
        (pin (num 33) (name D0) (type 3state))
        (pin (num 34) (name R/~W) (type output))
        (pin (num 35) (name NC) (type NotConnected))
        (pin (num 36) (name BE) (type input))
        (pin (num 37) (name PHI2) (type input))
        (pin (num 38) (name ~SO) (type output))
        (pin (num 39) (name PHI2out) (type output))
        (pin (num 40) (name ~RESET) (type input)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical 65xx)
      (uri 65xx.lib))
    (library (logical 74lvc)
      (uri 74lvc.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(P1-Pad39)")
      (node (ref P1) (pin 39)))
    (net (code 2) (name "Net-(P1-Pad40)")
      (node (ref P1) (pin 40)))
    (net (code 3) (name /5V)
      (node (ref U4) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref P2) (pin 11))
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref P1) (pin 11))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref C5) (pin 1)))
    (net (code 4) (name /3V3)
      (node (ref U6) (pin 24))
      (node (ref U5) (pin 24))
      (node (ref U5) (pin 23))
      (node (ref U5) (pin 13))
      (node (ref U2) (pin 24))
      (node (ref U2) (pin 23))
      (node (ref U6) (pin 23))
      (node (ref U4) (pin 23))
      (node (ref C12) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U4) (pin 24))
      (node (ref C8) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref U3) (pin 24))
      (node (ref C11) (pin 1))
      (node (ref P2) (pin 29))
      (node (ref P1) (pin 29))
      (node (ref C9) (pin 1))
      (node (ref U3) (pin 23)))
    (net (code 5) (name /GND)
      (node (ref U1) (pin 21))
      (node (ref P1) (pin 30))
      (node (ref P1) (pin 12))
      (node (ref P2) (pin 12))
      (node (ref U6) (pin 22))
      (node (ref U6) (pin 13))
      (node (ref U4) (pin 13))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 2))
      (node (ref P2) (pin 30))
      (node (ref U2) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref U6) (pin 12))
      (node (ref C7) (pin 2))
      (node (ref U5) (pin 12))
      (node (ref U5) (pin 11))
      (node (ref U2) (pin 13))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 11))
      (node (ref U2) (pin 22))
      (node (ref U3) (pin 11))
      (node (ref U3) (pin 13))
      (node (ref C1) (pin 2))
      (node (ref U3) (pin 12))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref P3) (pin 3))
      (node (ref U6) (pin 11)))
    (net (code 6) (name "Net-(P1-Pad25)")
      (node (ref P1) (pin 25)))
    (net (code 7) (name "Net-(P2-Pad25)")
      (node (ref P2) (pin 25)))
    (net (code 8) (name "Net-(P2-Pad28)")
      (node (ref P2) (pin 28)))
    (net (code 9) (name "Net-(P2-Pad14)")
      (node (ref P2) (pin 14)))
    (net (code 10) (name "Net-(P2-Pad16)")
      (node (ref P2) (pin 16)))
    (net (code 11) (name "Net-(P2-Pad15)")
      (node (ref P2) (pin 15)))
    (net (code 12) (name "Net-(P2-Pad13)")
      (node (ref P2) (pin 13)))
    (net (code 13) (name "Net-(P1-Pad38)")
      (node (ref P1) (pin 38)))
    (net (code 14) (name "Net-(P1-Pad28)")
      (node (ref P1) (pin 28)))
    (net (code 15) (name "Net-(P1-Pad27)")
      (node (ref P1) (pin 27)))
    (net (code 16) (name "Net-(P2-Pad27)")
      (node (ref P2) (pin 27)))
    (net (code 17) (name "Net-(P1-Pad26)")
      (node (ref P1) (pin 26)))
    (net (code 18) (name "Net-(P1-Pad24)")
      (node (ref P1) (pin 24)))
    (net (code 19) (name "Net-(P1-Pad14)")
      (node (ref P1) (pin 14)))
    (net (code 20) (name "Net-(P1-Pad10)")
      (node (ref P1) (pin 10)))
    (net (code 21) (name "Net-(P1-Pad8)")
      (node (ref P1) (pin 8)))
    (net (code 22) (name "Net-(P1-Pad6)")
      (node (ref P1) (pin 6)))
    (net (code 23) (name "Net-(P1-Pad4)")
      (node (ref P1) (pin 4)))
    (net (code 24) (name "Net-(P1-Pad2)")
      (node (ref P1) (pin 2)))
    (net (code 25) (name "Net-(P2-Pad39)")
      (node (ref P2) (pin 39)))
    (net (code 26) (name /nML)
      (node (ref U2) (pin 5))
      (node (ref P4) (pin 2)))
    (net (code 27) (name /RnW)
      (node (ref U2) (pin 4))
      (node (ref U5) (pin 2))
      (node (ref U1) (pin 34)))
    (net (code 28) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 29) (name "Net-(P3-Pad2)")
      (node (ref U1) (pin 1))
      (node (ref P3) (pin 2)))
    (net (code 30) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 31) (name "Net-(U2-Pad9)")
      (node (ref U2) (pin 9)))
    (net (code 32) (name "Net-(P1-Pad13)")
      (node (ref P1) (pin 13)))
    (net (code 33) (name "Net-(U6-Pad21)")
      (node (ref U6) (pin 21)))
    (net (code 34) (name "Net-(U6-Pad3)")
      (node (ref U6) (pin 3)))
    (net (code 35) (name "Net-(U2-Pad10)")
      (node (ref U2) (pin 10)))
    (net (code 36) (name "Net-(P4-Pad1)")
      (node (ref U1) (pin 5))
      (node (ref P4) (pin 1)))
    (net (code 37) (name "Net-(R1-Pad2)")
      (node (ref U6) (pin 2))
      (node (ref R1) (pin 2)))
    (net (code 38) (name "Net-(P1-Pad9)")
      (node (ref P1) (pin 9)))
    (net (code 39) (name "Net-(P1-Pad7)")
      (node (ref P1) (pin 7)))
    (net (code 40) (name "Net-(P1-Pad5)")
      (node (ref P1) (pin 5)))
    (net (code 41) (name "Net-(P1-Pad3)")
      (node (ref P1) (pin 3)))
    (net (code 42) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 43) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 44) (name "Net-(P2-Pad3)")
      (node (ref P2) (pin 3)))
    (net (code 45) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 46) (name "Net-(P2-Pad2)")
      (node (ref P2) (pin 2)))
    (net (code 47) (name "Net-(P2-Pad4)")
      (node (ref P2) (pin 4)))
    (net (code 48) (name /BE)
      (node (ref U6) (pin 9))
      (node (ref U1) (pin 36)))
    (net (code 49) (name /nSO)
      (node (ref U6) (pin 6))
      (node (ref U1) (pin 38)))
    (net (code 50) (name /nIRQ)
      (node (ref U1) (pin 4))
      (node (ref U6) (pin 7)))
    (net (code 51) (name /PHI2)
      (node (ref U1) (pin 37))
      (node (ref U6) (pin 8)))
    (net (code 52) (name /nNMI)
      (node (ref U1) (pin 6))
      (node (ref U6) (pin 10)))
    (net (code 53) (name /PHI2OUT)
      (node (ref U1) (pin 39))
      (node (ref U2) (pin 7)))
    (net (code 54) (name /PHI1OUT)
      (node (ref U2) (pin 6))
      (node (ref U1) (pin 3)))
    (net (code 55) (name /nVP)
      (node (ref U2) (pin 8))
      (node (ref P3) (pin 1)))
    (net (code 56) (name /SYNC)
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 7)))
    (net (code 57) (name /nRST)
      (node (ref U1) (pin 40))
      (node (ref U6) (pin 4)))
    (net (code 58) (name /RDY)
      (node (ref U1) (pin 2))
      (node (ref U6) (pin 5)))
    (net (code 59) (name /LV_A11)
      (node (ref U4) (pin 21))
      (node (ref P2) (pin 37)))
    (net (code 60) (name /LV_A0)
      (node (ref U3) (pin 14))
      (node (ref P2) (pin 18)))
    (net (code 61) (name /LV_A10)
      (node (ref P2) (pin 38))
      (node (ref U4) (pin 20)))
    (net (code 62) (name /LV_A3)
      (node (ref P2) (pin 19))
      (node (ref U3) (pin 17)))
    (net (code 63) (name /LV_A1)
      (node (ref P2) (pin 17))
      (node (ref U3) (pin 15)))
    (net (code 64) (name /LV_D2)
      (node (ref U5) (pin 19))
      (node (ref P1) (pin 20)))
    (net (code 65) (name /LV_A5)
      (node (ref P2) (pin 21))
      (node (ref U3) (pin 19)))
    (net (code 66) (name /LV_A14)
      (node (ref U4) (pin 15))
      (node (ref P2) (pin 31)))
    (net (code 67) (name /LV_A4)
      (node (ref P2) (pin 22))
      (node (ref U3) (pin 18)))
    (net (code 68) (name /LV_A15)
      (node (ref U4) (pin 14))
      (node (ref P2) (pin 32)))
    (net (code 69) (name /LV_A7)
      (node (ref P2) (pin 23))
      (node (ref U3) (pin 21)))
    (net (code 70) (name /LV_A12)
      (node (ref U4) (pin 17))
      (node (ref P2) (pin 33)))
    (net (code 71) (name /LV_A6)
      (node (ref P2) (pin 24))
      (node (ref U3) (pin 20)))
    (net (code 72) (name /LV_A13)
      (node (ref P2) (pin 34))
      (node (ref U4) (pin 16)))
    (net (code 73) (name /LV_A9)
      (node (ref P2) (pin 35))
      (node (ref U4) (pin 19)))
    (net (code 74) (name /LV_OEAL)
      (node (ref P2) (pin 26))
      (node (ref U3) (pin 22)))
    (net (code 75) (name /LV_A8)
      (node (ref P2) (pin 36))
      (node (ref U4) (pin 18)))
    (net (code 76) (name /LV_D5)
      (node (ref U5) (pin 16))
      (node (ref P1) (pin 17)))
    (net (code 77) (name /LV_nRST)
      (node (ref P1) (pin 37))
      (node (ref U6) (pin 20)))
    (net (code 78) (name /LV_D4)
      (node (ref P1) (pin 18))
      (node (ref U5) (pin 17)))
    (net (code 79) (name /LV_D3)
      (node (ref P1) (pin 19))
      (node (ref U5) (pin 18)))
    (net (code 80) (name /LV_RDY)
      (node (ref P1) (pin 36))
      (node (ref U6) (pin 19)))
    (net (code 81) (name /LV_PHI2)
      (node (ref P1) (pin 33))
      (node (ref U6) (pin 16)))
    (net (code 82) (name /LV_D1)
      (node (ref U5) (pin 20))
      (node (ref P1) (pin 21)))
    (net (code 83) (name /LV_nNMI)
      (node (ref U6) (pin 14))
      (node (ref P1) (pin 31)))
    (net (code 84) (name /LV_D0)
      (node (ref U5) (pin 21))
      (node (ref P1) (pin 22)))
    (net (code 85) (name /LV_BE)
      (node (ref U6) (pin 15))
      (node (ref P1) (pin 32)))
    (net (code 86) (name /LV_OED)
      (node (ref P1) (pin 23))
      (node (ref U5) (pin 22)))
    (net (code 87) (name /LV_OEAH)
      (node (ref P2) (pin 40))
      (node (ref U4) (pin 22)))
    (net (code 88) (name /LV_nIRQ)
      (node (ref P1) (pin 34))
      (node (ref U6) (pin 17)))
    (net (code 89) (name /LV_D7)
      (node (ref P1) (pin 15))
      (node (ref U5) (pin 14)))
    (net (code 90) (name /LV_nSO)
      (node (ref P1) (pin 35))
      (node (ref U6) (pin 18)))
    (net (code 91) (name /LV_D6)
      (node (ref P1) (pin 16))
      (node (ref U5) (pin 15)))
    (net (code 92) (name /LV_A2)
      (node (ref U3) (pin 16))
      (node (ref P2) (pin 20)))
    (net (code 93) (name /A0)
      (node (ref U1) (pin 9))
      (node (ref U3) (pin 10)))
    (net (code 94) (name /A1)
      (node (ref U3) (pin 9))
      (node (ref U1) (pin 10)))
    (net (code 95) (name /A2)
      (node (ref U1) (pin 11))
      (node (ref U3) (pin 8)))
    (net (code 96) (name /A3)
      (node (ref U1) (pin 12))
      (node (ref U3) (pin 7)))
    (net (code 97) (name /A4)
      (node (ref U3) (pin 6))
      (node (ref U1) (pin 13)))
    (net (code 98) (name /A5)
      (node (ref U3) (pin 5))
      (node (ref U1) (pin 14)))
    (net (code 99) (name /A6)
      (node (ref U1) (pin 15))
      (node (ref U3) (pin 4)))
    (net (code 100) (name /A7)
      (node (ref U1) (pin 16))
      (node (ref U3) (pin 3)))
    (net (code 101) (name /D0)
      (node (ref U5) (pin 3))
      (node (ref U1) (pin 33)))
    (net (code 102) (name /D1)
      (node (ref U1) (pin 32))
      (node (ref U5) (pin 4)))
    (net (code 103) (name /D2)
      (node (ref U1) (pin 31))
      (node (ref U5) (pin 5)))
    (net (code 104) (name /D3)
      (node (ref U1) (pin 30))
      (node (ref U5) (pin 6)))
    (net (code 105) (name /D4)
      (node (ref U5) (pin 7))
      (node (ref U1) (pin 29)))
    (net (code 106) (name /D5)
      (node (ref U5) (pin 8))
      (node (ref U1) (pin 28)))
    (net (code 107) (name /D6)
      (node (ref U5) (pin 9))
      (node (ref U1) (pin 27)))
    (net (code 108) (name /D7)
      (node (ref U5) (pin 10))
      (node (ref U1) (pin 26)))
    (net (code 109) (name /A12)
      (node (ref U4) (pin 7))
      (node (ref U1) (pin 22)))
    (net (code 110) (name /A8)
      (node (ref U1) (pin 17))
      (node (ref U4) (pin 6)))
    (net (code 111) (name /A9)
      (node (ref U4) (pin 5))
      (node (ref U1) (pin 18)))
    (net (code 112) (name /A10)
      (node (ref U1) (pin 19))
      (node (ref U4) (pin 4)))
    (net (code 113) (name /A11)
      (node (ref U4) (pin 3))
      (node (ref U1) (pin 20)))
    (net (code 114) (name /A15)
      (node (ref U1) (pin 25))
      (node (ref U4) (pin 10)))
    (net (code 115) (name /A14)
      (node (ref U4) (pin 9))
      (node (ref U1) (pin 24)))
    (net (code 116) (name /A13)
      (node (ref U1) (pin 23))
      (node (ref U4) (pin 8)))
    (net (code 117) (name /LV_RnW)
      (node (ref P2) (pin 10))
      (node (ref U2) (pin 20)))
    (net (code 118) (name /LV_SYNC)
      (node (ref P2) (pin 9))
      (node (ref U2) (pin 21)))
    (net (code 119) (name /LV_nVP)
      (node (ref U2) (pin 16))
      (node (ref P2) (pin 6)))
    (net (code 120) (name /LV_PHI2OUT)
      (node (ref U2) (pin 17))
      (node (ref P2) (pin 5)))
    (net (code 121) (name /LV_PHI1OUT)
      (node (ref U2) (pin 18))
      (node (ref P2) (pin 8)))
    (net (code 122) (name /LV_nML)
      (node (ref U2) (pin 19))
      (node (ref P2) (pin 7)))))