ADDRESS_MAP avrmap PPC405 0

    ADDRESS_SPACE rom_code RAMB16 [0x00000000:0x00003fff]
        BUS_BLOCK
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM8 [15:14];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM7 [13:12];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM6 [11:10];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM5 [ 9: 8];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM4 [ 7: 6];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM3 [ 5: 4];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM2 [ 3: 2];
	    core/mon/Inst_AVR8/PM_Inst/Mram_RAM1 [ 1: 0];
        END_BUS_BLOCK;
		  		  
    END_ADDRESS_SPACE;

END_ADDRESS_MAP;