# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal line has 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have the values:
# 0      key is not shifted for this keysym/scancode
# 1      key is shifted for this keysym/scancode
# 2      left shift
# 4      right shift
# 8      key can be shifted or not with this keysym/scancode
# 16     deshift key for this keysym/scancode
# 32     another definition for this keysym/scancode follows
# 64     shift lock
# 256    key is used for an alternative keyboard mapping
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key
# 'keysym -4 1' CAPS (ASCII/DIN) key
# 'keysym -5 n' joyport keypad, key n
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Symbolic Mapping, German Layout, C64, X11

#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT

# keys that can't be mapped symbolically are:
# (row0) arrow left (-> end), pound (-> ), clr/home (-> home)
# (row1) restore (-> F12)
# (row2) run/stop (-> escape)
# (row3) commodore (-> control)

# extra keys are:
# clr/home (-> altgr+\)
# ins/del (-> delete)
# ins/del+shift (-> insert)
# arrow left (-> underscore, ssharp, altgr+~)
# arrow up+shift (-> altgr+m)
# f1 (-> page up)
# f7 (-> page down)
# : (-> oe)
# :+shift (-> OE, altgr+[)
# ; (-> ae)
# ;+shift (-> AE, altgr+])
# @ (-> ue, altgr+Q)
# @+shift (-> UE)

#####################
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|

# inst/del
BackSpace      0 0 8
# extra: delete -> ins/del
Delete         0 0 8
# extra: insert -> shift+ins/del
Insert         0 0 1
# return
Return         0 1 8
# cursor r/l
Right          0 2 8
Left           0 2 1
# f7
F7             0 3 8
F8             0 3 1
# extra: pagedown -> f7
Page_Down      0 3 8
# f1
F1             0 4 8
F2             0 4 1
# extra: pagedown -> f1
Page_Up        0 4 8
# f3
F3             0 5 8
F4             0 5 1
# f4
F5             0 6 8
F6             0 6 1
# cursor u/d
Up             0 7 1
Down           0 7 8

#####################
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |

# shift+3
section        1 0 8
numbersign     1 0 1
# shift+4
dollar         1 3 8
# left shift
Shift_L        1 7 2
# shift lock
Caps_Lock      1 7 64

#####################
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |

# shift+5
percent        2 0 8
# shift+6
ampersand      2 3 8

#####################
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |

# shift+7
apostrophe     3 0 1
# shift+8
parenleft      3 3 8

#####################
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |

# shift+9
parenright     4 0 8

#####################
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |

# plus
plus           5 0 0
braceleft      5 0 1
# minus
minus          5 3 0
grave          5 3 8
braceright     5 3 1
# dot
period         5 4 8
greater        5 4 1
# colon
colon          5 5 0
# extra: oe -> colon
odiaeresis     5 5 0
# extra: OE -> :+shift
Odiaeresis     5 5 1
# extra: altgr+[ -> :+shift
bracketleft    5 5 1
# @-key
at             5 6 0
# extra: ue -> @
udiaeresis     5 6 8
# extra: UE -> @+shift
Udiaeresis     5 6 1
# comma
comma          5 7 8
less           5 7 1

#####################
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |

# pound
bar            6 0 8
brokenbar      6 0 8
acute          6 0 8
grave          6 0 8
# *
asterisk       6 1 16
# semicolon
semicolon      6 2 0
# extra: ae -> ;
adiaeresis     6 2 8
# extra: AE -> ;+shift
Adiaeresis     6 2 1
# extra: altgr+] -> ;+shift
bracketright   6 2 1
# clr/home
Home           6 3 8
# extra: altgr+\ -> clr/home
backslash      6 0 8
# right shift
Shift_R        6 4 4
# =
equal          6 5 16
# arrow up / pi
asciicircum    6 6 8
degree         6 6 8
# extra: altgr+m -> arrow up+shift (pi)
mu             6 6 1
# / ?
slash          6 7 16
question       6 7 8

#####################
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |

# shift+1
exclam         7 0 8
# left arrow
End            7 1 8
# extra: underscore -> arrow left
underscore     7 1 8
# extra: altgr+~ -> arrow left
asciitilde     7 1 8
# extra: ssharp -> arrow left
ssharp         7 1 8
# ctrl
Tab            7 2 8
ISO_Left_Tab   7 2 8
# Control_L      7 2 8
Control_R      7 2 8
# shift+2
quotedbl       7 3 8
# space
space          7 4 8
# cbm
Control_L      7 5 8
Alt_L      7 5 8
# run/stop
Escape         7 7 8

#####################
# letters and numbers

0 4 3 8
1 7 0 8
2 7 3 8
3 1 0 8
4 1 3 8
5 2 0 8
6 2 3 8
7 3 0 0
8 3 3 8
9 4 0 8

A 1 2 8
B 3 4 8
C 2 4 8
D 2 2 8
E 1 6 8
F 2 5 8
G 3 2 8
H 3 5 8
I 4 1 8
J 4 2 8
K 4 5 8
L 5 2 8
M 4 4 8
N 4 7 8
O 4 6 8
P 5 1 8
Q 7 6 8
R 2 1 8
S 1 5 8
T 2 6 8
U 3 6 8
V 3 7 8
W 1 1 8
X 2 7 8
Y 3 1 8
Z 1 4 8
a 1 2 8
b 3 4 8
c 2 4 8
d 2 2 8
e 1 6 8
f 2 5 8
g 3 2 8
h 3 5 8
i 4 1 8
j 4 2 8
k 4 5 8
l 5 2 8
m 4 4 8
n 4 7 8
o 4 6 8
p 5 1 8
q 7 6 8
r 2 1 8
s 1 5 8
t 2 6 8
u 3 6 8
v 3 7 8
w 1 1 8
x 2 7 8
y 3 1 8
z 1 4 8

#
# Restore key mappings
#
F12 -3 0
F12 -3 1

#
# joyport attached keypad
#
Num_Lock    -5 0
KP_7        -5 1
KP_8        -5 2
KP_9        -5 3
KP_Divide   -5 4
Scroll_Lock -5 5
KP_4        -5 6
KP_5        -5 7
KP_6        -5 8
KP_Multiply -5 9
Sys_Req     -5 10
KP_1        -5 11
KP_2        -5 12
KP_3        -5 13
KP_Subtract -5 14
Print       -5 15
KP_0        -5 16
KP_Delete   -5 17
KP_Enter    -5 18
KP_Add      -5 19
