Inlined call call __init

CONTROL FLOW GRAPH SSA

void main()
main: scope:[main]  from __start::@1
  to:main::@1
main::@1: scope:[main]  from main main::@2
  main::$0 = i < 7
  if(main::$0) goto main::@2
  to:main::@return
main::@2: scope:[main]  from main::@1
  SCREEN[i] = i
  i = ++ i
  to:main::@1
main::@return: scope:[main]  from main::@1
  return 
  to:@return

void __start()
__start: scope:[__start]  from
  to:__start::__init1
__start::__init1: scope:[__start]  from __start
  i = 3
  to:__start::@1
__start::@1: scope:[__start]  from __start::__init1
  call main
  to:__start::@2
__start::@2: scope:[__start]  from __start::@1
  to:__start::@return
__start::@return: scope:[__start]  from __start::@2
  return 
  to:@return

SYMBOL TABLE SSA
__constant char * const SCREEN = (char *)$400
void __start()
__loadstore char i // !zp[-1]:2
void main()
bool main::$0

Adding number conversion cast (unumber) 7 in main::$0 = i < 7
Successful SSA optimization PassNAddNumberTypeConversions
Simplifying constant pointer cast (char *) 1024
Simplifying constant integer cast 7
Successful SSA optimization PassNCastSimplification
Finalized unsigned number type (char) 7
Successful SSA optimization PassNFinalizeNumberTypeConversions
Simple Condition main::$0 [1] if(i<7) goto main::@2
Successful SSA optimization Pass2ConditionalJumpSimplification
Adding NOP phi() at start of __start
Adding NOP phi() at start of __start::@1
Adding NOP phi() at start of __start::@2
Adding NOP phi() at start of main
CALL GRAPH
Calls in [__start] to main:3 

Created 0 initial phi equivalence classes
Coalesced down to 0 phi equivalence classes
Culled Empty Block label __start::@2
Adding NOP phi() at start of __start
Adding NOP phi() at start of __start::@1
Adding NOP phi() at start of main

FINAL CONTROL FLOW GRAPH

void __start()
__start: scope:[__start]  from
  [0] phi()
  to:__start::__init1
__start::__init1: scope:[__start]  from __start
  [1] i = 3
  to:__start::@1
__start::@1: scope:[__start]  from __start::__init1
  [2] phi()
  [3] call main
  to:__start::@return
__start::@return: scope:[__start]  from __start::@1
  [4] return 
  to:@return

void main()
main: scope:[main]  from __start::@1
  [5] phi()
  to:main::@1
main::@1: scope:[main]  from main main::@2
  [6] if(i<7) goto main::@2
  to:main::@return
main::@return: scope:[main]  from main::@1
  [7] return 
  to:@return
main::@2: scope:[main]  from main::@1
  [8] SCREEN[i] = i
  [9] i = ++ i
  to:main::@1


VARIABLE REGISTER WEIGHTS
void __start()
__loadstore char i // !zp[-1]:2 84.49999999999999
void main()

Initial phi equivalence classes
Added variable i to live range equivalence class [ i ]
Complete equivalence classes
[ i ]
REGISTER UPLIFT POTENTIAL REGISTERS
Statement [1] i = 3 [ i ] (  [ i ] { }  ) always clobbers reg byte a 
Statement [6] if(i<7) goto main::@2 [ i ] ( main:3 [ i ] { }  ) always clobbers reg byte a 
Statement [8] SCREEN[i] = i [ i ] ( main:3 [ i ] { }  ) always clobbers reg byte a reg byte y 
Potential registers zp[1]:2 [ i ] : zp[1]:2 , 

REGISTER UPLIFT SCOPES
Uplift Scope [] 84.5: zp[1]:2 [ i ] 
Uplift Scope [main] 
Uplift Scope [__start] 

Uplifting [] best 374 combination zp[1]:2 [ i ] 
Uplifting [main] best 374 combination 
Uplifting [__start] best 374 combination 
Attempting to uplift remaining variables inzp[1]:2 [ i ]
Uplifting [] best 374 combination zp[1]:2 [ i ] 

ASSEMBLER BEFORE OPTIMIZATION
  // File Comments
// Test that address vars are turned into load/store and located at hardcoded addresses
// Hard-coded zero-page address - global variable
  // Upstart
  // Commodore 64 PRG executable file
.file [name="address-0.prg", type="prg", segments="Program"]
.segmentdef Program [segments="Basic, Code, Data"]
.segmentdef Basic [start=$0801]
.segmentdef Code [start=$80d]
.segmentdef Data [startAfter="Code"]
.segment Basic
:BasicUpstart(__start)
  // Global Constants & labels
  .label SCREEN = $400
  .label i = 2
.segment Code
  // __start
__start: {
    jmp __init1
    // __start::__init1
  __init1:
    // [1] i = 3 -- vbuz1=vbuc1 
    lda #3
    sta.z i
    // [2] phi from __start::__init1 to __start::@1 [phi:__start::__init1->__start::@1]
  __b1_from___init1:
    jmp __b1
    // __start::@1
  __b1:
    // [3] call main
    // [5] phi from __start::@1 to main [phi:__start::@1->main]
  main_from___b1:
    jsr main
    jmp __breturn
    // __start::@return
  __breturn:
    // [4] return 
    rts
}
  // main
main: {
    jmp __b1
    // main::@1
  __b1:
    // [6] if(i<7) goto main::@2 -- vbuz1_lt_vbuc1_then_la1 
    lda.z i
    cmp #7
    bcc __b2
    jmp __breturn
    // main::@return
  __breturn:
    // [7] return 
    rts
    // main::@2
  __b2:
    // [8] SCREEN[i] = i -- pbuc1_derefidx_vbuz1=vbuz1 
    ldy.z i
    tya
    sta SCREEN,y
    // [9] i = ++ i -- vbuz1=_inc_vbuz1 
    inc.z i
    jmp __b1
}
  // File Data

ASSEMBLER OPTIMIZATIONS
Removing instruction jmp __init1
Removing instruction jmp __b1
Removing instruction jmp __breturn
Removing instruction jmp __b1
Removing instruction jmp __breturn
Succesful ASM optimization Pass5NextJumpElimination
Removing instruction __b1_from___init1:
Removing instruction main_from___b1:
Succesful ASM optimization Pass5RedundantLabelElimination
Removing instruction __init1:
Removing instruction __b1:
Removing instruction __breturn:
Removing instruction __breturn:
Succesful ASM optimization Pass5UnusedLabelElimination

FINAL SYMBOL TABLE
__constant char * const SCREEN = (char *) 1024
void __start()
__loadstore char i // !zp[-1]:2 zp[1]:2 84.49999999999999
void main()

zp[1]:2 [ i ]


FINAL ASSEMBLER
Score: 278

  // File Comments
// Test that address vars are turned into load/store and located at hardcoded addresses
// Hard-coded zero-page address - global variable
  // Upstart
  // Commodore 64 PRG executable file
.file [name="address-0.prg", type="prg", segments="Program"]
.segmentdef Program [segments="Basic, Code, Data"]
.segmentdef Basic [start=$0801]
.segmentdef Code [start=$80d]
.segmentdef Data [startAfter="Code"]
.segment Basic
:BasicUpstart(__start)
  // Global Constants & labels
  .label SCREEN = $400
  .label i = 2
.segment Code
  // __start
__start: {
    // __start::__init1
    // char __address(0x02) i = 3
    // [1] i = 3 -- vbuz1=vbuc1 
    lda #3
    sta.z i
    // [2] phi from __start::__init1 to __start::@1 [phi:__start::__init1->__start::@1]
    // __start::@1
    // [3] call main
    // [5] phi from __start::@1 to main [phi:__start::@1->main]
    jsr main
    // __start::@return
    // [4] return 
    rts
}
  // main
main: {
    // main::@1
  __b1:
    // while(i<7)
    // [6] if(i<7) goto main::@2 -- vbuz1_lt_vbuc1_then_la1 
    lda.z i
    cmp #7
    bcc __b2
    // main::@return
    // }
    // [7] return 
    rts
    // main::@2
  __b2:
    // SCREEN[i++] = i
    // [8] SCREEN[i] = i -- pbuc1_derefidx_vbuz1=vbuz1 
    ldy.z i
    tya
    sta SCREEN,y
    // SCREEN[i++] = i;
    // [9] i = ++ i -- vbuz1=_inc_vbuz1 
    inc.z i
    jmp __b1
}
  // File Data

