__constant char * const BG_COLOR = (char *) 53281
__constant const char BLACK = 0
__constant char * const BORDER_COLOR = (char *) 53280
__constant struct MOS6526_CIA * const CIA1 = (struct MOS6526_CIA *) 56320
__constant const char CIA_INTERRUPT_CLEAR = $7f
__constant void (** const HARDWARE_IRQ)() = (void (**)()) 65534
__constant char * const IRQ_ENABLE = (char *) 53274
__constant const char IRQ_RASTER = 1
__constant char * const IRQ_STATUS = (char *) 53273
__constant char OFFSET_STRUCT_MOS6526_CIA_INTERRUPT = $d
__constant char * const PROCPORT = (char *) 1
__constant char * const PROCPORT_DDR = (char *) 0
__constant const char PROCPORT_DDR_MEMORY_MASK = 7
__constant const char PROCPORT_RAM_IO = 5
__constant char * const RASTER = (char *) 53266
__constant char * const VICII_CONTROL1 = (char *) 53265
__constant const char WHITE = 1
void do_irq()
__interrupt(hardware_clobber) void irq()
void main()

