__constant struct MOS6526_CIA * const CIA1 = (struct MOS6526_CIA *) 56320
__constant const char CIA_INTERRUPT_CLEAR = $7f
__constant char * const GHOST_BYTE = (char *) 16383
__constant void (** const HARDWARE_IRQ)() = (void (**)()) 65534
__constant const char IRQ_RASTER = 1
__constant char OFFSET_STRUCT_MOS6526_CIA_INTERRUPT = $d
__constant char OFFSET_STRUCT_MOS6569_VICII_BORDER_COLOR = $20
__constant char OFFSET_STRUCT_MOS6569_VICII_CONTROL1 = $11
__constant char OFFSET_STRUCT_MOS6569_VICII_IRQ_ENABLE = $1a
__constant char OFFSET_STRUCT_MOS6569_VICII_IRQ_STATUS = $19
__constant char OFFSET_STRUCT_MOS6569_VICII_RASTER = $12
__constant char * const PROCPORT = (char *) 1
__constant char * const PROCPORT_DDR = (char *) 0
__constant const char PROCPORT_DDR_MEMORY_MASK = 7
__constant const char PROCPORT_RAM_IO = 5
__constant const char RED = 2
__constant struct MOS6569_VICII * const VICII = (struct MOS6569_VICII *) 53248
__constant const char VICII_RSEL = 8
__constant const char WHITE = 1
__interrupt(hardware_clobber) void irq_bottom_1()
__interrupt(hardware_clobber) void irq_bottom_2()
void main()

