(export (version D)
  (design
    (source "D:/owncloud/Documents/Projects/RC6502/RC6502 VDU Color Amplifier/RC6502 VDU Color.sch")
    (date "20/02/2019 17:09:43")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 VDU Color.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C04594D))
    (comp (ref J3)
      (value VIDEO)
      (footprint Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x07))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0D33B4))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B8324))
    (comp (ref U1)
      (value MC1372)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib "RC6502 VDU Color-cache") (part MC1372))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B2F29))
    (comp (ref D1)
      (value 1N914)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B3590))
    (comp (ref R1)
      (value 360)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B38E2))
    (comp (ref R3)
      (value 560)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B4684))
    (comp (ref Q1)
      (value 2N3906)
      (footprint TO_SOT_Packages_THT:TO-92_Inline_Wide)
      (libsource (lib transistors) (part 2N3906))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B477E))
    (comp (ref R5)
      (value 3k3)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B4B7A))
    (comp (ref Q2)
      (value 2N3904)
      (footprint TO_SOT_Packages_THT:TO-92_Inline_Wide)
      (libsource (lib transistors) (part 2N3904))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B4E8D))
    (comp (ref R6)
      (value 470)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B523B))
    (comp (ref R7)
      (value 75)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B5761))
    (comp (ref R4)
      (value 3k9)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B6627))
    (comp (ref J1)
      (value Video_IN)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6C2ED6))
    (comp (ref J2)
      (value Video_OUT)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6C3428))
    (comp (ref RV1)
      (value 1k)
      (footprint Potentiometers:Potentiometer_Trimmer_Bourns_3296W)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6C8619))
    (comp (ref C3)
      (value 50pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6CCEE8))
    (comp (ref Y1)
      (value 3.579545)
      (footprint Crystals:Crystal_HC49-U_Vertical)
      (libsource (lib device) (part Crystal))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6CD17F))
    (comp (ref C4)
      (value 27pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6CD3B3))
    (comp (ref R2)
      (value 5k6)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6CE6DE))
    (comp (ref C5)
      (value 10uF)
      (footprint Capacitors_THT:CP_Radial_D4.0mm_P2.00mm)
      (libsource (lib device) (part CP_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6D2DE8))
    (comp (ref J4)
      (value OSC_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6D5C68)))
  (libparts
    (libpart (lib transistors) (part 2N3904)
      (description "40V Vce, 0.2A Ic, NPN, Small Signal Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3904)
        (field (name Footprint) TO_SOT_Packages_THT:TO-92_Molded_Narrow))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib transistors) (part 2N3906)
      (aliases
        (alias 2N3905))
      (description "-40V Vce, -0.2A Ic, PNP, Small Signal Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3906)
        (field (name Footprint) TO_SOT_Packages_THT:TO-92_Molded_Narrow))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP_Small)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib conn) (part Conn_01x04)
      (description "Generic connector, single row, 01x04")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib conn) (part Conn_01x07)
      (description "Generic connector, single row, 01x07")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x07))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))))
    (libpart (lib device) (part Crystal)
      (description "Two pin crystal")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib "RC6502 VDU Color-cache") (part MC1372)
      (fields
        (field (name Reference) U)
        (field (name Value) MC1372))
      (pins
        (pin (num 1) (name CLK_OUT) (type output))
        (pin (num 2) (name OSC_IN) (type input))
        (pin (num 3) (name DA) (type 3state))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name @B) (type input))
        (pin (num 6) (name CHB) (type input))
        (pin (num 7) (name @A) (type input))
        (pin (num 8) (name CHROMA_OUT) (type output))
        (pin (num 9) (name Y) (type input))
        (pin (num 10) (name CHROMA_IN) (type input))
        (pin (num 11) (name VCC) (type power_in))
        (pin (num 12) (name RF_OUT) (type output))
        (pin (num 13) (name RF1) (type input))
        (pin (num 14) (name RF0) (type input))))
    (libpart (lib device) (part POT)
      (description Potentiometer)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical transistors)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\transistors.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical "RC6502 VDU Color-cache")
      (uri "D:\\owncloud\\Documents\\Projects\\RC6502\\RC6502 VDU Color Amplifier\\RC6502 VDU Color-cache.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib")))
  (nets
    (net (code 1) (name /CHB)
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 2) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref RV1) (pin 2)))
    (net (code 3) (name /CLK)
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref J3) (pin 5)))
    (net (code 4) (name /Y)
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 9)))
    (net (code 5) (name /@A)
      (node (ref J3) (pin 3))
      (node (ref U1) (pin 7)))
    (net (code 6) (name /@B)
      (node (ref J3) (pin 2))
      (node (ref U1) (pin 5)))
    (net (code 7) (name GND)
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref C4) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref J3) (pin 6))
      (node (ref R5) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref J2) (pin 3))
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref C5) (pin 2)))
    (net (code 8) (name VIDEO)
      (node (ref R7) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 9) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 10) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 11) (name VCC)
      (node (ref U1) (pin 11))
      (node (ref C5) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 12) (name "Net-(J3-Pad4)")
      (node (ref J3) (pin 4)))
    (net (code 13) (name "Net-(RV1-Pad1)")
      (node (ref RV1) (pin 1)))
    (net (code 14) (name "Net-(J4-Pad1)")
      (node (ref J4) (pin 1)))
    (net (code 15) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2)))
    (net (code 16) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7)))
    (net (code 17) (name "Net-(C3-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref Y1) (pin 1))
      (node (ref C3) (pin 2)))
    (net (code 18) (name /OSC_IN)
      (node (ref U1) (pin 2))
      (node (ref Y1) (pin 2))
      (node (ref C4) (pin 2)))
    (net (code 19) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 20) (name "Net-(C2-Pad2)")
      (node (ref U1) (pin 8))
      (node (ref C2) (pin 2)))
    (net (code 21) (name "Net-(RV1-Pad3)")
      (node (ref U1) (pin 10))
      (node (ref RV1) (pin 3)))
    (net (code 22) (name "Net-(D1-Pad1)")
      (node (ref U1) (pin 13))
      (node (ref D1) (pin 1)))
    (net (code 23) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 14))
      (node (ref R1) (pin 2)))
    (net (code 24) (name "Net-(Q1-Pad3)")
      (node (ref R5) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref Q2) (pin 2)))
    (net (code 25) (name "Net-(Q2-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref Q2) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 26) (name "Net-(Q1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 27) (name "Net-(Q1-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U1) (pin 12))
      (node (ref Q1) (pin 2))
      (node (ref R4) (pin 2)))))