(export (version D)
  (design
    (source "D:/ownCloud/Documents/Projects/RC6502/RC6502 General Video Adapter/RC6502 General Video Adapter.sch")
    (date "17/06/2017 16:52:47")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 General Video Adapter.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J3)
      (value CONN_01X39)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X39))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942C0A9))
    (comp (ref J2)
      (value Video)
      (footprint rca:rca_yellow)
      (libsource (lib rca) (part RCA_PLUG))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942C0BB))
    (comp (ref J1)
      (value "General Video Connector")
      (footprint Connectors:IDC_Header_Straight_40pins)
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942C0BE))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942C0C0))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942C0C1))
    (comp (ref U13)
      (value 74HCT373)
      (footprint Housings_DIP:DIP-20_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS373))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942EDB7))
    (comp (ref U12)
      (value 74HCT373)
      (footprint Housings_DIP:DIP-20_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS373))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942F086))
    (comp (ref U11)
      (value 74HCT373)
      (footprint Housings_DIP:DIP-20_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS373))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942F323))
    (comp (ref U16)
      (value 74HCT00)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS00))
      (sheetpath (names /) (tstamps /))
      (tstamp 5942FCA2))
    (comp (ref U15)
      (value 74HCT32)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS32))
      (sheetpath (names /) (tstamps /))
      (tstamp 59432819))
    (comp (ref U17)
      (value 74HCT04)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS04))
      (sheetpath (names /) (tstamps /))
      (tstamp 59438AAE))
    (comp (ref U14)
      (value 74HCT86)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS86))
      (sheetpath (names /) (tstamps /))
      (tstamp 594395D3))
    (comp (ref U6)
      (value 74HCT86)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS86))
      (sheetpath (names /) (tstamps /))
      (tstamp 5943976D))
    (comp (ref U10)
      (value CY7C199)
      (footprint Housings_DIP:DIP-28_W7.62mm_Socket)
      (libsource (lib cypress) (part CY7C199))
      (sheetpath (names /) (tstamps /))
      (tstamp 59442397))
    (comp (ref C20)
      (value 470pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59456FEA))
    (comp (ref R17)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5947320E))
    (comp (ref R16)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5947822C))
    (comp (ref R15)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 594782A4))
    (comp (ref R14)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5947831D))
    (comp (ref R13)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478399))
    (comp (ref R12)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478414))
    (comp (ref R11)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478492))
    (comp (ref R10)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478513))
    (comp (ref R9)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 594787DB))
    (comp (ref R8)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478862))
    (comp (ref R7)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 594788EC))
    (comp (ref R6)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478979))
    (comp (ref R5)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478BC1))
    (comp (ref R4)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59478C5A))
    (comp (ref U3)
      (value 74HCT04)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS04))
      (sheetpath (names /) (tstamps /))
      (tstamp 594868F5))
    (comp (ref U7)
      (value 74HCT04)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS04))
      (sheetpath (names /) (tstamps /))
      (tstamp 59486E5E))
    (comp (ref R1)
      (value 47k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948AA3F))
    (comp (ref R3)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948C4E6))
    (comp (ref Y1)
      (value "8 Mhz")
      (footprint Crystals:Crystal_HC49-4H_Vertical)
      (libsource (lib device) (part Crystal_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948D0CD))
    (comp (ref C26)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948E4FA))
    (comp (ref C25)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59490A90))
    (comp (ref D8)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5949D5B5))
    (comp (ref D1)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A49A2))
    (comp (ref D9)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A4A7F))
    (comp (ref D2)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A4B51))
    (comp (ref D10)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A4C2A))
    (comp (ref D3)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A4D00))
    (comp (ref D11)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A4DD9))
    (comp (ref D4)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A4EB7))
    (comp (ref D12)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A51A0))
    (comp (ref D5)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5280))
    (comp (ref D13)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5365))
    (comp (ref D6)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5449))
    (comp (ref D14)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5A55))
    (comp (ref D15)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5B43))
    (comp (ref D7)
      (value BAT42)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5C32))
    (comp (ref R2)
      (value 680)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 594AA97C))
    (comp (ref C27)
      (value 470pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594AFB22))
    (comp (ref RV1)
      (value 5k)
      (footprint Potentiometers:Potentiometer_Trimmer_Bourns_3296W)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 594B1408))
    (comp (ref U4)
      (value 74HCT08)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS08))
      (sheetpath (names /) (tstamps /))
      (tstamp 594DC9F0))
    (comp (ref U5)
      (value 74HCT08)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS08))
      (sheetpath (names /) (tstamps /))
      (tstamp 5954BB79))
    (comp (ref U9)
      (value 74HCT165)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS165))
      (sheetpath (names /) (tstamps /))
      (tstamp 5956A8E3))
    (comp (ref RV2)
      (value 10k)
      (footprint Potentiometers:Potentiometer_Trimmer_Bourns_3296W)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5958E190))
    (comp (ref D16)
      (value 1N4848)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59594811))
    (comp (ref R18)
      (value 1k8)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5959EE0F))
    (comp (ref Q1)
      (value BC547)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib transistors) (part BC547))
      (sheetpath (names /) (tstamps /))
      (tstamp 595A1E86))
    (comp (ref R19)
      (value 2k2)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 595A3886))
    (comp (ref R20)
      (value 75)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 595A39C9))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BC75C))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BC762))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BCEBC))
    (comp (ref C7)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BCEC2))
    (comp (ref C8)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BCEC8))
    (comp (ref C9)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BCECE))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD31D))
    (comp (ref C11)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD323))
    (comp (ref C12)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD329))
    (comp (ref C13)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD32F))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD335))
    (comp (ref C15)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD33B))
    (comp (ref C16)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD341))
    (comp (ref C17)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596BD347))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 596C5EDB))
    (comp (ref U1)
      (value 4040_vcc)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 4040) (part 4040_vcc))
      (sheetpath (names /) (tstamps /))
      (tstamp 597253FB))
    (comp (ref U2)
      (value 4040_vcc)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 4040) (part 4040_vcc))
      (sheetpath (names /) (tstamps /))
      (tstamp 59726C94)))
  (libparts
    (libpart (lib 4040) (part 4040_vcc)
      (description "Binary Counter 12 stages (Asynchronous)")
      (docs cmos4000/MC14040.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 4040_vcc))
      (pins
        (pin (num 1) (name Q11) (type output))
        (pin (num 2) (name Q5) (type output))
        (pin (num 3) (name Q4) (type output))
        (pin (num 4) (name Q6) (type output))
        (pin (num 5) (name Q3) (type output))
        (pin (num 6) (name Q2) (type output))
        (pin (num 7) (name Q1) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name Q0) (type output))
        (pin (num 10) (name CLK) (type input))
        (pin (num 11) (name Reset) (type input))
        (pin (num 12) (name Q8) (type output))
        (pin (num 13) (name Q7) (type output))
        (pin (num 14) (name Q9) (type output))
        (pin (num 15) (name Q10) (type output))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS00)
      (aliases
        (alias 74LS37)
        (alias 7400)
        (alias 74HCT00)
        (alias 74HC00))
      (description "Quad nand2")
      (footprints
        (fp 14DIP300*)
        (fp SO14*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS00))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS04)
      (description "Hex Inverseur")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS04))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type output))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type output))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type output))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type output))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS08)
      (aliases
        (alias 74LS09))
      (description "Quad And2")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS08))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS165)
      (description "Shift Register 8 bits, parallel load")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS165))
      (pins
        (pin (num 1) (name Pl) (type input))
        (pin (num 2) (name CP) (type input))
        (pin (num 3) (name P4) (type input))
        (pin (num 4) (name P5) (type input))
        (pin (num 5) (name P6) (type input))
        (pin (num 6) (name P7) (type input))
        (pin (num 7) (name ~Q7) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name Q7) (type output))
        (pin (num 10) (name Ds) (type input))
        (pin (num 11) (name P0) (type input))
        (pin (num 12) (name P1) (type input))
        (pin (num 13) (name P2) (type input))
        (pin (num 14) (name P3) (type input))
        (pin (num 15) (name CE) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS32)
      (description "Quad Or 2 inputs")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS32))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS373)
      (description "8 bits Latch, 3 state Out")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS373))
      (pins
        (pin (num 1) (name OE) (type input))
        (pin (num 2) (name O0) (type 3state))
        (pin (num 3) (name D0) (type input))
        (pin (num 4) (name D1) (type input))
        (pin (num 5) (name O1) (type 3state))
        (pin (num 6) (name O2) (type 3state))
        (pin (num 7) (name D2) (type input))
        (pin (num 8) (name D3) (type input))
        (pin (num 9) (name O3) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name LE) (type input))
        (pin (num 12) (name O4) (type 3state))
        (pin (num 13) (name D4) (type input))
        (pin (num 14) (name D5) (type input))
        (pin (num 15) (name O5) (type 3state))
        (pin (num 16) (name O6) (type 3state))
        (pin (num 17) (name D6) (type input))
        (pin (num 18) (name D7) (type input))
        (pin (num 19) (name O7) (type 3state))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS86)
      (aliases
        (alias 74HC86))
      (description "Quad XOR 2 inputs")
      (docs 74xx/74ls86.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS86))
      (pins
        (pin (num 1) (name IN1) (type input))
        (pin (num 2) (name IN2) (type input))
        (pin (num 3) (name OUT) (type output))
        (pin (num 4) (name IN1) (type input))
        (pin (num 5) (name IN2) (type input))
        (pin (num 6) (name OUT) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT) (type output))
        (pin (num 9) (name IN1) (type input))
        (pin (num 10) (name IN2) (type input))
        (pin (num 11) (name OUT) (type output))
        (pin (num 12) (name IN1) (type input))
        (pin (num 13) (name IN2) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib transistors) (part BC547)
      (aliases
        (alias BC546)
        (alias BC548)
        (alias BC549)
        (alias BC550))
      (description "45V Vce, 0.1A Ic, NPN, Small Signal Transistor, TO-92")
      (docs http://www.fairchildsemi.com/ds/BC/BC547.pdf)
      (footprints
        (fp TO-92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC547)
        (field (name Footprint) TO_SOT_Packages_THT:TO-92_Molded_Narrow))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib conn) (part CONN_01X39)
      (description "Connector, single row, 01x39, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X39))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))))
    (libpart (lib conn) (part CONN_02X20)
      (description "Connector, double row, 02x20, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X20))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))))
    (libpart (lib cypress) (part CY7C199)
      (fields
        (field (name Reference) U)
        (field (name Value) CY7C199))
      (pins
        (pin (num 1) (name A5) (type input))
        (pin (num 2) (name A6) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A8) (type input))
        (pin (num 5) (name A9) (type input))
        (pin (num 6) (name A10) (type input))
        (pin (num 7) (name A11) (type input))
        (pin (num 8) (name A12) (type input))
        (pin (num 9) (name A13) (type input))
        (pin (num 10) (name A14) (type input))
        (pin (num 11) (name D0) (type 3state))
        (pin (num 12) (name D1) (type 3state))
        (pin (num 13) (name D2) (type 3state))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name D3) (type 3state))
        (pin (num 16) (name D4) (type 3state))
        (pin (num 17) (name D5) (type 3state))
        (pin (num 18) (name D6) (type 3state))
        (pin (num 19) (name D7) (type 3state))
        (pin (num 20) (name ~CE~) (type input))
        (pin (num 21) (name A0) (type input))
        (pin (num 22) (name ~OE~) (type input))
        (pin (num 23) (name A1) (type input))
        (pin (num 24) (name A2) (type input))
        (pin (num 25) (name A3) (type input))
        (pin (num 26) (name A4) (type input))
        (pin (num 27) (name ~WE~) (type input))
        (pin (num 28) (name VCC) (type power_in))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal_Small)
      (description "Two pin crystal, small symbol")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part D_Schottky_Small)
      (description "Schottky diode, small symbol")
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part D_Small)
      (description "Diode, small symbol")
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentionmeter)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib rca) (part RCA_PLUG)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) RCA_PLUG))
      (pins
        (pin (num 1) (name Ext) (type passive))
        (pin (num 2) (name In) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\74xx.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical cypress)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\cypress.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical transistors)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\transistors.lib"))
    (library (logical rca)
      (uri "D:\\ownCloud\\Documents\\Projects\\RC6502\\RC6502 General Video Adapter\\rca.lib"))
    (library (logical 4040)
      (uri "D:\\ownCloud\\Documents\\Projects\\RC6502\\RC6502 General Video Adapter\\4040.lib")))
  (nets
    (net (code 1) (name GND)
      (node (ref C27) (pin 2))
      (node (ref U17) (pin 3))
      (node (ref U15) (pin 10))
      (node (ref U15) (pin 9))
      (node (ref U9) (pin 8))
      (node (ref U15) (pin 4))
      (node (ref U15) (pin 13))
      (node (ref U15) (pin 12))
      (node (ref U15) (pin 5))
      (node (ref U14) (pin 5))
      (node (ref U14) (pin 4))
      (node (ref U10) (pin 14))
      (node (ref U6) (pin 12))
      (node (ref U6) (pin 7))
      (node (ref C20) (pin 2))
      (node (ref U10) (pin 10))
      (node (ref R20) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref U14) (pin 7))
      (node (ref U14) (pin 10))
      (node (ref U2) (pin 8))
      (node (ref C4) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref C6) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U9) (pin 15))
      (node (ref U9) (pin 10))
      (node (ref C15) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U14) (pin 9))
      (node (ref U5) (pin 7))
      (node (ref U15) (pin 7))
      (node (ref U17) (pin 7))
      (node (ref U16) (pin 7))
      (node (ref U7) (pin 7))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref U13) (pin 10))
      (node (ref J1) (pin 1))
      (node (ref J1) (pin 39))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 40))
      (node (ref U11) (pin 10))
      (node (ref J1) (pin 37))
      (node (ref U10) (pin 20))
      (node (ref J3) (pin 17))
      (node (ref U13) (pin 17))
      (node (ref U12) (pin 10))
      (node (ref U3) (pin 7))
      (node (ref U13) (pin 18))
      (node (ref U4) (pin 7)))
    (net (code 2) (name VCC)
      (node (ref C8) (pin 2))
      (node (ref U16) (pin 2))
      (node (ref U16) (pin 14))
      (node (ref J3) (pin 18))
      (node (ref U1) (pin 16))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref U16) (pin 9))
      (node (ref U2) (pin 16))
      (node (ref C7) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref U15) (pin 14))
      (node (ref U11) (pin 20))
      (node (ref U12) (pin 20))
      (node (ref U13) (pin 20))
      (node (ref U10) (pin 28))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U14) (pin 14))
      (node (ref U5) (pin 14))
      (node (ref R18) (pin 2))
      (node (ref U3) (pin 14))
      (node (ref U17) (pin 14))
      (node (ref U9) (pin 16))
      (node (ref U4) (pin 14))
      (node (ref C3) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref U6) (pin 14))
      (node (ref C11) (pin 2))
      (node (ref U7) (pin 14))
      (node (ref C12) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C4) (pin 2)))
    (net (code 3) (name N7)
      (node (ref U1) (pin 13))
      (node (ref U4) (pin 4))
      (node (ref R8) (pin 2))
      (node (ref D4) (pin 1)))
    (net (code 4) (name HSYNC)
      (node (ref U4) (pin 8))
      (node (ref U6) (pin 1)))
    (net (code 5) (name N6)
      (node (ref U4) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref D11) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 6) (name N5)
      (node (ref D3) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref U4) (pin 1)))
    (net (code 7) (name "Net-(U4-Pad13)")
      (node (ref U7) (pin 2))
      (node (ref U4) (pin 13)))
    (net (code 8) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 9))
      (node (ref U4) (pin 3)))
    (net (code 9) (name "Net-(U4-Pad10)")
      (node (ref U4) (pin 10))
      (node (ref U4) (pin 6)))
    (net (code 10) (name "Net-(U4-Pad12)")
      (node (ref U6) (pin 8))
      (node (ref U4) (pin 12)))
    (net (code 11) (name N3)
      (node (ref D2) (pin 1))
      (node (ref U17) (pin 13))
      (node (ref U1) (pin 5))
      (node (ref R4) (pin 2))
      (node (ref U14) (pin 12))
      (node (ref U6) (pin 10)))
    (net (code 12) (name N9)
      (node (ref D5) (pin 1))
      (node (ref U1) (pin 14))
      (node (ref R10) (pin 2)))
    (net (code 13) (name N1)
      (node (ref U14) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 14) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 15) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 16) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 17) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 18) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 19) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 20) (name N15)
      (node (ref R16) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 21) (name N17)
      (node (ref U2) (pin 2))
      (node (ref U5) (pin 13))
      (node (ref U7) (pin 1))
      (node (ref D15) (pin 1)))
    (net (code 22) (name N13)
      (node (ref U5) (pin 4))
      (node (ref R14) (pin 2))
      (node (ref D14) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 23) (name "Net-(U5-Pad1)")
      (node (ref U5) (pin 1))
      (node (ref U7) (pin 4)))
    (net (code 24) (name "Net-(U5-Pad10)")
      (node (ref U5) (pin 6))
      (node (ref U5) (pin 10)))
    (net (code 25) (name "Net-(U5-Pad12)")
      (node (ref U5) (pin 8))
      (node (ref U5) (pin 12)))
    (net (code 26) (name "Net-(U5-Pad2)")
      (node (ref U7) (pin 6))
      (node (ref U5) (pin 2)))
    (net (code 27) (name "Net-(U5-Pad3)")
      (node (ref U5) (pin 9))
      (node (ref U5) (pin 3)))
    (net (code 28) (name "Net-(U5-Pad5)")
      (node (ref U5) (pin 5))
      (node (ref U7) (pin 8)))
    (net (code 29) (name N11)
      (node (ref U1) (pin 1))
      (node (ref U7) (pin 3))
      (node (ref D6) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref U2) (pin 10)))
    (net (code 30) (name "Net-(U3-Pad9)")
      (node (ref U4) (pin 11))
      (node (ref U3) (pin 9))
      (node (ref U6) (pin 4)))
    (net (code 31) (name SYNC)
      (node (ref U7) (pin 10))
      (node (ref D16) (pin 1)))
    (net (code 32) (name "Net-(U7-Pad13)")
      (node (ref U9) (pin 7))
      (node (ref U7) (pin 13)))
    (net (code 33) (name LUMA)
      (node (ref RV2) (pin 2))
      (node (ref U7) (pin 12))
      (node (ref RV2) (pin 3)))
    (net (code 34) (name "Net-(U6-Pad3)")
      (node (ref U7) (pin 11))
      (node (ref U6) (pin 3)))
    (net (code 35) (name SHIFT_LOAD)
      (node (ref U9) (pin 1))
      (node (ref U6) (pin 6)))
    (net (code 36) (name "Net-(C26-Pad2)")
      (node (ref Y1) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref C26) (pin 2)))
    (net (code 37) (name "Net-(C25-Pad2)")
      (node (ref U3) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref Y1) (pin 1)))
    (net (code 38) (name "Net-(U3-Pad12)")
      (node (ref U6) (pin 5))
      (node (ref U3) (pin 12)))
    (net (code 39) (name "Net-(C27-Pad1)")
      (node (ref C27) (pin 1))
      (node (ref U6) (pin 11))
      (node (ref RV1) (pin 3)))
    (net (code 40) (name "Net-(D1-Pad2)")
      (node (ref R2) (pin 1))
      (node (ref D15) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref D12) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref D13) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref D14) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref D10) (pin 2))
      (node (ref D11) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref D9) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref U6) (pin 13))
      (node (ref D3) (pin 2)))
    (net (code 41) (name "Net-(U14-Pad8)")
      (node (ref U14) (pin 8)))
    (net (code 42) (name "Net-(U14-Pad6)")
      (node (ref U14) (pin 6)))
    (net (code 43) (name "Net-(U15-Pad6)")
      (node (ref U15) (pin 6)))
    (net (code 44) (name "Net-(U15-Pad11)")
      (node (ref U15) (pin 11)))
    (net (code 45) (name "Net-(U15-Pad8)")
      (node (ref U15) (pin 8)))
    (net (code 46) (name "Net-(U17-Pad4)")
      (node (ref U17) (pin 4)))
    (net (code 47) (name N10)
      (node (ref R11) (pin 2))
      (node (ref D13) (pin 1))
      (node (ref U1) (pin 15)))
    (net (code 48) (name N8)
      (node (ref U4) (pin 5))
      (node (ref D12) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref U1) (pin 12)))
    (net (code 49) (name CLOCK)
      (node (ref U9) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref U1) (pin 10)))
    (net (code 50) (name N0)
      (node (ref U1) (pin 9))
      (node (ref D8) (pin 1)))
    (net (code 51) (name N2)
      (node (ref D9) (pin 1))
      (node (ref U6) (pin 9))
      (node (ref U1) (pin 6))
      (node (ref U14) (pin 2)))
    (net (code 52) (name N4)
      (node (ref U1) (pin 3))
      (node (ref R5) (pin 2))
      (node (ref D10) (pin 1)))
    (net (code 53) (name N14)
      (node (ref R15) (pin 2))
      (node (ref U7) (pin 9))
      (node (ref U2) (pin 6))
      (node (ref D7) (pin 1)))
    (net (code 54) (name RESET)
      (node (ref U2) (pin 11))
      (node (ref RV1) (pin 1))
      (node (ref U1) (pin 11))
      (node (ref RV1) (pin 2)))
    (net (code 55) (name N12)
      (node (ref R13) (pin 2))
      (node (ref U2) (pin 9))
      (node (ref U7) (pin 5)))
    (net (code 56) (name N16)
      (node (ref U2) (pin 3))
      (node (ref R17) (pin 2)))
    (net (code 57) (name "Net-(U9-Pad9)")
      (node (ref U9) (pin 9)))
    (net (code 58) (name D3)
      (node (ref U10) (pin 15))
      (node (ref U11) (pin 9))
      (node (ref U9) (pin 14)))
    (net (code 59) (name VSYNC)
      (node (ref U6) (pin 2))
      (node (ref U5) (pin 11)))
    (net (code 60) (name D5)
      (node (ref U11) (pin 15))
      (node (ref U9) (pin 4))
      (node (ref U10) (pin 17)))
    (net (code 61) (name D2)
      (node (ref U9) (pin 13))
      (node (ref U10) (pin 13))
      (node (ref U11) (pin 6)))
    (net (code 62) (name D1)
      (node (ref U11) (pin 5))
      (node (ref U9) (pin 12))
      (node (ref U10) (pin 12)))
    (net (code 63) (name D0)
      (node (ref U10) (pin 11))
      (node (ref U11) (pin 2))
      (node (ref U9) (pin 11)))
    (net (code 64) (name D7)
      (node (ref U11) (pin 19))
      (node (ref U9) (pin 6))
      (node (ref U10) (pin 19)))
    (net (code 65) (name D6)
      (node (ref U9) (pin 5))
      (node (ref U10) (pin 18))
      (node (ref U11) (pin 16)))
    (net (code 66) (name D4)
      (node (ref U9) (pin 3))
      (node (ref U10) (pin 16))
      (node (ref U11) (pin 12)))
    (net (code 67) (name "Net-(J3-Pad36)")
      (node (ref J3) (pin 36)))
    (net (code 68) (name "Net-(J3-Pad35)")
      (node (ref J3) (pin 35)))
    (net (code 69) (name "Net-(D16-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref D16) (pin 2))
      (node (ref R18) (pin 1))
      (node (ref RV2) (pin 1)))
    (net (code 70) (name "Net-(J2-Pad2)")
      (node (ref R20) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref Q1) (pin 3)))
    (net (code 71) (name "Net-(J3-Pad24)")
      (node (ref J3) (pin 24)))
    (net (code 72) (name "Net-(U13-Pad19)")
      (node (ref U13) (pin 19)))
    (net (code 73) (name "Net-(U13-Pad16)")
      (node (ref U13) (pin 16)))
    (net (code 74) (name TRAN_OE)
      (node (ref U13) (pin 1))
      (node (ref U11) (pin 1))
      (node (ref U17) (pin 1))
      (node (ref U14) (pin 3))
      (node (ref C20) (pin 1))
      (node (ref U12) (pin 1)))
    (net (code 75) (name "Net-(U15-Pad3)")
      (node (ref U15) (pin 3))
      (node (ref U16) (pin 1)))
    (net (code 76) (name GV_CS)
      (node (ref U16) (pin 12))
      (node (ref U15) (pin 2))
      (node (ref J1) (pin 11)))
    (net (code 77) (name GV_RW)
      (node (ref J1) (pin 36))
      (node (ref U15) (pin 1)))
    (net (code 78) (name "Net-(U14-Pad13)")
      (node (ref U14) (pin 13))
      (node (ref U17) (pin 8)))
    (net (code 79) (name "Net-(U17-Pad11)")
      (node (ref U17) (pin 12))
      (node (ref U17) (pin 11)))
    (net (code 80) (name "Net-(U17-Pad10)")
      (node (ref U17) (pin 9))
      (node (ref U17) (pin 10)))
    (net (code 81) (name "Net-(U16-Pad13)")
      (node (ref U16) (pin 13))
      (node (ref U17) (pin 6)))
    (net (code 82) (name "Net-(U14-Pad11)")
      (node (ref U14) (pin 11))
      (node (ref U17) (pin 5)))
    (net (code 83) (name "Net-(U16-Pad10)")
      (node (ref U16) (pin 6))
      (node (ref U16) (pin 10)))
    (net (code 84) (name "Net-(U16-Pad3)")
      (node (ref U16) (pin 3))
      (node (ref U16) (pin 5)))
    (net (code 85) (name "Net-(J3-Pad12)")
      (node (ref J3) (pin 12)))
    (net (code 86) (name GV_E)
      (node (ref U16) (pin 4))
      (node (ref J1) (pin 38)))
    (net (code 87) (name "Net-(J3-Pad23)")
      (node (ref J3) (pin 23)))
    (net (code 88) (name "Net-(J3-Pad8)")
      (node (ref J3) (pin 8)))
    (net (code 89) (name "Net-(J3-Pad9)")
      (node (ref J3) (pin 9)))
    (net (code 90) (name "Net-(J3-Pad10)")
      (node (ref J3) (pin 10)))
    (net (code 91) (name "Net-(J3-Pad11)")
      (node (ref J3) (pin 11)))
    (net (code 92) (name "Net-(J3-Pad13)")
      (node (ref J3) (pin 13)))
    (net (code 93) (name "Net-(J3-Pad14)")
      (node (ref J3) (pin 14)))
    (net (code 94) (name "Net-(J3-Pad21)")
      (node (ref J3) (pin 21)))
    (net (code 95) (name "Net-(J3-Pad39)")
      (node (ref J3) (pin 39)))
    (net (code 96) (name "Net-(J3-Pad25)")
      (node (ref J3) (pin 25)))
    (net (code 97) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7)))
    (net (code 98) (name "Net-(J3-Pad38)")
      (node (ref J3) (pin 38)))
    (net (code 99) (name "Net-(J3-Pad29)")
      (node (ref J3) (pin 29)))
    (net (code 100) (name "Net-(J3-Pad19)")
      (node (ref J3) (pin 19)))
    (net (code 101) (name "Net-(J3-Pad28)")
      (node (ref J3) (pin 28)))
    (net (code 102) (name "Net-(J3-Pad37)")
      (node (ref J3) (pin 37)))
    (net (code 103) (name "Net-(J3-Pad33)")
      (node (ref J3) (pin 33)))
    (net (code 104) (name "Net-(J3-Pad16)")
      (node (ref J3) (pin 16)))
    (net (code 105) (name "Net-(J3-Pad15)")
      (node (ref J3) (pin 15)))
    (net (code 106) (name "Net-(J3-Pad4)")
      (node (ref J3) (pin 4)))
    (net (code 107) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3)))
    (net (code 108) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2)))
    (net (code 109) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1)))
    (net (code 110) (name "Net-(J3-Pad34)")
      (node (ref J3) (pin 34)))
    (net (code 111) (name "Net-(J3-Pad27)")
      (node (ref J3) (pin 27)))
    (net (code 112) (name "Net-(J3-Pad32)")
      (node (ref J3) (pin 32)))
    (net (code 113) (name "Net-(J3-Pad31)")
      (node (ref J3) (pin 31)))
    (net (code 114) (name "Net-(J3-Pad30)")
      (node (ref J3) (pin 30)))
    (net (code 115) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5)))
    (net (code 116) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6)))
    (net (code 117) (name "Net-(J3-Pad20)")
      (node (ref J3) (pin 20)))
    (net (code 118) (name "Net-(J3-Pad26)")
      (node (ref J3) (pin 26)))
    (net (code 119) (name "Net-(J3-Pad22)")
      (node (ref J3) (pin 22)))
    (net (code 120) (name GV_A13)
      (node (ref U13) (pin 14))
      (node (ref J1) (pin 29)))
    (net (code 121) (name GV_A8)
      (node (ref U13) (pin 3))
      (node (ref J1) (pin 19)))
    (net (code 122) (name GV_A4)
      (node (ref J1) (pin 28))
      (node (ref U12) (pin 13)))
    (net (code 123) (name GV_D7)
      (node (ref U11) (pin 18))
      (node (ref J1) (pin 18)))
    (net (code 124) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 125) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 126) (name "Net-(J1-Pad33)")
      (node (ref J1) (pin 33)))
    (net (code 127) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 128) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 129) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 130) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 131) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 132) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 133) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 134) (name GV_A9)
      (node (ref U13) (pin 4))
      (node (ref J1) (pin 21)))
    (net (code 135) (name GV_A5)
      (node (ref J1) (pin 30))
      (node (ref U12) (pin 14)))
    (net (code 136) (name GV_A0)
      (node (ref U12) (pin 3))
      (node (ref J1) (pin 20)))
    (net (code 137) (name GV_D3)
      (node (ref U11) (pin 8))
      (node (ref J1) (pin 10)))
    (net (code 138) (name GV_D2)
      (node (ref U11) (pin 7))
      (node (ref J1) (pin 8)))
    (net (code 139) (name GV_D1)
      (node (ref J1) (pin 6))
      (node (ref U11) (pin 4)))
    (net (code 140) (name GV_D0)
      (node (ref U11) (pin 3))
      (node (ref J1) (pin 4)))
    (net (code 141) (name GV_A7)
      (node (ref U12) (pin 18))
      (node (ref J1) (pin 34)))
    (net (code 142) (name GV_A12)
      (node (ref U13) (pin 13))
      (node (ref J1) (pin 27)))
    (net (code 143) (name GV_A3)
      (node (ref J1) (pin 26))
      (node (ref U12) (pin 8)))
    (net (code 144) (name GV_D6)
      (node (ref J1) (pin 16))
      (node (ref U11) (pin 17)))
    (net (code 145) (name GV_A11)
      (node (ref U13) (pin 8))
      (node (ref J1) (pin 25)))
    (net (code 146) (name GV_A2)
      (node (ref U12) (pin 7))
      (node (ref J1) (pin 24)))
    (net (code 147) (name GV_D5)
      (node (ref U11) (pin 14))
      (node (ref J1) (pin 14)))
    (net (code 148) (name GV_A10)
      (node (ref J1) (pin 23))
      (node (ref U13) (pin 7)))
    (net (code 149) (name GV_A6)
      (node (ref U12) (pin 17))
      (node (ref J1) (pin 32)))
    (net (code 150) (name GV_A1)
      (node (ref U12) (pin 4))
      (node (ref J1) (pin 22)))
    (net (code 151) (name GV_D4)
      (node (ref J1) (pin 12))
      (node (ref U11) (pin 13)))
    (net (code 152) (name A9)
      (node (ref U10) (pin 5))
      (node (ref R13) (pin 1))
      (node (ref U13) (pin 5)))
    (net (code 153) (name A10)
      (node (ref U13) (pin 6))
      (node (ref R14) (pin 1))
      (node (ref U10) (pin 6)))
    (net (code 154) (name A11)
      (node (ref U13) (pin 9))
      (node (ref R15) (pin 1))
      (node (ref U10) (pin 7)))
    (net (code 155) (name A12)
      (node (ref U13) (pin 12))
      (node (ref U10) (pin 8))
      (node (ref R16) (pin 1)))
    (net (code 156) (name TRAN_LE)
      (node (ref U11) (pin 11))
      (node (ref U16) (pin 8))
      (node (ref U13) (pin 11))
      (node (ref U12) (pin 11)))
    (net (code 157) (name A4)
      (node (ref U10) (pin 26))
      (node (ref R8) (pin 1))
      (node (ref U12) (pin 12)))
    (net (code 158) (name A0)
      (node (ref U10) (pin 21))
      (node (ref U12) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 159) (name A1)
      (node (ref R5) (pin 1))
      (node (ref U10) (pin 23))
      (node (ref U12) (pin 5)))
    (net (code 160) (name A2)
      (node (ref U12) (pin 6))
      (node (ref R6) (pin 1))
      (node (ref U10) (pin 24)))
    (net (code 161) (name A3)
      (node (ref R7) (pin 1))
      (node (ref U12) (pin 9))
      (node (ref U10) (pin 25)))
    (net (code 162) (name A5)
      (node (ref U12) (pin 15))
      (node (ref U10) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 163) (name A6)
      (node (ref U10) (pin 2))
      (node (ref U12) (pin 16))
      (node (ref R10) (pin 1)))
    (net (code 164) (name A7)
      (node (ref U12) (pin 19))
      (node (ref R11) (pin 1))
      (node (ref U10) (pin 3)))
    (net (code 165) (name A8)
      (node (ref U10) (pin 4))
      (node (ref U13) (pin 2))
      (node (ref R12) (pin 1)))
    (net (code 166) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 8))
      (node (ref U3) (pin 11)))
    (net (code 167) (name "Net-(U3-Pad10)")
      (node (ref U3) (pin 13))
      (node (ref U3) (pin 10)))
    (net (code 168) (name "Net-(R1-Pad1)")
      (node (ref R3) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 169) (name RAM_OE)
      (node (ref U10) (pin 22))
      (node (ref U17) (pin 2)))
    (net (code 170) (name RAM_WE)
      (node (ref U16) (pin 11))
      (node (ref U10) (pin 27)))
    (net (code 171) (name A13)
      (node (ref U13) (pin 15))
      (node (ref R17) (pin 1))
      (node (ref U10) (pin 9)))))