(export (version D)
  (design
    (source "D:/owncloud/Documents/Projects/RC6502/RC6502 RIOT/RC6502 RIOT.sch")
    (date "14/02/2019 13:45:02")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 RIOT.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value 74HCT138)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS138))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C045924))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C04594C))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C04594D))
    (comp (ref J2)
      (value VDU_BASE)
      (footprint Pin_Headers:Pin_Header_Straight_2x07_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x07_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0413AA))
    (comp (ref J9)
      (value RC6502_Backplane_Extra)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane_Extra))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62AABD))
    (comp (ref JP5)
      (value T0_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C634111))
    (comp (ref JP4)
      (value T1_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6341DF))
    (comp (ref JP2)
      (value CS1_SEL)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63AB60))
    (comp (ref JP3)
      (value CS2_SEL)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63ADD6))
    (comp (ref U1)
      (value RIOT)
      (footprint Housings_DIP:DIP-40_W15.24mm_Socket)
      (libsource (lib atari_riot) (part RIOT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6443AB))
    (comp (ref R1)
      (value 3k3)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6454FA))
    (comp (ref JP1)
      (value IRQ_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64756E))
    (comp (ref JP7)
      (value IRQ_SEL)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64ECF6))
    (comp (ref J4)
      (value "RIGHT PLAYER")
      (footprint RND_DSUB:DSUB-9_Male_Vertical_Pitch2.77x2.84mm)
      (libsource (lib atari_joystick) (part Atari_Joystick))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65088B))
    (comp (ref J1)
      (value "LEFT PLAYER")
      (footprint RND_DSUB:DSUB-9_Male_Vertical_Pitch2.77x2.84mm)
      (libsource (lib atari_joystick) (part Atari_Joystick))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6508D7))
    (comp (ref J3)
      (value Analog)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C650F09))
    (comp (ref C3)
      (value 1nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C652694))
    (comp (ref JP8)
      (value B/W)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65BFA4))
    (comp (ref JP9)
      (value L_DIFF)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65C817))
    (comp (ref JP10)
      (value R_DIFF)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65CC4B))
    (comp (ref SW1)
      (value SELECT)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65D4C5))
    (comp (ref SW2)
      (value START)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65E10D))
    (comp (ref C4)
      (value 1nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65F1AC))
    (comp (ref J5)
      (value AUX)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C662E55))
    (comp (ref JP6)
      (value RAM_SEL)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C669D81))
    (comp (ref JP11)
      (value RAM_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C66BB42)))
  (libparts
    (libpart (lib 74xx) (part 74LS138)
      (description "Decoder 3 to 8 (active low outputs)")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS138))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name E1) (type input))
        (pin (num 5) (name E2) (type input))
        (pin (num 6) (name E3) (type input))
        (pin (num 7) (name O7) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name O6) (type output))
        (pin (num 10) (name O5) (type output))
        (pin (num 11) (name O4) (type output))
        (pin (num 12) (name O3) (type output))
        (pin (num 13) (name O2) (type output))
        (pin (num 14) (name O1) (type output))
        (pin (num 15) (name O0) (type output))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib atari_joystick) (part Atari_Joystick)
      (description "9-pin male D-SUB connector")
      (footprints
        (fp DB*M*))
      (fields
        (field (name Reference) J)
        (field (name Value) Atari_Joystick))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type power_in))
        (pin (num 8) (name 8) (type power_in))
        (pin (num 9) (name 9) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x03)
      (description "Generic connector, single row, 01x03")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib conn) (part Conn_01x04)
      (description "Generic connector, single row, 01x04")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib conn) (part Conn_02x07_Odd_Even)
      (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x07_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))))
    (libpart (lib device) (part Jumper_NC_Dual)
      (description "Dual Jumper, normally closed")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Dual))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib rc6502_backplane) (part RC6502_Backplane_Extra)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) RC6502_Backplane_Extra))
      (pins
        (pin (num 1) (name A15) (type BiDi))
        (pin (num 2) (name A14) (type BiDi))
        (pin (num 3) (name A13) (type BiDi))
        (pin (num 4) (name A12) (type BiDi))
        (pin (num 5) (name A11) (type BiDi))
        (pin (num 6) (name A10) (type BiDi))
        (pin (num 7) (name A9) (type BiDi))
        (pin (num 8) (name A8) (type BiDi))
        (pin (num 9) (name A7) (type BiDi))
        (pin (num 10) (name A6) (type BiDi))
        (pin (num 11) (name A5) (type BiDi))
        (pin (num 12) (name A4) (type BiDi))
        (pin (num 13) (name A3) (type BiDi))
        (pin (num 14) (name A2) (type BiDi))
        (pin (num 15) (name A1) (type BiDi))
        (pin (num 16) (name A0) (type BiDi))
        (pin (num 17) (name P17) (type power_out))
        (pin (num 18) (name P18) (type power_out))
        (pin (num 19) (name PHI2) (type BiDi))
        (pin (num 20) (name RESET) (type BiDi))
        (pin (num 21) (name PHI0) (type BiDi))
        (pin (num 22) (name IRQ) (type BiDi))
        (pin (num 23) (name EX0) (type BiDi))
        (pin (num 24) (name RW) (type BiDi))
        (pin (num 25) (name READY) (type BiDi))
        (pin (num 26) (name SYNC) (type BiDi))
        (pin (num 27) (name D0) (type BiDi))
        (pin (num 28) (name D1) (type BiDi))
        (pin (num 29) (name D2) (type BiDi))
        (pin (num 30) (name D3) (type BiDi))
        (pin (num 31) (name D4) (type BiDi))
        (pin (num 32) (name D5) (type BiDi))
        (pin (num 33) (name D6) (type BiDi))
        (pin (num 34) (name D7) (type BiDi))
        (pin (num 35) (name TX) (type BiDi))
        (pin (num 36) (name RX) (type BiDi))
        (pin (num 37) (name NMI) (type BiDi))
        (pin (num 38) (name EX1) (type BiDi))
        (pin (num 39) (name EX2) (type BiDi))))
    (libpart (lib atari_riot) (part RIOT)
      (fields
        (field (name Reference) U)
        (field (name Value) RIOT))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name A5) (type input))
        (pin (num 3) (name A4) (type input))
        (pin (num 4) (name A3) (type input))
        (pin (num 5) (name A2) (type input))
        (pin (num 6) (name A1) (type input))
        (pin (num 7) (name A0) (type input))
        (pin (num 8) (name PA0) (type BiDi))
        (pin (num 9) (name PA1) (type BiDi))
        (pin (num 10) (name PA2) (type BiDi))
        (pin (num 11) (name PA3) (type BiDi))
        (pin (num 12) (name PA4) (type BiDi))
        (pin (num 13) (name PA5) (type BiDi))
        (pin (num 14) (name PA6) (type BiDi))
        (pin (num 15) (name PA7) (type BiDi))
        (pin (num 16) (name PB7) (type BiDi))
        (pin (num 17) (name PB6) (type BiDi))
        (pin (num 18) (name PB5) (type BiDi))
        (pin (num 19) (name PB4) (type BiDi))
        (pin (num 20) (name VCC) (type power_in))
        (pin (num 21) (name PB3) (type BiDi))
        (pin (num 22) (name PB2) (type BiDi))
        (pin (num 23) (name PB1) (type BiDi))
        (pin (num 24) (name PB0) (type BiDi))
        (pin (num 25) (name ~IRQ) (type input))
        (pin (num 26) (name D7) (type input))
        (pin (num 27) (name D6) (type input))
        (pin (num 28) (name D5) (type input))
        (pin (num 29) (name D4) (type input))
        (pin (num 30) (name D3) (type input))
        (pin (num 31) (name D2) (type input))
        (pin (num 32) (name D1) (type input))
        (pin (num 33) (name D0) (type input))
        (pin (num 34) (name ~RES) (type input))
        (pin (num 35) (name R/~W) (type input))
        (pin (num 36) (name ~RS) (type input))
        (pin (num 37) (name ~CS2) (type input))
        (pin (num 38) (name CS1) (type input))
        (pin (num 39) (name PHI2) (type input))
        (pin (num 40) (name A6) (type input))))
    (libpart (lib switches) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\74xx.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical rc6502_backplane)
      (uri D:\ownCloud\Documents\Projects\RC6502\Templates\rc6502_backplane.lib))
    (library (logical atari_riot)
      (uri D:\owncloud\Documents\Projects\RC6502\Templates\atari_riot.lib))
    (library (logical atari_joystick)
      (uri D:\owncloud\Documents\Projects\RC6502\Templates\atari_joystick.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical switches)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\switches.lib")))
  (nets
    (net (code 1) (name /A11)
      (node (ref JP6) (pin 3))
      (node (ref J9) (pin 5)))
    (net (code 2) (name VCC)
      (node (ref JP11) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 20))
      (node (ref J4) (pin 7))
      (node (ref U2) (pin 16))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref J9) (pin 18))
      (node (ref JP2) (pin 3))
      (node (ref J1) (pin 7)))
    (net (code 3) (name /A9)
      (node (ref JP6) (pin 1))
      (node (ref J9) (pin 7)))
    (net (code 4) (name "Net-(JP1-Pad3)")
      (node (ref JP1) (pin 3))
      (node (ref JP7) (pin 2)))
    (net (code 5) (name /CS1)
      (node (ref JP2) (pin 2))
      (node (ref U1) (pin 38)))
    (net (code 6) (name /~CS2)
      (node (ref U1) (pin 37))
      (node (ref JP3) (pin 2)))
    (net (code 7) (name /A6)
      (node (ref J9) (pin 10))
      (node (ref U1) (pin 40)))
    (net (code 8) (name /IRQ_IN)
      (node (ref JP7) (pin 1))
      (node (ref J9) (pin 22)))
    (net (code 9) (name /NMI_IN)
      (node (ref JP7) (pin 3))
      (node (ref J9) (pin 37)))
    (net (code 10) (name /~IRQ)
      (node (ref JP1) (pin 2))
      (node (ref U1) (pin 25)))
    (net (code 11) (name /~RES)
      (node (ref U1) (pin 34))
      (node (ref J9) (pin 20)))
    (net (code 12) (name /PB4)
      (node (ref U1) (pin 19))
      (node (ref J5) (pin 2)))
    (net (code 13) (name /PB5)
      (node (ref J5) (pin 1))
      (node (ref U1) (pin 18)))
    (net (code 14) (name /PB6)
      (node (ref U1) (pin 17))
      (node (ref JP9) (pin 2)))
    (net (code 15) (name /PB7)
      (node (ref JP10) (pin 2))
      (node (ref U1) (pin 16)))
    (net (code 16) (name "Net-(JP1-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref JP1) (pin 1)))
    (net (code 17) (name /PB3)
      (node (ref JP8) (pin 2))
      (node (ref U1) (pin 21)))
    (net (code 18) (name /PA1)
      (node (ref J4) (pin 2))
      (node (ref U1) (pin 9)))
    (net (code 19) (name /PB2)
      (node (ref J5) (pin 3))
      (node (ref U1) (pin 22)))
    (net (code 20) (name /PB1)
      (node (ref U1) (pin 23))
      (node (ref SW1) (pin 1)))
    (net (code 21) (name /PB0)
      (node (ref U1) (pin 24))
      (node (ref C4) (pin 1))
      (node (ref SW2) (pin 1)))
    (net (code 22) (name /PA7)
      (node (ref J1) (pin 4))
      (node (ref U1) (pin 15)))
    (net (code 23) (name /PA6)
      (node (ref J1) (pin 3))
      (node (ref U1) (pin 14)))
    (net (code 24) (name /PA5)
      (node (ref U1) (pin 13))
      (node (ref J1) (pin 2)))
    (net (code 25) (name /PA4)
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 12)))
    (net (code 26) (name /PA3)
      (node (ref J4) (pin 4))
      (node (ref U1) (pin 11)))
    (net (code 27) (name /PA2)
      (node (ref U1) (pin 10))
      (node (ref J4) (pin 3)))
    (net (code 28) (name /PHI2)
      (node (ref J9) (pin 19))
      (node (ref U1) (pin 39)))
    (net (code 29) (name GND)
      (node (ref C2) (pin 2))
      (node (ref J9) (pin 17))
      (node (ref J4) (pin 8))
      (node (ref JP8) (pin 3))
      (node (ref U1) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref JP10) (pin 3))
      (node (ref C4) (pin 2))
      (node (ref JP9) (pin 3))
      (node (ref SW2) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 8))
      (node (ref C3) (pin 2)))
    (net (code 30) (name "Net-(JP10-Pad1)")
      (node (ref JP10) (pin 1)))
    (net (code 31) (name "Net-(JP9-Pad1)")
      (node (ref JP9) (pin 1)))
    (net (code 32) (name "Net-(JP8-Pad1)")
      (node (ref JP8) (pin 1)))
    (net (code 33) (name "Net-(JP11-Pad3)")
      (node (ref JP6) (pin 2))
      (node (ref JP11) (pin 3)))
    (net (code 34) (name /~RS)
      (node (ref U1) (pin 36))
      (node (ref JP11) (pin 2)))
    (net (code 35) (name /P2)
      (node (ref J1) (pin 5))
      (node (ref J3) (pin 3)))
    (net (code 36) (name /PA0)
      (node (ref C3) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 37) (name /P0)
      (node (ref J3) (pin 1))
      (node (ref J4) (pin 5)))
    (net (code 38) (name /P1)
      (node (ref J3) (pin 2))
      (node (ref J4) (pin 9)))
    (net (code 39) (name /P3)
      (node (ref J3) (pin 4))
      (node (ref J1) (pin 9)))
    (net (code 40) (name /T0)
      (node (ref J4) (pin 6))
      (node (ref JP5) (pin 1)))
    (net (code 41) (name /T1)
      (node (ref JP4) (pin 1))
      (node (ref J1) (pin 6)))
    (net (code 42) (name "Net-(J9-Pad6)")
      (node (ref J9) (pin 6)))
    (net (code 43) (name "Net-(J9-Pad8)")
      (node (ref J9) (pin 8)))
    (net (code 44) (name "Net-(J9-Pad21)")
      (node (ref J9) (pin 21)))
    (net (code 45) (name "Net-(J9-Pad23)")
      (node (ref J9) (pin 23)))
    (net (code 46) (name "Net-(J2-Pad13)")
      (node (ref J2) (pin 13))
      (node (ref U2) (pin 9)))
    (net (code 47) (name "Net-(J2-Pad11)")
      (node (ref J2) (pin 11))
      (node (ref U2) (pin 10)))
    (net (code 48) (name /A4)
      (node (ref J9) (pin 12))
      (node (ref U1) (pin 3)))
    (net (code 49) (name /A15)
      (node (ref U2) (pin 6))
      (node (ref J9) (pin 1)))
    (net (code 50) (name /A14)
      (node (ref J9) (pin 2))
      (node (ref U2) (pin 3)))
    (net (code 51) (name /A3)
      (node (ref U1) (pin 4))
      (node (ref J9) (pin 13)))
    (net (code 52) (name /A5)
      (node (ref U1) (pin 2))
      (node (ref J9) (pin 11)))
    (net (code 53) (name /A7)
      (node (ref J9) (pin 9))
      (node (ref JP2) (pin 1)))
    (net (code 54) (name /A13)
      (node (ref U2) (pin 2))
      (node (ref J9) (pin 3)))
    (net (code 55) (name "Net-(J9-Pad38)")
      (node (ref J9) (pin 38))
      (node (ref JP5) (pin 2)))
    (net (code 56) (name "Net-(J9-Pad36)")
      (node (ref J9) (pin 36)))
    (net (code 57) (name "Net-(J9-Pad26)")
      (node (ref J9) (pin 26)))
    (net (code 58) (name /A0)
      (node (ref U1) (pin 7))
      (node (ref J9) (pin 16)))
    (net (code 59) (name "Net-(J9-Pad35)")
      (node (ref J9) (pin 35)))
    (net (code 60) (name "Net-(J9-Pad25)")
      (node (ref J9) (pin 25)))
    (net (code 61) (name /A1)
      (node (ref U1) (pin 6))
      (node (ref J9) (pin 15)))
    (net (code 62) (name /A2)
      (node (ref J9) (pin 14))
      (node (ref U1) (pin 5)))
    (net (code 63) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 64) (name "Net-(J2-Pad9)")
      (node (ref U2) (pin 11))
      (node (ref J2) (pin 9)))
    (net (code 65) (name "Net-(J2-Pad7)")
      (node (ref U2) (pin 12))
      (node (ref J2) (pin 7)))
    (net (code 66) (name "Net-(J2-Pad5)")
      (node (ref U2) (pin 13))
      (node (ref J2) (pin 5)))
    (net (code 67) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref U2) (pin 14)))
    (net (code 68) (name "Net-(J2-Pad1)")
      (node (ref U2) (pin 15))
      (node (ref J2) (pin 1)))
    (net (code 69) (name RIOT_BASE)
      (node (ref J2) (pin 14))
      (node (ref J2) (pin 12))
      (node (ref J2) (pin 10))
      (node (ref J2) (pin 8))
      (node (ref J2) (pin 6))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 2))
      (node (ref JP3) (pin 3)))
    (net (code 70) (name "Net-(J9-Pad39)")
      (node (ref J9) (pin 39))
      (node (ref JP4) (pin 2)))
    (net (code 71) (name /A12)
      (node (ref J9) (pin 4))
      (node (ref U2) (pin 1))
      (node (ref JP3) (pin 1)))
    (net (code 72) (name /D1)
      (node (ref U1) (pin 32))
      (node (ref J9) (pin 28)))
    (net (code 73) (name /D0)
      (node (ref U1) (pin 33))
      (node (ref J9) (pin 27)))
    (net (code 74) (name /D2)
      (node (ref J9) (pin 29))
      (node (ref U1) (pin 31)))
    (net (code 75) (name /D3)
      (node (ref U1) (pin 30))
      (node (ref J9) (pin 30)))
    (net (code 76) (name /D4)
      (node (ref J9) (pin 31))
      (node (ref U1) (pin 29)))
    (net (code 77) (name /D5)
      (node (ref U1) (pin 28))
      (node (ref J9) (pin 32)))
    (net (code 78) (name /D6)
      (node (ref U1) (pin 27))
      (node (ref J9) (pin 33)))
    (net (code 79) (name /D7)
      (node (ref U1) (pin 26))
      (node (ref J9) (pin 34)))
    (net (code 80) (name /R/~W)
      (node (ref J9) (pin 24))
      (node (ref U1) (pin 35)))))