(export (version D)
  (design
    (source "D:/owncloud/Documents/Projects/RC6502/RC6502 Joystick/RC6502 Joystick.sch")
    (date "11/02/2019 15:30:15")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 Joystick.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J4)
      (value RC6502_Backplane)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C225E9D))
    (comp (ref U4)
      (value 74LS138)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS138))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C225F79))
    (comp (ref U3)
      (value 74LS138)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS138))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C225FA2))
    (comp (ref J3)
      (value Base)
      (footprint Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x08_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C226011))
    (comp (ref J2)
      (value Port)
      (footprint Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x08_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C22CCC7))
    (comp (ref U2)
      (value 74LS373)
      (footprint Housings_DIP:DIP-20_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS373))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C237A24))
    (comp (ref U1)
      (value 74LS245)
      (footprint Housings_DIP:DIP-20_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS245))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C615D1F))
    (comp (ref J1)
      (value Atari_Joystick)
      (footprint RND_DSUB:DSUB-9_Male_Vertical_Pitch2.77x2.84mm)
      (libsource (lib atari_joystick) (part Atari_Joystick))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C615D86))
    (comp (ref R1)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C616FBA))
    (comp (ref R2)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61718E))
    (comp (ref R3)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6171D2))
    (comp (ref R6)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61721D))
    (comp (ref R4)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C617267))
    (comp (ref R7)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6172B4))
    (comp (ref R5)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C617308))
    (comp (ref R9)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61BCE7))
    (comp (ref D1)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61BEFE))
    (comp (ref D2)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C307))
    (comp (ref D3)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C3BC))
    (comp (ref D4)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C3CB))
    (comp (ref D5)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C67C))
    (comp (ref D6)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C68B))
    (comp (ref D7)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C69A))
    (comp (ref D8)
      (value LED_Small)
      (footprint LEDs:LED_D5.0mm)
      (libsource (lib device) (part LED_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61C6A9))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61DA49))
    (comp (ref SW2)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61F45D))
    (comp (ref SW3)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61F6C5))
    (comp (ref SW4)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61F937))
    (comp (ref SW5)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61F9C6))
    (comp (ref SW6)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61FA58))
    (comp (ref SW7)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61FAEF))
    (comp (ref SW8)
      (value SW_Push)
      (footprint Buttons_Switches_THT:SW_PUSH_6mm_h5mm)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61FB87))
    (comp (ref R10)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62581E))
    (comp (ref R11)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6258AA))
    (comp (ref R12)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C625971))
    (comp (ref R13)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C625977))
    (comp (ref R14)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62597D))
    (comp (ref R15)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C625983))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62ACC5))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62AD75))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62AE28))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62AECE))
    (comp (ref R8)
      (value 4k7)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62D2F7))
    (comp (ref R16)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62D743)))
  (libparts
    (libpart (lib 74xx) (part 74LS138)
      (description "Decoder 3 to 8 (active low outputs)")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS138))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name E1) (type input))
        (pin (num 5) (name E2) (type input))
        (pin (num 6) (name E3) (type input))
        (pin (num 7) (name O7) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name O6) (type output))
        (pin (num 10) (name O5) (type output))
        (pin (num 11) (name O4) (type output))
        (pin (num 12) (name O3) (type output))
        (pin (num 13) (name O2) (type output))
        (pin (num 14) (name O1) (type output))
        (pin (num 15) (name O0) (type output))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS245)
      (aliases
        (alias 74HC245))
      (description "Octal BUS Transceivers, 3 State out")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS373)
      (description "8 bits Latch, 3 state Out")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS373))
      (pins
        (pin (num 1) (name OE) (type input))
        (pin (num 2) (name O0) (type 3state))
        (pin (num 3) (name D0) (type input))
        (pin (num 4) (name D1) (type input))
        (pin (num 5) (name O1) (type 3state))
        (pin (num 6) (name O2) (type 3state))
        (pin (num 7) (name D2) (type input))
        (pin (num 8) (name D3) (type input))
        (pin (num 9) (name O3) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name LE) (type input))
        (pin (num 12) (name O4) (type 3state))
        (pin (num 13) (name D4) (type input))
        (pin (num 14) (name D5) (type input))
        (pin (num 15) (name O5) (type 3state))
        (pin (num 16) (name O6) (type 3state))
        (pin (num 17) (name D6) (type input))
        (pin (num 18) (name D7) (type input))
        (pin (num 19) (name O7) (type 3state))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib atari_joystick) (part Atari_Joystick)
      (description "9-pin male D-SUB connector")
      (footprints
        (fp DB*M*))
      (fields
        (field (name Reference) J)
        (field (name Value) Atari_Joystick))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type power_out))
        (pin (num 8) (name 8) (type power_out))
        (pin (num 9) (name 9) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_02x08_Odd_Even)
      (description "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x08_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib device) (part LED_Small)
      (description "LED, small symbol")
      (footprints
        (fp LED-*)
        (fp LED_*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib rc6502_backplane) (part RC6502_Backplane)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) RC6502_Backplane))
      (pins
        (pin (num 1) (name A15) (type BiDi))
        (pin (num 2) (name A14) (type BiDi))
        (pin (num 3) (name A13) (type BiDi))
        (pin (num 4) (name A12) (type BiDi))
        (pin (num 5) (name A11) (type BiDi))
        (pin (num 6) (name A10) (type BiDi))
        (pin (num 7) (name A9) (type BiDi))
        (pin (num 8) (name A8) (type BiDi))
        (pin (num 9) (name A7) (type BiDi))
        (pin (num 10) (name A6) (type BiDi))
        (pin (num 11) (name A5) (type BiDi))
        (pin (num 12) (name A4) (type BiDi))
        (pin (num 13) (name A3) (type BiDi))
        (pin (num 14) (name A2) (type BiDi))
        (pin (num 15) (name A1) (type BiDi))
        (pin (num 16) (name A0) (type BiDi))
        (pin (num 17) (name P17) (type power_out))
        (pin (num 18) (name P18) (type power_out))
        (pin (num 19) (name PHI2) (type BiDi))
        (pin (num 20) (name RESET) (type BiDi))
        (pin (num 21) (name PHI0) (type BiDi))
        (pin (num 22) (name IRQ) (type BiDi))
        (pin (num 23) (name P23) (type NotConnected))
        (pin (num 24) (name RW) (type BiDi))
        (pin (num 25) (name READY) (type BiDi))
        (pin (num 26) (name SYNC) (type BiDi))
        (pin (num 27) (name D0) (type BiDi))
        (pin (num 28) (name D1) (type BiDi))
        (pin (num 29) (name D2) (type BiDi))
        (pin (num 30) (name D3) (type BiDi))
        (pin (num 31) (name D4) (type BiDi))
        (pin (num 32) (name D5) (type BiDi))
        (pin (num 33) (name D6) (type BiDi))
        (pin (num 34) (name D7) (type BiDi))
        (pin (num 35) (name TX) (type BiDi))
        (pin (num 36) (name RX) (type BiDi))
        (pin (num 37) (name NMI) (type BiDi))
        (pin (num 38) (name P38) (type NotConnected))
        (pin (num 39) (name P39) (type NotConnected))))
    (libpart (lib switches) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\74xx.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical switches)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\switches.lib"))
    (library (logical rc6502_backplane)
      (uri D:\ownCloud\Documents\Projects\RC6502\Templates\rc6502_backplane.lib))
    (library (logical atari_joystick)
      (uri D:\owncloud\Documents\Projects\RC6502\Templates\atari_joystick.lib)))
  (nets
    (net (code 1) (name "Net-(D8-Pad2)")
      (node (ref R16) (pin 1))
      (node (ref D8) (pin 2)))
    (net (code 2) (name "Net-(D7-Pad2)")
      (node (ref D7) (pin 2))
      (node (ref R15) (pin 1)))
    (net (code 3) (name READ)
      (node (ref J2) (pin 16))
      (node (ref J2) (pin 14))
      (node (ref U1) (pin 19))
      (node (ref J2) (pin 12))
      (node (ref J2) (pin 10)))
    (net (code 4) (name "Net-(D6-Pad2)")
      (node (ref R14) (pin 1))
      (node (ref D6) (pin 2)))
    (net (code 5) (name "Net-(D5-Pad2)")
      (node (ref R13) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 6) (name "Net-(D4-Pad2)")
      (node (ref R12) (pin 1))
      (node (ref D4) (pin 2)))
    (net (code 7) (name "Net-(D3-Pad2)")
      (node (ref R11) (pin 1))
      (node (ref D3) (pin 2)))
    (net (code 8) (name VCC)
      (node (ref SW3) (pin 2))
      (node (ref SW7) (pin 2))
      (node (ref SW6) (pin 2))
      (node (ref SW5) (pin 2))
      (node (ref SW4) (pin 2))
      (node (ref SW8) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref U3) (pin 16))
      (node (ref U4) (pin 16))
      (node (ref J4) (pin 18))
      (node (ref C4) (pin 1))
      (node (ref J1) (pin 7))
      (node (ref C3) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U2) (pin 20))
      (node (ref U1) (pin 20)))
    (net (code 9) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 10) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R9) (pin 1)))
    (net (code 11) (name WRITE)
      (node (ref J2) (pin 8))
      (node (ref J2) (pin 6))
      (node (ref U2) (pin 11))
      (node (ref J2) (pin 2))
      (node (ref J2) (pin 4)))
    (net (code 12) (name /IN_D7)
      (node (ref SW8) (pin 1))
      (node (ref U1) (pin 11))
      (node (ref R8) (pin 1)))
    (net (code 13) (name /OUT_D7)
      (node (ref R16) (pin 2))
      (node (ref U2) (pin 19)))
    (net (code 14) (name /OUT_D0_UP)
      (node (ref R9) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 15) (name /OUT_D1_DOWN)
      (node (ref R10) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 16) (name /OUT_D2_LEFT)
      (node (ref U2) (pin 6))
      (node (ref R11) (pin 2)))
    (net (code 17) (name /OUT_D3_RIGHT)
      (node (ref U2) (pin 9))
      (node (ref R12) (pin 2)))
    (net (code 18) (name /OUT_D4_FIRE0)
      (node (ref R13) (pin 2))
      (node (ref U2) (pin 12)))
    (net (code 19) (name /OUT_D5_FIRE1)
      (node (ref R14) (pin 2))
      (node (ref U2) (pin 15)))
    (net (code 20) (name /OUT_D6_FIRE2)
      (node (ref U2) (pin 16))
      (node (ref R15) (pin 2)))
    (net (code 21) (name "Net-(J3-Pad10)")
      (node (ref J3) (pin 6))
      (node (ref J3) (pin 10))
      (node (ref J3) (pin 8))
      (node (ref J3) (pin 12))
      (node (ref J3) (pin 16))
      (node (ref J3) (pin 14))
      (node (ref U3) (pin 4))
      (node (ref J3) (pin 2))
      (node (ref J3) (pin 4)))
    (net (code 22) (name "Net-(J2-Pad11)")
      (node (ref J2) (pin 11))
      (node (ref U3) (pin 10)))
    (net (code 23) (name "Net-(J2-Pad9)")
      (node (ref J2) (pin 9))
      (node (ref U3) (pin 11)))
    (net (code 24) (name "Net-(J2-Pad7)")
      (node (ref U3) (pin 12))
      (node (ref J2) (pin 7)))
    (net (code 25) (name "Net-(J2-Pad5)")
      (node (ref U3) (pin 13))
      (node (ref J2) (pin 5)))
    (net (code 26) (name "Net-(J2-Pad3)")
      (node (ref U3) (pin 14))
      (node (ref J2) (pin 3)))
    (net (code 27) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1))
      (node (ref U3) (pin 15)))
    (net (code 28) (name "Net-(J3-Pad9)")
      (node (ref U4) (pin 11))
      (node (ref J3) (pin 9)))
    (net (code 29) (name "Net-(J3-Pad13)")
      (node (ref U4) (pin 9))
      (node (ref J3) (pin 13)))
    (net (code 30) (name "Net-(J3-Pad11)")
      (node (ref U4) (pin 10))
      (node (ref J3) (pin 11)))
    (net (code 31) (name "Net-(J3-Pad15)")
      (node (ref U4) (pin 7))
      (node (ref J3) (pin 15)))
    (net (code 32) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7))
      (node (ref U4) (pin 12)))
    (net (code 33) (name "Net-(J3-Pad5)")
      (node (ref U4) (pin 13))
      (node (ref J3) (pin 5)))
    (net (code 34) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3))
      (node (ref U4) (pin 14)))
    (net (code 35) (name "Net-(J3-Pad1)")
      (node (ref U4) (pin 15))
      (node (ref J3) (pin 1)))
    (net (code 36) (name "Net-(J2-Pad13)")
      (node (ref J2) (pin 13))
      (node (ref U3) (pin 9)))
    (net (code 37) (name GND)
      (node (ref U1) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref D8) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref U3) (pin 8))
      (node (ref R6) (pin 2))
      (node (ref U4) (pin 8))
      (node (ref U4) (pin 5))
      (node (ref U4) (pin 4))
      (node (ref J4) (pin 17))
      (node (ref R4) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref U3) (pin 5))
      (node (ref R3) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 10))
      (node (ref U2) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref U2) (pin 10))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref R8) (pin 2)))
    (net (code 38) (name /IN_D5_FIRE1)
      (node (ref SW6) (pin 1))
      (node (ref J1) (pin 9))
      (node (ref R6) (pin 1))
      (node (ref U1) (pin 13)))
    (net (code 39) (name /IN_D6_FIRE2)
      (node (ref J1) (pin 5))
      (node (ref U1) (pin 12))
      (node (ref SW7) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 40) (name /IN_D3_RIGHT)
      (node (ref R5) (pin 1))
      (node (ref SW4) (pin 1))
      (node (ref J1) (pin 4))
      (node (ref U1) (pin 15)))
    (net (code 41) (name /IN_D2_LEFT)
      (node (ref J1) (pin 3))
      (node (ref U1) (pin 16))
      (node (ref R4) (pin 1))
      (node (ref SW3) (pin 1)))
    (net (code 42) (name /IN_D1_DOWN)
      (node (ref R3) (pin 1))
      (node (ref U1) (pin 17))
      (node (ref J1) (pin 2))
      (node (ref SW2) (pin 1)))
    (net (code 43) (name /IN_D4_FIRE0)
      (node (ref U1) (pin 14))
      (node (ref R2) (pin 1))
      (node (ref J1) (pin 6))
      (node (ref SW5) (pin 1)))
    (net (code 44) (name /IN_D0_UP)
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 18))
      (node (ref SW1) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 45) (name "Net-(J2-Pad15)")
      (node (ref J2) (pin 15))
      (node (ref U3) (pin 7)))
    (net (code 46) (name /A12)
      (node (ref J4) (pin 4))
      (node (ref U4) (pin 1)))
    (net (code 47) (name /A15)
      (node (ref J4) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 48) (name /A14)
      (node (ref U4) (pin 3))
      (node (ref J4) (pin 2)))
    (net (code 49) (name /A13)
      (node (ref J4) (pin 3))
      (node (ref U4) (pin 2)))
    (net (code 50) (name /A10)
      (node (ref J4) (pin 6))
      (node (ref U3) (pin 1)))
    (net (code 51) (name /A11)
      (node (ref U3) (pin 2))
      (node (ref J4) (pin 5)))
    (net (code 52) (name /Phi2)
      (node (ref J4) (pin 19))
      (node (ref U3) (pin 6)))
    (net (code 53) (name /D5)
      (node (ref J4) (pin 32))
      (node (ref U1) (pin 7))
      (node (ref U2) (pin 14)))
    (net (code 54) (name /D6)
      (node (ref J4) (pin 33))
      (node (ref U1) (pin 8))
      (node (ref U2) (pin 17)))
    (net (code 55) (name /D7)
      (node (ref U2) (pin 18))
      (node (ref J4) (pin 34))
      (node (ref U1) (pin 9)))
    (net (code 56) (name /D4)
      (node (ref U1) (pin 6))
      (node (ref U2) (pin 13))
      (node (ref J4) (pin 31)))
    (net (code 57) (name "Net-(J4-Pad25)")
      (node (ref J4) (pin 25)))
    (net (code 58) (name /R/~W)
      (node (ref U3) (pin 3))
      (node (ref J4) (pin 24)))
    (net (code 59) (name "Net-(J4-Pad35)")
      (node (ref J4) (pin 35)))
    (net (code 60) (name "Net-(J4-Pad36)")
      (node (ref J4) (pin 36)))
    (net (code 61) (name "Net-(J4-Pad37)")
      (node (ref J4) (pin 37)))
    (net (code 62) (name "Net-(J4-Pad26)")
      (node (ref J4) (pin 26)))
    (net (code 63) (name "Net-(J4-Pad22)")
      (node (ref J4) (pin 22)))
    (net (code 64) (name "Net-(J4-Pad20)")
      (node (ref J4) (pin 20)))
    (net (code 65) (name /D0)
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 2))
      (node (ref J4) (pin 27)))
    (net (code 66) (name /D1)
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 4))
      (node (ref J4) (pin 28)))
    (net (code 67) (name /D2)
      (node (ref U2) (pin 7))
      (node (ref U1) (pin 4))
      (node (ref J4) (pin 29)))
    (net (code 68) (name /D3)
      (node (ref J4) (pin 30))
      (node (ref U1) (pin 5))
      (node (ref U2) (pin 8)))
    (net (code 69) (name "Net-(J4-Pad13)")
      (node (ref J4) (pin 13)))
    (net (code 70) (name "Net-(J4-Pad23)")
      (node (ref J4) (pin 23)))
    (net (code 71) (name "Net-(J4-Pad14)")
      (node (ref J4) (pin 14)))
    (net (code 72) (name "Net-(J4-Pad15)")
      (node (ref J4) (pin 15)))
    (net (code 73) (name "Net-(J4-Pad16)")
      (node (ref J4) (pin 16)))
    (net (code 74) (name "Net-(J4-Pad10)")
      (node (ref J4) (pin 10)))
    (net (code 75) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7)))
    (net (code 76) (name "Net-(J4-Pad8)")
      (node (ref J4) (pin 8)))
    (net (code 77) (name "Net-(J4-Pad9)")
      (node (ref J4) (pin 9)))
    (net (code 78) (name "Net-(J4-Pad38)")
      (node (ref J4) (pin 38)))
    (net (code 79) (name "Net-(J4-Pad11)")
      (node (ref J4) (pin 11)))
    (net (code 80) (name "Net-(J4-Pad21)")
      (node (ref J4) (pin 21)))
    (net (code 81) (name "Net-(J4-Pad12)")
      (node (ref J4) (pin 12)))
    (net (code 82) (name "Net-(J4-Pad39)")
      (node (ref J4) (pin 39)))))