(export (version D)
  (design
    (source "D:/ownCloud/Documents/Projects/RC6502/RC6502 CPU/RC6502 CPU.sch")
    (date "14/06/2017 15:22:08")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 CPU.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R1)
      (value 3.3k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590BA496))
    (comp (ref R2)
      (value 3.3k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590BA57A))
    (comp (ref R3)
      (value 3.3k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590BA5A2))
    (comp (ref J1)
      (value CONN_01X39)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X39))
      (sheetpath (names /) (tstamps /))
      (tstamp 590BAB0E))
    (comp (ref U1)
      (value WD65C02)
      (footprint Housings_DIP:DIP-40_W15.24mm_Socket)
      (libsource (lib 65xx) (part WD65C02))
      (sheetpath (names /) (tstamps /))
      (tstamp 590BAEA4))
    (comp (ref J2)
      (value "IRQ OnBus")
      (footprint Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D2BF8))
    (comp (ref J3)
      (value "NMI OnBus")
      (footprint Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D2C70))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 590DA9CE))
    (comp (ref X1)
      (value CXO_DIP14)
      (footprint Oscillators:Oscillator_DIP-14)
      (libsource (lib Oscillators) (part CXO_DIP14))
      (sheetpath (names /) (tstamps /))
      (tstamp 5918B14F))
    (comp (ref JP1)
      (value "XTAL Power")
      (footprint Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5918C6D4))
    (comp (ref JP2)
      (value "XTAL Enable")
      (footprint Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5918CD82))
    (comp (ref J4)
      (value "VP GND")
      (footprint Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 59304984)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X39)
      (description "Connector, single row, 01x39, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X39))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))))
    (libpart (lib Oscillators) (part CXO_DIP14)
      (aliases
        (alias TFT680)
        (alias GTXO-14T))
      (description "Crystal Clock Oscillator, DIP14-style metal package")
      (docs http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf)
      (footprints
        (fp Oscillator*DIP*14*))
      (fields
        (field (name Reference) X)
        (field (name Value) CXO_DIP14)
        (field (name Footprint) Oscillators:Oscillator_DIP-14))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT) (type output))
        (pin (num 14) (name Vcc) (type power_in))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib 65xx) (part WD65C02)
      (fields
        (field (name Reference) U)
        (field (name Value) WD65C02))
      (pins
        (pin (num 1) (name ~VP) (type output))
        (pin (num 2) (name RDY) (type BiDi))
        (pin (num 3) (name PHI1out) (type output))
        (pin (num 4) (name ~IRQ) (type input))
        (pin (num 5) (name ~ML) (type output))
        (pin (num 6) (name ~NMI) (type input))
        (pin (num 7) (name SYNC) (type output))
        (pin (num 8) (name VCC) (type power_in))
        (pin (num 9) (name A0) (type output))
        (pin (num 10) (name A1) (type output))
        (pin (num 11) (name A2) (type output))
        (pin (num 12) (name A3) (type output))
        (pin (num 13) (name A4) (type output))
        (pin (num 14) (name A5) (type output))
        (pin (num 15) (name A6) (type output))
        (pin (num 16) (name A7) (type output))
        (pin (num 17) (name A8) (type output))
        (pin (num 18) (name A9) (type output))
        (pin (num 19) (name A10) (type output))
        (pin (num 20) (name A11) (type output))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name A12) (type output))
        (pin (num 23) (name A13) (type output))
        (pin (num 24) (name A14) (type output))
        (pin (num 25) (name A15) (type output))
        (pin (num 26) (name D7) (type 3state))
        (pin (num 27) (name D6) (type 3state))
        (pin (num 28) (name D5) (type 3state))
        (pin (num 29) (name D4) (type 3state))
        (pin (num 30) (name D3) (type 3state))
        (pin (num 31) (name D2) (type 3state))
        (pin (num 32) (name D1) (type 3state))
        (pin (num 33) (name D0) (type 3state))
        (pin (num 34) (name R/~W) (type output))
        (pin (num 35) (name NC) (type NotConnected))
        (pin (num 36) (name BE) (type input))
        (pin (num 37) (name PHI2) (type input))
        (pin (num 38) (name ~SO) (type output))
        (pin (num 39) (name PHI2out) (type output))
        (pin (num 40) (name ~RESET) (type input)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical Oscillators)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\Oscillators.lib"))
    (library (logical 65xx)
      (uri "D:\\ownCloud\\Documents\\Projects\\RC6502\\RC6502 CPU\\65xx.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 2) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36)))
    (net (code 3) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 4) (name GND)
      (node (ref C1) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref U1) (pin 21))
      (node (ref J1) (pin 17))
      (node (ref X1) (pin 7)))
    (net (code 5) (name NMI)
      (node (ref J1) (pin 37))
      (node (ref J3) (pin 1)))
    (net (code 6) (name "Net-(X1-Pad1)")
      (node (ref X1) (pin 1)))
    (net (code 7) (name "Net-(JP1-Pad2)")
      (node (ref X1) (pin 14))
      (node (ref JP1) (pin 2)))
    (net (code 8) (name "Net-(JP2-Pad2)")
      (node (ref JP2) (pin 2))
      (node (ref X1) (pin 8)))
    (net (code 9) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 10) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 11) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 12) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 13) (name "Net-(J1-Pad36)")
      (node (ref J1) (pin 36)))
    (net (code 14) (name "Net-(J1-Pad38)")
      (node (ref J1) (pin 38)))
    (net (code 15) (name "Net-(J1-Pad39)")
      (node (ref J1) (pin 39)))
    (net (code 16) (name VCC)
      (node (ref R1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 38))
      (node (ref J1) (pin 18))
      (node (ref U1) (pin 8))
      (node (ref R2) (pin 2))
      (node (ref JP1) (pin 1)))
    (net (code 17) (name IRQ)
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 22)))
    (net (code 18) (name A3)
      (node (ref J1) (pin 13))
      (node (ref U1) (pin 12)))
    (net (code 19) (name A2)
      (node (ref J1) (pin 14))
      (node (ref U1) (pin 11)))
    (net (code 20) (name RW)
      (node (ref J1) (pin 24))
      (node (ref U1) (pin 34)))
    (net (code 21) (name A1)
      (node (ref U1) (pin 10))
      (node (ref J1) (pin 15)))
    (net (code 22) (name RDY)
      (node (ref J1) (pin 25))
      (node (ref U1) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 23) (name A0)
      (node (ref U1) (pin 9))
      (node (ref J1) (pin 16)))
    (net (code 24) (name SYNC)
      (node (ref U1) (pin 7))
      (node (ref J1) (pin 26)))
    (net (code 25) (name A4)
      (node (ref U1) (pin 13))
      (node (ref J1) (pin 12)))
    (net (code 26) (name D0)
      (node (ref J1) (pin 27))
      (node (ref U1) (pin 33)))
    (net (code 27) (name D1)
      (node (ref U1) (pin 32))
      (node (ref J1) (pin 28)))
    (net (code 28) (name PHI2)
      (node (ref U1) (pin 39))
      (node (ref J1) (pin 19)))
    (net (code 29) (name D2)
      (node (ref U1) (pin 31))
      (node (ref J1) (pin 29)))
    (net (code 30) (name "Net-(J3-Pad2)")
      (node (ref R3) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 31) (name "Net-(J2-Pad1)")
      (node (ref U1) (pin 4))
      (node (ref J2) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 32) (name A10)
      (node (ref U1) (pin 19))
      (node (ref J1) (pin 6)))
    (net (code 33) (name A9)
      (node (ref J1) (pin 7))
      (node (ref U1) (pin 18)))
    (net (code 34) (name A8)
      (node (ref J1) (pin 8))
      (node (ref U1) (pin 17)))
    (net (code 35) (name A7)
      (node (ref U1) (pin 16))
      (node (ref J1) (pin 9)))
    (net (code 36) (name A6)
      (node (ref U1) (pin 15))
      (node (ref J1) (pin 10)))
    (net (code 37) (name D3)
      (node (ref J1) (pin 30))
      (node (ref U1) (pin 30)))
    (net (code 38) (name A5)
      (node (ref U1) (pin 14))
      (node (ref J1) (pin 11)))
    (net (code 39) (name D4)
      (node (ref U1) (pin 29))
      (node (ref J1) (pin 31)))
    (net (code 40) (name D6)
      (node (ref J1) (pin 33))
      (node (ref U1) (pin 27)))
    (net (code 41) (name CLOCK)
      (node (ref JP2) (pin 1))
      (node (ref J1) (pin 21))
      (node (ref U1) (pin 37)))
    (net (code 42) (name D5)
      (node (ref J1) (pin 32))
      (node (ref U1) (pin 28)))
    (net (code 43) (name A12)
      (node (ref U1) (pin 22))
      (node (ref J1) (pin 4)))
    (net (code 44) (name A11)
      (node (ref J1) (pin 5))
      (node (ref U1) (pin 20)))
    (net (code 45) (name RESET)
      (node (ref J1) (pin 20))
      (node (ref U1) (pin 40)))
    (net (code 46) (name A13)
      (node (ref U1) (pin 23))
      (node (ref J1) (pin 3)))
    (net (code 47) (name A14)
      (node (ref U1) (pin 24))
      (node (ref J1) (pin 2)))
    (net (code 48) (name A15)
      (node (ref U1) (pin 25))
      (node (ref J1) (pin 1)))
    (net (code 49) (name D7)
      (node (ref J1) (pin 34))
      (node (ref U1) (pin 26)))))