(export (version D)
  (design
    (source "D:\\owncloud\\Documents\\Projects\\RC6502\\RC6502 TIA NTSC\\RC6502 TIA NTSC.sch")
    (date "13/02/2019 20:16:04")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 TIA NTSC.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value 74HCT138)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib 74xx) (part 74LS138))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C045924))
    (comp (ref X1)
      (value "3.579545 MHz")
      (footprint Oscillator:Oscillator_DIP-14)
      (libsource (lib oscillator) (part Oscillator))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C04593A))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C04594C))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C04594D))
    (comp (ref J2)
      (value VDU_BASE)
      (footprint Pin_Headers:Pin_Header_Straight_2x07_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x07_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0413AA))
    (comp (ref J8)
      (value Composite)
      (footprint RCA:rca_yellow)
      (libsource (lib rca_plug) (part RCA_PLUG))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0DE558))
    (comp (ref U3)
      (value VDU_Port)
      (footprint vdu_amplifier:Amplifier)
      (libsource (lib vdu_port) (part VDU_Port))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C12C79F))
    (comp (ref J1)
      (value Audio)
      (footprint RCA:rca_yellow)
      (libsource (lib rca_plug) (part RCA_PLUG))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C623180))
    (comp (ref U1)
      (value TIA_NTSC)
      (footprint Housings_DIP:DIP-40_W15.24mm_Socket)
      (libsource (lib atari_tia) (part TIA_NTSC))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C627812))
    (comp (ref J9)
      (value RC6502_Backplane_Extra)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane_Extra))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62AABD))
    (comp (ref JP5)
      (value T0_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C634111))
    (comp (ref JP4)
      (value T1_EN)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6341DF))
    (comp (ref JP2)
      (value CS0_SEL)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63AB60))
    (comp (ref JP3)
      (value CS3_SEL)
      (footprint Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Dual))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63ADD6))
    (comp (ref R12)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64140A))
    (comp (ref R14)
      (value 9k1)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64155C))
    (comp (ref C12)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6421D7))
    (comp (ref C11)
      (value 820pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C642603))
    (comp (ref R13)
      (value 18k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6434FB))
    (comp (ref R17)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64C923))
    (comp (ref R15)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64CB26))
    (comp (ref C9)
      (value 470pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C64CEE0))
    (comp (ref R18)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C651556))
    (comp (ref R16)
      (value 220)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65155C))
    (comp (ref C10)
      (value 470pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C651562))
    (comp (ref R1)
      (value 27k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C657F65))
    (comp (ref R2)
      (value 3K3)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C658200))
    (comp (ref R3)
      (value 56k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65A77B))
    (comp (ref R4)
      (value 3K3)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65A781))
    (comp (ref R5)
      (value 27K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65BB40))
    (comp (ref R6)
      (value 3K3)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65BB46))
    (comp (ref R7)
      (value 110k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65CC09))
    (comp (ref R8)
      (value 3K3)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65CC0F))
    (comp (ref C8)
      (value 47pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65DBC9))
    (comp (ref R11)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65E4DC))
    (comp (ref R9)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65F2FE))
    (comp (ref R10)
      (value 6k8)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C65FC86))
    (comp (ref C7)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6606E8))
    (comp (ref J3)
      (value Analog)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C66D220))
    (comp (ref RV1)
      (value 500k)
      (footprint Potentiometers:Potentiometer_Trimmer_Bourns_3296W)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C67AAE3))
    (comp (ref JP1)
      (value CADJ)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C682A3C))
    (comp (ref C3)
      (value 68nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C688EFB))
    (comp (ref C4)
      (value 68nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6899DB))
    (comp (ref C5)
      (value 68nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68A08D))
    (comp (ref C6)
      (value 68nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68A13E)))
  (libparts
    (libpart (lib 74xx) (part 74LS138)
      (description "Decoder 3 to 8 (active low outputs)")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS138))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name E1) (type input))
        (pin (num 5) (name E2) (type input))
        (pin (num 6) (name E3) (type input))
        (pin (num 7) (name O7) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name O6) (type output))
        (pin (num 10) (name O5) (type output))
        (pin (num 11) (name O4) (type output))
        (pin (num 12) (name O3) (type output))
        (pin (num 13) (name O2) (type output))
        (pin (num 14) (name O1) (type output))
        (pin (num 15) (name O0) (type output))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x04)
      (description "Generic connector, single row, 01x04")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib conn) (part Conn_02x07_Odd_Even)
      (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x07_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))))
    (libpart (lib device) (part Jumper_NC_Dual)
      (description "Dual Jumper, normally closed")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Dual))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part Jumper_NC_Small)
      (description "Jumper, normally closed")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib oscillator) (part Oscillator)
      (footprints
        (fp Oscillator*DIP*14*))
      (fields
        (field (name Reference) X)
        (field (name Value) Oscillator)
        (field (name Footprint) Oscillators:Oscillator_DIP-14))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT) (type output))
        (pin (num 14) (name Vcc) (type power_in))))
    (libpart (lib device) (part POT)
      (description Potentiometer)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib rc6502_backplane) (part RC6502_Backplane_Extra)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) RC6502_Backplane_Extra))
      (pins
        (pin (num 1) (name A15) (type BiDi))
        (pin (num 2) (name A14) (type BiDi))
        (pin (num 3) (name A13) (type BiDi))
        (pin (num 4) (name A12) (type BiDi))
        (pin (num 5) (name A11) (type BiDi))
        (pin (num 6) (name A10) (type BiDi))
        (pin (num 7) (name A9) (type BiDi))
        (pin (num 8) (name A8) (type BiDi))
        (pin (num 9) (name A7) (type BiDi))
        (pin (num 10) (name A6) (type BiDi))
        (pin (num 11) (name A5) (type BiDi))
        (pin (num 12) (name A4) (type BiDi))
        (pin (num 13) (name A3) (type BiDi))
        (pin (num 14) (name A2) (type BiDi))
        (pin (num 15) (name A1) (type BiDi))
        (pin (num 16) (name A0) (type BiDi))
        (pin (num 17) (name P17) (type power_out))
        (pin (num 18) (name P18) (type power_out))
        (pin (num 19) (name PHI2) (type BiDi))
        (pin (num 20) (name RESET) (type BiDi))
        (pin (num 21) (name PHI0) (type BiDi))
        (pin (num 22) (name IRQ) (type BiDi))
        (pin (num 23) (name EX0) (type BiDi))
        (pin (num 24) (name RW) (type BiDi))
        (pin (num 25) (name READY) (type BiDi))
        (pin (num 26) (name SYNC) (type BiDi))
        (pin (num 27) (name D0) (type BiDi))
        (pin (num 28) (name D1) (type BiDi))
        (pin (num 29) (name D2) (type BiDi))
        (pin (num 30) (name D3) (type BiDi))
        (pin (num 31) (name D4) (type BiDi))
        (pin (num 32) (name D5) (type BiDi))
        (pin (num 33) (name D6) (type BiDi))
        (pin (num 34) (name D7) (type BiDi))
        (pin (num 35) (name TX) (type BiDi))
        (pin (num 36) (name RX) (type BiDi))
        (pin (num 37) (name NMI) (type BiDi))
        (pin (num 38) (name EX1) (type BiDi))
        (pin (num 39) (name EX2) (type BiDi))))
    (libpart (lib rca_plug) (part RCA_PLUG)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) RCA_PLUG))
      (pins
        (pin (num 1) (name Ext) (type passive))
        (pin (num 2) (name In) (type passive))))
    (libpart (lib atari_tia) (part TIA_NTSC)
      (fields
        (field (name Reference) U)
        (field (name Value) TIA_NTSC))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name CSYNC) (type 3state))
        (pin (num 3) (name RDY) (type 3state))
        (pin (num 4) (name Phi0) (type output))
        (pin (num 5) (name LUM1) (type output))
        (pin (num 6) (name ~BLK) (type input))
        (pin (num 7) (name LUM2) (type output))
        (pin (num 8) (name LUM0) (type output))
        (pin (num 9) (name COLOR) (type 3state))
        (pin (num 10) (name CADJ) (type input))
        (pin (num 11) (name OSC) (type input))
        (pin (num 12) (name AUD1) (type passive))
        (pin (num 13) (name AUD0) (type passive))
        (pin (num 14) (name D0) (type input))
        (pin (num 15) (name D1) (type input))
        (pin (num 16) (name D2) (type input))
        (pin (num 17) (name D3) (type input))
        (pin (num 18) (name D4) (type input))
        (pin (num 19) (name D5) (type input))
        (pin (num 20) (name VCC) (type power_in))
        (pin (num 21) (name ~CS3) (type input))
        (pin (num 22) (name ~CS2) (type input))
        (pin (num 23) (name CS1) (type input))
        (pin (num 24) (name ~CS0) (type input))
        (pin (num 25) (name R/~W) (type 3state))
        (pin (num 26) (name Phi2) (type input))
        (pin (num 27) (name A5) (type input))
        (pin (num 28) (name A4) (type input))
        (pin (num 29) (name A3) (type input))
        (pin (num 30) (name A2) (type input))
        (pin (num 31) (name A1) (type input))
        (pin (num 32) (name A0) (type input))
        (pin (num 33) (name D6) (type input))
        (pin (num 34) (name D7) (type input))
        (pin (num 35) (name T1) (type output))
        (pin (num 36) (name T0) (type output))
        (pin (num 37) (name P3) (type output))
        (pin (num 38) (name P2) (type input))
        (pin (num 39) (name P1) (type 3state))
        (pin (num 40) (name P0) (type 3state))))
    (libpart (lib vdu_port) (part VDU_Port)
      (fields
        (field (name Reference) U)
        (field (name Value) VDU_Port))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name VID_IN) (type input))
        (pin (num 3) (name VID_OUT) (type power_out))
        (pin (num 4) (name AUD_IN) (type power_out))
        (pin (num 5) (name AUD_OUT) (type power_out))
        (pin (num 6) (name GND) (type power_in)))))
  (libraries
    (library (logical rc6502_backplane)
      (uri D:\ownCloud\Documents\Projects\RC6502\Templates\rc6502_backplane.lib))
    (library (logical atari_tia)
      (uri D:\owncloud\Documents\Projects\RC6502\Templates\atari_tia.lib))
    (library (logical vdu_port)
      (uri "D:\\owncloud\\Documents\\Projects\\RC6502\\RC6502 TIA NTSC\\vdu_port.lib"))
    (library (logical oscillator)
      (uri D:\ownCloud\Documents\Projects\RC6502\Templates\oscillator.lib))
    (library (logical rca_plug)
      (uri D:\ownCloud\Documents\Projects\RC6502\Templates\rca_plug.lib))
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\74xx.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name GND)
      (node (ref C6) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref JP3) (pin 3))
      (node (ref C5) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref RV1) (pin 3))
      (node (ref X1) (pin 7))
      (node (ref U1) (pin 1))
      (node (ref R14) (pin 2))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 4))
      (node (ref C4) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref U3) (pin 6))
      (node (ref J1) (pin 1))
      (node (ref J9) (pin 17))
      (node (ref U1) (pin 22))
      (node (ref J8) (pin 1)))
    (net (code 2) (name VCC)
      (node (ref J9) (pin 18))
      (node (ref R8) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref U1) (pin 23))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 20))
      (node (ref R12) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref X1) (pin 14))
      (node (ref R11) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref RV1) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref U2) (pin 16))
      (node (ref R18) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 3) (name /T1_IN)
      (node (ref JP4) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref C10) (pin 1)))
    (net (code 4) (name "Net-(J9-Pad39)")
      (node (ref JP4) (pin 2))
      (node (ref J9) (pin 39)))
    (net (code 5) (name /T0_IN)
      (node (ref C9) (pin 1))
      (node (ref R15) (pin 2))
      (node (ref JP5) (pin 1)))
    (net (code 6) (name /LUM0)
      (node (ref R7) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 7) (name /CSYNC)
      (node (ref U1) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 8) (name /RDY)
      (node (ref J9) (pin 25))
      (node (ref U1) (pin 3)))
    (net (code 9) (name /LUM1)
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 10) (name /LUM2)
      (node (ref R6) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref R5) (pin 1)))
    (net (code 11) (name /COLOR)
      (node (ref C8) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref R11) (pin 1)))
    (net (code 12) (name /~CS0)
      (node (ref JP2) (pin 2))
      (node (ref U1) (pin 24)))
    (net (code 13) (name /A7)
      (node (ref J9) (pin 9))
      (node (ref JP3) (pin 1)))
    (net (code 14) (name /A12)
      (node (ref U2) (pin 1))
      (node (ref J9) (pin 4))
      (node (ref JP2) (pin 1)))
    (net (code 15) (name /~CS3)
      (node (ref JP3) (pin 2))
      (node (ref U1) (pin 21)))
    (net (code 16) (name TIA_BASE)
      (node (ref J2) (pin 12))
      (node (ref J2) (pin 8))
      (node (ref J2) (pin 14))
      (node (ref J2) (pin 10))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 2))
      (node (ref J2) (pin 6))
      (node (ref JP2) (pin 3)))
    (net (code 17) (name /AUD0)
      (node (ref U1) (pin 12))
      (node (ref U1) (pin 13))
      (node (ref R12) (pin 1))
      (node (ref C12) (pin 1)))
    (net (code 18) (name "Net-(C12-Pad2)")
      (node (ref C12) (pin 2))
      (node (ref R13) (pin 2)))
    (net (code 19) (name AUDIO)
      (node (ref C11) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 20) (name /CADJ)
      (node (ref U1) (pin 10))
      (node (ref JP1) (pin 2)))
    (net (code 21) (name "Net-(JP1-Pad1)")
      (node (ref RV1) (pin 2))
      (node (ref JP1) (pin 1)))
    (net (code 22) (name /A15)
      (node (ref U2) (pin 6))
      (node (ref J9) (pin 1)))
    (net (code 23) (name /A13)
      (node (ref U2) (pin 2))
      (node (ref J9) (pin 3)))
    (net (code 24) (name /A14)
      (node (ref U2) (pin 3))
      (node (ref J9) (pin 2)))
    (net (code 25) (name /T0)
      (node (ref U1) (pin 36))
      (node (ref R15) (pin 1))
      (node (ref R17) (pin 2)))
    (net (code 26) (name /T1)
      (node (ref R16) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref U1) (pin 35)))
    (net (code 27) (name "Net-(J9-Pad5)")
      (node (ref J9) (pin 5)))
    (net (code 28) (name "Net-(J9-Pad6)")
      (node (ref J9) (pin 6)))
    (net (code 29) (name "Net-(J9-Pad7)")
      (node (ref J9) (pin 7)))
    (net (code 30) (name "Net-(J9-Pad8)")
      (node (ref J9) (pin 8)))
    (net (code 31) (name "Net-(J9-Pad10)")
      (node (ref J9) (pin 10)))
    (net (code 32) (name "Net-(C8-Pad2)")
      (node (ref R9) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 33) (name /P0)
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 40))
      (node (ref C3) (pin 2)))
    (net (code 34) (name /P1)
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 39))
      (node (ref J3) (pin 2)))
    (net (code 35) (name /P2)
      (node (ref J3) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref U1) (pin 38)))
    (net (code 36) (name /P3)
      (node (ref C6) (pin 2))
      (node (ref U1) (pin 37))
      (node (ref J3) (pin 4)))
    (net (code 37) (name "Net-(C7-Pad1)")
      (node (ref R10) (pin 2))
      (node (ref C7) (pin 1)))
    (net (code 38) (name VIDEO)
      (node (ref R5) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 39) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 40) (name "Net-(J8-Pad2)")
      (node (ref U3) (pin 3))
      (node (ref J8) (pin 2)))
    (net (code 41) (name "Net-(J2-Pad11)")
      (node (ref J2) (pin 11))
      (node (ref U2) (pin 10)))
    (net (code 42) (name "Net-(J2-Pad13)")
      (node (ref J2) (pin 13))
      (node (ref U2) (pin 9)))
    (net (code 43) (name "Net-(J9-Pad20)")
      (node (ref J9) (pin 20)))
    (net (code 44) (name "Net-(J1-Pad2)")
      (node (ref U3) (pin 5))
      (node (ref J1) (pin 2)))
    (net (code 45) (name "Net-(X1-Pad1)")
      (node (ref X1) (pin 1)))
    (net (code 46) (name "Net-(J9-Pad35)")
      (node (ref J9) (pin 35)))
    (net (code 47) (name "Net-(J9-Pad36)")
      (node (ref J9) (pin 36)))
    (net (code 48) (name "Net-(J9-Pad37)")
      (node (ref J9) (pin 37)))
    (net (code 49) (name "Net-(J9-Pad22)")
      (node (ref J9) (pin 22)))
    (net (code 50) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 51) (name "Net-(J9-Pad23)")
      (node (ref J9) (pin 23)))
    (net (code 52) (name "Net-(J2-Pad9)")
      (node (ref U2) (pin 11))
      (node (ref J2) (pin 9)))
    (net (code 53) (name "Net-(J2-Pad7)")
      (node (ref J2) (pin 7))
      (node (ref U2) (pin 12)))
    (net (code 54) (name "Net-(J2-Pad5)")
      (node (ref U2) (pin 13))
      (node (ref J2) (pin 5)))
    (net (code 55) (name "Net-(J2-Pad3)")
      (node (ref U2) (pin 14))
      (node (ref J2) (pin 3)))
    (net (code 56) (name "Net-(J2-Pad1)")
      (node (ref U2) (pin 15))
      (node (ref J2) (pin 1)))
    (net (code 57) (name /D6)
      (node (ref J9) (pin 33))
      (node (ref U1) (pin 33)))
    (net (code 58) (name /D7)
      (node (ref J9) (pin 34))
      (node (ref U1) (pin 34)))
    (net (code 59) (name /D5)
      (node (ref U1) (pin 19))
      (node (ref J9) (pin 32)))
    (net (code 60) (name /D0)
      (node (ref U1) (pin 14))
      (node (ref J9) (pin 27)))
    (net (code 61) (name /D1)
      (node (ref J9) (pin 28))
      (node (ref U1) (pin 15)))
    (net (code 62) (name /D2)
      (node (ref J9) (pin 29))
      (node (ref U1) (pin 16)))
    (net (code 63) (name /D3)
      (node (ref J9) (pin 30))
      (node (ref U1) (pin 17)))
    (net (code 64) (name /D4)
      (node (ref U1) (pin 18))
      (node (ref J9) (pin 31)))
    (net (code 65) (name /A4)
      (node (ref U1) (pin 28))
      (node (ref J9) (pin 12)))
    (net (code 66) (name /A5)
      (node (ref U1) (pin 27))
      (node (ref J9) (pin 11)))
    (net (code 67) (name /OSC_IN)
      (node (ref X1) (pin 8))
      (node (ref U1) (pin 11)))
    (net (code 68) (name "Net-(J9-Pad38)")
      (node (ref J9) (pin 38))
      (node (ref JP5) (pin 2)))
    (net (code 69) (name /R/~W)
      (node (ref J9) (pin 24))
      (node (ref U1) (pin 25)))
    (net (code 70) (name "Net-(J9-Pad26)")
      (node (ref J9) (pin 26)))
    (net (code 71) (name /PHI2)
      (node (ref J9) (pin 19))
      (node (ref U1) (pin 26)))
    (net (code 72) (name /A3)
      (node (ref J9) (pin 13))
      (node (ref U1) (pin 29)))
    (net (code 73) (name /PHI0)
      (node (ref J9) (pin 21))
      (node (ref U1) (pin 4)))
    (net (code 74) (name /A0)
      (node (ref J9) (pin 16))
      (node (ref U1) (pin 32)))
    (net (code 75) (name /A1)
      (node (ref U1) (pin 31))
      (node (ref J9) (pin 15)))
    (net (code 76) (name /A2)
      (node (ref U1) (pin 30))
      (node (ref J9) (pin 14)))))