(export (version D)
  (design
    (source "D:/ownCloud/Documents/Projects/RC6502/RC6502 Video Adapter/RC6502 Video Adapter.sch")
    (date "11/06/2017 19:52:05")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 Video Adapter.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value CONN_01X39)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X39))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938011B))
    (comp (ref J2)
      (value "Peripheral Bus")
      (footprint Connectors:IDC_Header_Straight_40pins)
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 59380E36))
    (comp (ref U1)
      (value ATMEGA328P-PU)
      (footprint Housings_DIP:DIP-28_W7.62mm_Socket)
      (libsource (lib atmel) (part ATMEGA328P-PU))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939AF11))
    (comp (ref Y1)
      (value "16 Mhz")
      (footprint Crystals:Crystal_HC49-4H_Vertical)
      (libsource (lib device) (part Crystal))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939BD6D))
    (comp (ref C4)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939BE54))
    (comp (ref C3)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939BEA4))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939E123))
    (comp (ref J4)
      (value FTDI)
      (footprint Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 593AA693))
    (comp (ref R4)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593AAA90))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 593AC0A1))
    (comp (ref J5)
      (value ICSP)
      (footprint Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 593B2B97))
    (comp (ref JP1)
      (value PullDown)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 593C2A0A))
    (comp (ref R1)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593C2BF9))
    (comp (ref R2)
      (value 330)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593C2C43))
    (comp (ref D1)
      (value 1N4848)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 593C3A9B))
    (comp (ref D2)
      (value 1N4848)
      (footprint Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 593C3C52))
    (comp (ref R3)
      (value 75)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593C6F39))
    (comp (ref JP2)
      (value Power)
      (footprint Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 593CEF5C))
    (comp (ref J3)
      (value Video)
      (footprint rca:rca_yellow)
      (libsource (lib rca) (part RCA_PLUG))
      (sheetpath (names /) (tstamps /))
      (tstamp 593A2D19))
    (comp (ref U2)
      (value MCP23S17)
      (footprint Housings_DIP:DIP-28_W7.62mm_Socket)
      (libsource (lib microchip) (part MCP23S17))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3FAB))
    (comp (ref U3)
      (value MCP23S17)
      (footprint Housings_DIP:DIP-28_W7.62mm_Socket)
      (libsource (lib microchip) (part MCP23S17))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D4204))
    (comp (ref J6)
      (value "General Video Connector")
      (footprint Connectors:IDC_Header_Straight_40pins)
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D5AF3))
    (comp (ref R5)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593F4AC9))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 594097F8))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 59409B10)))
  (libparts
    (libpart (lib atmel) (part ATMEGA168A-PU)
      (aliases
        (alias ATMEGA48A-PU)
        (alias ATMEGA48PA-PU)
        (alias ATMEGA88A-PU)
        (alias ATMEGA88PA-PU)
        (alias ATMEGA168PA-PU)
        (alias ATMEGA328-PU)
        (alias ATMEGA328P-PU))
      (description "PDIP28 Narrow, 16k Flash, 1kB SRAM, 512B EEPROM")
      (docs http://www.atmel.com/images/atmel-8271-8-bit-avr-microcontroller-atmega48a-48pa-88a-88pa-168a-168pa-328-328p_datasheet.pdf)
      (footprints
        (fp 28DIP-ELL600)
        (fp 28dip600))
      (fields
        (field (name Reference) U)
        (field (name Value) ATMEGA168A-PU)
        (field (name Footprint) DIL28))
      (pins
        (pin (num 1) (name "(PCINT14/~RESET~)PC6") (type BiDi))
        (pin (num 2) (name "(PCINT16/RXD)PD0") (type BiDi))
        (pin (num 3) (name "(PCINT17/TXD)PD1") (type BiDi))
        (pin (num 4) (name "(PCINT18/INT0)PD2") (type BiDi))
        (pin (num 5) (name "(PCINT19/OC2B/INT1)PD3") (type BiDi))
        (pin (num 6) (name "(PCINT20/XCK/T0)PD4") (type BiDi))
        (pin (num 7) (name VCC) (type power_in))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name "(PCINT6/XTAL1/TOSC1)PB6") (type BiDi))
        (pin (num 10) (name "(PCINT7/XTAL2/TOSC2)PB7") (type BiDi))
        (pin (num 11) (name "(PCINT21/OC0B/T1)PD5") (type BiDi))
        (pin (num 12) (name "(PCINT22/OC0A/AIN0)PD6") (type BiDi))
        (pin (num 13) (name "(PCINT23/AIN1)PD7") (type BiDi))
        (pin (num 14) (name "(PCINT0/CLKO/ICP1)PB0") (type BiDi))
        (pin (num 15) (name "(PCINT1/OC1A)PB1") (type BiDi))
        (pin (num 16) (name "(PCINT2/OC1B/~SS~)PB2") (type BiDi))
        (pin (num 17) (name "(PCINT3/OC2A/MOSI)PB3") (type BiDi))
        (pin (num 18) (name "(PCINT4/MISO)PB4") (type BiDi))
        (pin (num 19) (name "(PCINT5/SCK)PB5") (type BiDi))
        (pin (num 20) (name AVCC) (type power_in))
        (pin (num 21) (name AREF) (type BiDi))
        (pin (num 22) (name GND) (type power_in))
        (pin (num 23) (name "(PCINT8/ADC0)PC0") (type BiDi))
        (pin (num 24) (name "(PCINT9/ADC1)PC1") (type BiDi))
        (pin (num 25) (name "(PCINT10/ADC2)PC2") (type BiDi))
        (pin (num 26) (name "(PCINT11/ADC3)PC3") (type BiDi))
        (pin (num 27) (name "(PCINT12/SDA/ADC4)PC4") (type BiDi))
        (pin (num 28) (name "(PCINT13/SCL/ADC5)PC5") (type BiDi))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_01X39)
      (description "Connector, single row, 01x39, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X39))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))))
    (libpart (lib conn) (part CONN_02X03)
      (description "Connector, double row, 02x03, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_02X20)
      (description "Connector, double row, 02x20, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X20))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal)
      (description "Two pin crystal")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib microchip) (part MCP23S17)
      (description "16-Bit I/O Expander with SPI Interface (PDIP/SOIC/SSOP)")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf)
      (footprints
        (fp DIP-28_W7.62mm*)
        (fp SOIC-28)
        (fp SSOP-28))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP23S17))
      (pins
        (pin (num 1) (name GPB0) (type BiDi))
        (pin (num 2) (name GPB1) (type BiDi))
        (pin (num 3) (name GPB2) (type BiDi))
        (pin (num 4) (name GPB3) (type BiDi))
        (pin (num 5) (name GPB4) (type BiDi))
        (pin (num 6) (name GPB5) (type BiDi))
        (pin (num 7) (name GPB6) (type BiDi))
        (pin (num 8) (name GPB7) (type BiDi))
        (pin (num 9) (name VCC) (type power_in))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name ~CS) (type input))
        (pin (num 12) (name SCK) (type input))
        (pin (num 13) (name SI) (type output))
        (pin (num 14) (name SO) (type output))
        (pin (num 15) (name A0) (type input))
        (pin (num 16) (name A1) (type input))
        (pin (num 17) (name A2) (type input))
        (pin (num 18) (name ~RESET) (type input))
        (pin (num 19) (name INTB) (type output))
        (pin (num 20) (name INTA) (type output))
        (pin (num 21) (name GPA0) (type BiDi))
        (pin (num 22) (name GPA1) (type BiDi))
        (pin (num 23) (name GPA2) (type BiDi))
        (pin (num 24) (name GPA3) (type BiDi))
        (pin (num 25) (name GPA4) (type BiDi))
        (pin (num 26) (name GPA5) (type BiDi))
        (pin (num 27) (name GPA6) (type BiDi))
        (pin (num 28) (name GPA7) (type BiDi))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib rca) (part RCA_PLUG)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) RCA_PLUG))
      (pins
        (pin (num 1) (name Ext) (type passive))
        (pin (num 2) (name In) (type passive)))))
  (libraries
    (library (logical microchip)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\microchip.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical rca)
      (uri "D:\\ownCloud\\Documents\\Projects\\RC6502\\RC6502 Video Adapter\\rca.lib"))
    (library (logical atmel)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\atmel.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name GV_D0)
      (node (ref J6) (pin 4))
      (node (ref U3) (pin 21)))
    (net (code 2) (name MISO)
      (node (ref U1) (pin 18))
      (node (ref J5) (pin 1))
      (node (ref U2) (pin 14))
      (node (ref U3) (pin 14)))
    (net (code 3) (name "Net-(J6-Pad3)")
      (node (ref J6) (pin 3)))
    (net (code 4) (name "Net-(J6-Pad5)")
      (node (ref J6) (pin 5)))
    (net (code 5) (name GV_D1)
      (node (ref J6) (pin 6))
      (node (ref U3) (pin 22)))
    (net (code 6) (name "Net-(J6-Pad7)")
      (node (ref J6) (pin 7)))
    (net (code 7) (name GV_D2)
      (node (ref U3) (pin 23))
      (node (ref J6) (pin 8)))
    (net (code 8) (name "Net-(J6-Pad9)")
      (node (ref J6) (pin 9)))
    (net (code 9) (name GV_D3)
      (node (ref U3) (pin 24))
      (node (ref J6) (pin 10)))
    (net (code 10) (name GV_A0)
      (node (ref U2) (pin 28))
      (node (ref J6) (pin 20)))
    (net (code 11) (name GV_A5)
      (node (ref U2) (pin 23))
      (node (ref J6) (pin 30)))
    (net (code 12) (name GV_D5)
      (node (ref U3) (pin 26))
      (node (ref J6) (pin 14)))
    (net (code 13) (name GV_D6)
      (node (ref J6) (pin 16))
      (node (ref U3) (pin 27)))
    (net (code 14) (name GV_D7)
      (node (ref J6) (pin 18))
      (node (ref U3) (pin 28)))
    (net (code 15) (name "Net-(U3-Pad19)")
      (node (ref U3) (pin 19)))
    (net (code 16) (name "Net-(J6-Pad17)")
      (node (ref J6) (pin 17)))
    (net (code 17) (name GV_A4)
      (node (ref J6) (pin 28))
      (node (ref U2) (pin 24)))
    (net (code 18) (name GV_A8)
      (node (ref U2) (pin 8))
      (node (ref J6) (pin 19)))
    (net (code 19) (name "Net-(J6-Pad33)")
      (node (ref J6) (pin 33)))
    (net (code 20) (name GV_CS)
      (node (ref U1) (pin 23))
      (node (ref J6) (pin 11)))
    (net (code 21) (name GV_A9)
      (node (ref U2) (pin 7))
      (node (ref J6) (pin 21)))
    (net (code 22) (name "Net-(J6-Pad31)")
      (node (ref J6) (pin 31)))
    (net (code 23) (name GV_D4)
      (node (ref U3) (pin 25))
      (node (ref J6) (pin 12)))
    (net (code 24) (name GV_A1)
      (node (ref U2) (pin 27))
      (node (ref J6) (pin 22)))
    (net (code 25) (name GV_A6)
      (node (ref J6) (pin 32))
      (node (ref U2) (pin 22)))
    (net (code 26) (name "Net-(J6-Pad13)")
      (node (ref J6) (pin 13)))
    (net (code 27) (name "Net-(U3-Pad20)")
      (node (ref U3) (pin 20)))
    (net (code 28) (name GV_A2)
      (node (ref U2) (pin 26))
      (node (ref J6) (pin 24)))
    (net (code 29) (name GV_A7)
      (node (ref U2) (pin 21))
      (node (ref J6) (pin 34)))
    (net (code 30) (name "Net-(J6-Pad15)")
      (node (ref J6) (pin 15)))
    (net (code 31) (name "Net-(J6-Pad35)")
      (node (ref J6) (pin 35)))
    (net (code 32) (name GV_A3)
      (node (ref J6) (pin 26))
      (node (ref U2) (pin 25)))
    (net (code 33) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 34) (name "Net-(J3-Pad2)")
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref JP1) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 35) (name "Net-(JP1-Pad1)")
      (node (ref R3) (pin 2))
      (node (ref JP1) (pin 1)))
    (net (code 36) (name "Net-(U2-Pad2)")
      (node (ref U2) (pin 2)))
    (net (code 37) (name "Net-(J2-Pad37)")
      (node (ref J2) (pin 37)))
    (net (code 38) (name "Net-(J2-Pad35)")
      (node (ref J2) (pin 35)))
    (net (code 39) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19)))
    (net (code 40) (name "Net-(U2-Pad20)")
      (node (ref U2) (pin 20)))
    (net (code 41) (name GV_A13)
      (node (ref U2) (pin 3))
      (node (ref J6) (pin 29)))
    (net (code 42) (name GV_A12)
      (node (ref U2) (pin 4))
      (node (ref J6) (pin 27)))
    (net (code 43) (name GV_A11)
      (node (ref U2) (pin 5))
      (node (ref J6) (pin 25)))
    (net (code 44) (name GV_A10)
      (node (ref U2) (pin 6))
      (node (ref J6) (pin 23)))
    (net (code 45) (name VCC)
      (node (ref J1) (pin 18))
      (node (ref C6) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref U1) (pin 20))
      (node (ref JP2) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref C1) (pin 2))
      (node (ref U3) (pin 9))
      (node (ref U3) (pin 15))
      (node (ref U2) (pin 9)))
    (net (code 46) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 47) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 48) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 50) (name GND)
      (node (ref J4) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref J2) (pin 22))
      (node (ref J2) (pin 30))
      (node (ref J2) (pin 40))
      (node (ref J2) (pin 32))
      (node (ref J2) (pin 19))
      (node (ref J1) (pin 17))
      (node (ref J2) (pin 2))
      (node (ref U1) (pin 22))
      (node (ref J2) (pin 26))
      (node (ref J6) (pin 40))
      (node (ref U3) (pin 16))
      (node (ref U3) (pin 17))
      (node (ref U1) (pin 8))
      (node (ref J4) (pin 2))
      (node (ref J6) (pin 39))
      (node (ref U2) (pin 16))
      (node (ref J5) (pin 6))
      (node (ref U3) (pin 10))
      (node (ref R3) (pin 1))
      (node (ref U2) (pin 10))
      (node (ref U3) (pin 8))
      (node (ref C1) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 17))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 15)))
    (net (code 51) (name "Net-(U1-Pad27)")
      (node (ref U1) (pin 27)))
    (net (code 52) (name P_RESET)
      (node (ref U1) (pin 1))
      (node (ref J5) (pin 5))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 18))
      (node (ref J2) (pin 36))
      (node (ref U2) (pin 18)))
    (net (code 53) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 54) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 55) (name "Net-(J2-Pad38)")
      (node (ref J2) (pin 38)))
    (net (code 56) (name "Net-(J2-Pad16)")
      (node (ref J2) (pin 16)))
    (net (code 57) (name OUT_D0)
      (node (ref U3) (pin 1))
      (node (ref J2) (pin 17)))
    (net (code 58) (name "Net-(J2-Pad27)")
      (node (ref J2) (pin 27)))
    (net (code 59) (name "Net-(J2-Pad18)")
      (node (ref J2) (pin 18)))
    (net (code 60) (name "Net-(J2-Pad28)")
      (node (ref J2) (pin 28)))
    (net (code 61) (name "Net-(J2-Pad25)")
      (node (ref J2) (pin 25)))
    (net (code 62) (name "Net-(J2-Pad29)")
      (node (ref J2) (pin 29)))
    (net (code 63) (name "Net-(J2-Pad39)")
      (node (ref J2) (pin 39)))
    (net (code 64) (name "Net-(J1-Pad27)")
      (node (ref J1) (pin 27)))
    (net (code 65) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 66) (name "Net-(J1-Pad29)")
      (node (ref J1) (pin 29)))
    (net (code 67) (name "Net-(J1-Pad30)")
      (node (ref J1) (pin 30)))
    (net (code 68) (name "Net-(J2-Pad10)")
      (node (ref J2) (pin 10)))
    (net (code 69) (name "Net-(J2-Pad20)")
      (node (ref J2) (pin 20)))
    (net (code 70) (name OUT_D3)
      (node (ref J2) (pin 11))
      (node (ref U3) (pin 4)))
    (net (code 71) (name "Net-(J2-Pad21)")
      (node (ref J2) (pin 21)))
    (net (code 72) (name "Net-(J2-Pad31)")
      (node (ref J2) (pin 31)))
    (net (code 73) (name "Net-(J2-Pad12)")
      (node (ref J2) (pin 12)))
    (net (code 74) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 75) (name OUT_D2)
      (node (ref U3) (pin 3))
      (node (ref J2) (pin 13)))
    (net (code 76) (name "Net-(J2-Pad23)")
      (node (ref J2) (pin 23)))
    (net (code 77) (name "Net-(J2-Pad33)")
      (node (ref J2) (pin 33)))
    (net (code 78) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14)))
    (net (code 79) (name "Net-(J2-Pad24)")
      (node (ref J2) (pin 24)))
    (net (code 80) (name OUT_RDA)
      (node (ref J2) (pin 34))
      (node (ref U1) (pin 4)))
    (net (code 81) (name OUT_D1)
      (node (ref U3) (pin 2))
      (node (ref J2) (pin 15)))
    (net (code 82) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1)))
    (net (code 83) (name "Net-(J2-Pad8)")
      (node (ref J2) (pin 8)))
    (net (code 84) (name "Net-(J2-Pad6)")
      (node (ref J2) (pin 6)))
    (net (code 85) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 86) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 87) (name "Net-(J1-Pad32)")
      (node (ref J1) (pin 32)))
    (net (code 88) (name "Net-(J1-Pad33)")
      (node (ref J1) (pin 33)))
    (net (code 89) (name "Net-(J1-Pad34)")
      (node (ref J1) (pin 34)))
    (net (code 90) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 91) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 92) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 93) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 94) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 95) (name OUT_D4)
      (node (ref U3) (pin 5))
      (node (ref J2) (pin 9)))
    (net (code 96) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 97) (name "Net-(J1-Pad20)")
      (node (ref J1) (pin 20)))
    (net (code 98) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 99) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 100) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 101) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 102) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21)))
    (net (code 103) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25)))
    (net (code 104) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 105) (name RX)
      (node (ref U1) (pin 3))
      (node (ref J1) (pin 36))
      (node (ref J4) (pin 5)))
    (net (code 106) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 107) (name "Net-(J1-Pad37)")
      (node (ref J1) (pin 37)))
    (net (code 108) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 109) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 110) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 111) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 112) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 113) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 114) (name OUT_DA)
      (node (ref U1) (pin 5))
      (node (ref J2) (pin 3)))
    (net (code 115) (name OUT_D6)
      (node (ref U3) (pin 7))
      (node (ref J2) (pin 5)))
    (net (code 116) (name OUT_D5)
      (node (ref J2) (pin 7))
      (node (ref U3) (pin 6)))
    (net (code 117) (name "Net-(J1-Pad38)")
      (node (ref J1) (pin 38)))
    (net (code 118) (name "Net-(J1-Pad39)")
      (node (ref J1) (pin 39)))
    (net (code 119) (name TX)
      (node (ref J1) (pin 35))
      (node (ref U1) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 120) (name "Net-(J4-Pad3)")
      (node (ref J4) (pin 3))
      (node (ref JP2) (pin 2)))
    (net (code 121) (name "Net-(D1-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref D1) (pin 1)))
    (net (code 122) (name "Net-(D2-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref D2) (pin 1)))
    (net (code 123) (name RCA_SYNC)
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 15)))
    (net (code 124) (name SCK)
      (node (ref U3) (pin 12))
      (node (ref U1) (pin 19))
      (node (ref U2) (pin 12))
      (node (ref J5) (pin 3)))
    (net (code 125) (name MOSI)
      (node (ref J5) (pin 4))
      (node (ref U1) (pin 17))
      (node (ref U3) (pin 13))
      (node (ref U2) (pin 13)))
    (net (code 126) (name "Net-(J4-Pad4)")
      (node (ref R4) (pin 1))
      (node (ref J4) (pin 4)))
    (net (code 127) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref J4) (pin 6)))
    (net (code 128) (name GV_E)
      (node (ref U1) (pin 25))
      (node (ref J6) (pin 38)))
    (net (code 129) (name SS)
      (node (ref U1) (pin 16))
      (node (ref U2) (pin 11))
      (node (ref U3) (pin 11)))
    (net (code 130) (name GV_DETECT)
      (node (ref R5) (pin 1))
      (node (ref J6) (pin 37))
      (node (ref U1) (pin 26)))
    (net (code 131) (name "Net-(U1-Pad28)")
      (node (ref U1) (pin 28)))
    (net (code 132) (name XTAL1)
      (node (ref U1) (pin 9))
      (node (ref C3) (pin 2))
      (node (ref Y1) (pin 1)))
    (net (code 133) (name XTAL2)
      (node (ref Y1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 10)))
    (net (code 134) (name "Net-(U1-Pad21)")
      (node (ref U1) (pin 21)))
    (net (code 135) (name RCA_VIDEO)
      (node (ref U1) (pin 13))
      (node (ref D2) (pin 2)))
    (net (code 136) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 137) (name GV_RW)
      (node (ref J6) (pin 36))
      (node (ref U1) (pin 24)))))