(export (version D)
  (design
    (source "D:/ownCloud/Documents/Projects/RC6502/RC6502 ATTiny Clock/ATTiny Clock.sch")
    (date "06/05/2017 01:16:10")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "ATTiny Clock.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value ATTINY85-20PU)
      (footprint Housings_DIP:DIP-8_W7.62mm_Socket)
      (libsource (lib atmel) (part ATTINY85-20PU))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909A23E))
    (comp (ref Y1)
      (value 20Mhz)
      (footprint Crystals:Crystal_HC52-6mm_Vertical)
      (libsource (lib device) (part Crystal))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909A2A2))
    (comp (ref C1)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909A2DD))
    (comp (ref C2)
      (value 22pF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909A308))
    (comp (ref R2)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909E871))
    (comp (ref C3)
      (value 0.1uF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909E8EA))
    (comp (ref R1)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909EE05))
    (comp (ref J3)
      (value CONN_01X06)
      (footprint Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A30B6))
    (comp (ref J1)
      (value CONN_01X39)
      (footprint Pin_Headers:Pin_Header_Angled_1x39_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X39))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3213)))
  (libparts
    (libpart (lib atmel) (part ATTINY25-20PU)
      (aliases
        (alias ATTINY45-20PU)
        (alias ATTINY85-20PU))
      (description "PDIP8, 2k Flash, 128B SRAM, 128B EEPROM, Debug Wire")
      (docs http://www.atmel.com/images/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) ATTINY25-20PU)
        (field (name Footprint) Housings_DIP:DIP-8_W7.62mm))
      (pins
        (pin (num 1) (name "PB5(~RESET~/dW/ADC0/PCINT5)") (type BiDi))
        (pin (num 2) (name "PB3(XTAL1/CLKI/OC1B/ADC3/PCINT3)") (type BiDi))
        (pin (num 3) (name "PB4(XTAL2/CLKO/OC1B/ADC2/PCINT4)") (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name "PB0(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)") (type BiDi))
        (pin (num 6) (name "PB1(MISO/DO/AIN1/OC0B/OC1A/PCINT1)") (type BiDi))
        (pin (num 7) (name "PB2(SCK/USCK/SCL/T0/INT0/ADC1/PCINT2)") (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_01X39)
      (description "Connector, single row, 01x39, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X39))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))))
    (libpart (lib device) (part Crystal)
      (description "Two pin crystal")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical atmel)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\atmel.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 2) (name "Net-(J1-Pad32)")
      (node (ref J1) (pin 32)))
    (net (code 3) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 4) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 5) (name "Net-(J1-Pad33)")
      (node (ref J1) (pin 33)))
    (net (code 6) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 7) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 8) (name "Net-(J1-Pad34)")
      (node (ref J1) (pin 34)))
    (net (code 9) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 10) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25)))
    (net (code 11) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 12) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 13) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 14) (name "Net-(J1-Pad36)")
      (node (ref J1) (pin 36)))
    (net (code 15) (name "Net-(J1-Pad27)")
      (node (ref J1) (pin 27)))
    (net (code 16) (name "Net-(J1-Pad37)")
      (node (ref J1) (pin 37)))
    (net (code 17) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 18) (name "Net-(J1-Pad38)")
      (node (ref J1) (pin 38)))
    (net (code 19) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 20) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 21) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 22) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 23) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 24) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 25) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 26) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 27) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 28) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 29) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 30) (name RESET)
      (node (ref U1) (pin 1))
      (node (ref J3) (pin 6))
      (node (ref J1) (pin 20)))
    (net (code 31) (name "Net-(J1-Pad30)")
      (node (ref J1) (pin 30)))
    (net (code 32) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 33) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 34) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 35) (name "Net-(J1-Pad29)")
      (node (ref J1) (pin 29)))
    (net (code 36) (name "Net-(J1-Pad39)")
      (node (ref J1) (pin 39)))
    (net (code 37) (name "Net-(C3-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 38) (name CLOCK)
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref J3) (pin 5))
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 17))
      (node (ref C3) (pin 2))
      (node (ref J1) (pin 21)))
    (net (code 39) (name XTAL1)
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref Y1) (pin 1)))
    (net (code 40) (name XTAL2)
      (node (ref U1) (pin 3))
      (node (ref Y1) (pin 2))
      (node (ref C2) (pin 1)))
    (net (code 41) (name Vcc)
      (node (ref J1) (pin 18))
      (node (ref U1) (pin 8))
      (node (ref J3) (pin 1)))
    (net (code 42) (name PB2)
      (node (ref J3) (pin 2))
      (node (ref U1) (pin 7)))
    (net (code 43) (name PB1)
      (node (ref J3) (pin 3))
      (node (ref U1) (pin 6)))
    (net (code 44) (name PB0)
      (node (ref J3) (pin 4))
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 5)))))