(export (version D)
  (design
    (source "D:/ownCloud/Documents/Projects/RC6502/RC6502 Backplane/RC6502 Backplane.sch")
    (date "07/01/2019 14:06:22")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "RC6502 Backplane.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J6)
      (value RC6502_Backplane)
      (footprint Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E0F5B))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4437))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4504))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4527))
    (comp (ref C7)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F454F))
    (comp (ref C8)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4586))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4692))
    (comp (ref J5)
      (value RC6502_Backplane)
      (footprint Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4D1E))
    (comp (ref J4)
      (value RC6502_Backplane)
      (footprint Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4E90))
    (comp (ref J3)
      (value RC6502_Backplane)
      (footprint Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F4F1A))
    (comp (ref J1)
      (value RC6502_Backplane)
      (footprint Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm)
      (libsource (lib rc6502_backplane) (part RC6502_Backplane))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F510F))
    (comp (ref J2)
      (value Barrel_Jack)
      (footprint Connectors:BARREL_JACK)
      (libsource (lib conn) (part Barrel_Jack))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F5BA8))
    (comp (ref U1)
      (value LM7805)
      (footprint TO_SOT_Packages_THT:TO-220-3_Horizontal)
      (libsource (lib regul) (part LM7805_TO220))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F5C17))
    (comp (ref JP1)
      (value NO_REG)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F5CB9))
    (comp (ref C1)
      (value 100uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F607E))
    (comp (ref C2)
      (value 10uF)
      (footprint Capacitors_THT:CP_Radial_D4.0mm_P2.00mm)
      (libsource (lib device) (part CP_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2F6198))
    (comp (ref J7)
      (value Mounting)
      (footprint mounting:Mounting)
      (libsource (lib mounting) (part Mounting))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C334F92))
    (comp (ref J8)
      (value Mounting)
      (footprint mounting:Mounting)
      (libsource (lib mounting) (part Mounting))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3350AD))
    (comp (ref J9)
      (value Mounting)
      (footprint mounting:Mounting)
      (libsource (lib mounting) (part Mounting))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3350FF))
    (comp (ref J10)
      (value Mounting)
      (footprint mounting:Mounting)
      (libsource (lib mounting) (part Mounting))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C33514E)))
  (libparts
    (libpart (lib conn) (part Barrel_Jack)
      (aliases
        (alias Jack-DC))
      (description "DC Barrel Jack")
      (docs ~)
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib device) (part CP_Small)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib regul) (part LM7805_TO220)
      (aliases
        (alias LM7806_TO220)
        (alias LM7808_TO220)
        (alias LM7809_TO220)
        (alias LM7810_TO220)
        (alias LM7812_TO220)
        (alias LM7815_TO220)
        (alias LM7818_TO220)
        (alias LM7824_TO220)
        (alias LM78M05_TO220)
        (alias SPX2920U-3.3_TO220)
        (alias SPX2920U-5.0_TO220)
        (alias LF15_TO220)
        (alias LF18_TO220)
        (alias LF25_TO220)
        (alias LF33_TO220)
        (alias LF50_TO220)
        (alias LF60_TO220)
        (alias LF80_TO220)
        (alias LF85_TO220)
        (alias LF120_TO220)
        (alias LF47_TO220)
        (alias LF90_TO220)
        (alias LM341T-05_TO220)
        (alias LM341T-12_TO220)
        (alias LM341T-15_TO220))
      (description "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
      (docs http://www.fairchildsemi.com/ds/LM/LM7805.pdf)
      (footprints
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM7805_TO220)
        (field (name Footprint) TO_SOT_Packages_THT:TO-220_Vertical))
      (pins
        (pin (num 1) (name VI) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib mounting) (part Mounting)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Mounting))
      (pins
        (pin (num 1) (name P1) (type NotConnected))))
    (libpart (lib rc6502_backplane) (part RC6502_Backplane)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) RC6502_Backplane))
      (pins
        (pin (num 1) (name A15) (type BiDi))
        (pin (num 2) (name A14) (type BiDi))
        (pin (num 3) (name A13) (type BiDi))
        (pin (num 4) (name A12) (type BiDi))
        (pin (num 5) (name A11) (type BiDi))
        (pin (num 6) (name A10) (type BiDi))
        (pin (num 7) (name A9) (type BiDi))
        (pin (num 8) (name A8) (type BiDi))
        (pin (num 9) (name A7) (type BiDi))
        (pin (num 10) (name A6) (type BiDi))
        (pin (num 11) (name A5) (type BiDi))
        (pin (num 12) (name A4) (type BiDi))
        (pin (num 13) (name A3) (type BiDi))
        (pin (num 14) (name A2) (type BiDi))
        (pin (num 15) (name A1) (type BiDi))
        (pin (num 16) (name A0) (type BiDi))
        (pin (num 17) (name P17) (type power_out))
        (pin (num 18) (name P18) (type power_out))
        (pin (num 19) (name PHI2) (type BiDi))
        (pin (num 20) (name RESET) (type BiDi))
        (pin (num 21) (name PHI0) (type BiDi))
        (pin (num 22) (name IRQ) (type BiDi))
        (pin (num 23) (name P23) (type BiDi))
        (pin (num 24) (name RW) (type BiDi))
        (pin (num 25) (name READY) (type BiDi))
        (pin (num 26) (name SYNC) (type BiDi))
        (pin (num 27) (name D0) (type BiDi))
        (pin (num 28) (name D1) (type BiDi))
        (pin (num 29) (name D2) (type BiDi))
        (pin (num 30) (name D3) (type BiDi))
        (pin (num 31) (name D4) (type BiDi))
        (pin (num 32) (name D5) (type BiDi))
        (pin (num 33) (name D6) (type BiDi))
        (pin (num 34) (name D7) (type BiDi))
        (pin (num 35) (name TX) (type BiDi))
        (pin (num 36) (name RX) (type BiDi))
        (pin (num 37) (name NMI) (type BiDi))
        (pin (num 38) (name P38) (type BiDi))
        (pin (num 39) (name P39) (type BiDi)))))
  (libraries
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical regul)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\regul.lib"))
    (library (logical rc6502_backplane)
      (uri "D:\\ownCloud\\Documents\\Projects\\RC6502\\RC6502 Backplane\\rc6502_backplane.lib"))
    (library (logical mounting)
      (uri D:\ownCloud\Documents\Projects\RC6502\Templates\mounting.lib)))
  (nets
    (net (code 1) (name /A6)
      (node (ref J5) (pin 10))
      (node (ref J6) (pin 10))
      (node (ref J3) (pin 10))
      (node (ref J4) (pin 10))
      (node (ref J1) (pin 10)))
    (net (code 2) (name /A7)
      (node (ref J1) (pin 9))
      (node (ref J4) (pin 9))
      (node (ref J6) (pin 9))
      (node (ref J3) (pin 9))
      (node (ref J5) (pin 9)))
    (net (code 3) (name /A8)
      (node (ref J4) (pin 8))
      (node (ref J5) (pin 8))
      (node (ref J6) (pin 8))
      (node (ref J3) (pin 8))
      (node (ref J1) (pin 8)))
    (net (code 4) (name /A9)
      (node (ref J5) (pin 7))
      (node (ref J1) (pin 7))
      (node (ref J3) (pin 7))
      (node (ref J6) (pin 7))
      (node (ref J4) (pin 7)))
    (net (code 5) (name /A10)
      (node (ref J5) (pin 6))
      (node (ref J1) (pin 6))
      (node (ref J3) (pin 6))
      (node (ref J6) (pin 6))
      (node (ref J4) (pin 6)))
    (net (code 6) (name /A11)
      (node (ref J4) (pin 5))
      (node (ref J5) (pin 5))
      (node (ref J3) (pin 5))
      (node (ref J6) (pin 5))
      (node (ref J1) (pin 5)))
    (net (code 7) (name /A12)
      (node (ref J4) (pin 4))
      (node (ref J6) (pin 4))
      (node (ref J5) (pin 4))
      (node (ref J3) (pin 4))
      (node (ref J1) (pin 4)))
    (net (code 8) (name /A13)
      (node (ref J4) (pin 3))
      (node (ref J1) (pin 3))
      (node (ref J6) (pin 3))
      (node (ref J3) (pin 3))
      (node (ref J5) (pin 3)))
    (net (code 9) (name /A14)
      (node (ref J5) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref J3) (pin 2))
      (node (ref J6) (pin 2)))
    (net (code 10) (name /A2)
      (node (ref J4) (pin 14))
      (node (ref J3) (pin 14))
      (node (ref J5) (pin 14))
      (node (ref J1) (pin 14))
      (node (ref J6) (pin 14)))
    (net (code 11) (name /A5)
      (node (ref J5) (pin 11))
      (node (ref J1) (pin 11))
      (node (ref J3) (pin 11))
      (node (ref J4) (pin 11))
      (node (ref J6) (pin 11)))
    (net (code 12) (name /A4)
      (node (ref J3) (pin 12))
      (node (ref J6) (pin 12))
      (node (ref J5) (pin 12))
      (node (ref J1) (pin 12))
      (node (ref J4) (pin 12)))
    (net (code 13) (name /A3)
      (node (ref J1) (pin 13))
      (node (ref J6) (pin 13))
      (node (ref J4) (pin 13))
      (node (ref J3) (pin 13))
      (node (ref J5) (pin 13)))
    (net (code 14) (name /A15)
      (node (ref J5) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref J3) (pin 1)))
    (net (code 15) (name /A1)
      (node (ref J4) (pin 15))
      (node (ref J6) (pin 15))
      (node (ref J5) (pin 15))
      (node (ref J3) (pin 15))
      (node (ref J1) (pin 15)))
    (net (code 16) (name /A0)
      (node (ref J4) (pin 16))
      (node (ref J5) (pin 16))
      (node (ref J1) (pin 16))
      (node (ref J3) (pin 16))
      (node (ref J6) (pin 16)))
    (net (code 17) (name VCC)
      (node (ref C6) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref J5) (pin 18))
      (node (ref J3) (pin 18))
      (node (ref C7) (pin 1))
      (node (ref J6) (pin 18))
      (node (ref J4) (pin 18))
      (node (ref C2) (pin 1))
      (node (ref JP1) (pin 2))
      (node (ref J1) (pin 18))
      (node (ref U1) (pin 3)))
    (net (code 18) (name GND)
      (node (ref J2) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref J5) (pin 17))
      (node (ref C4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref J6) (pin 17))
      (node (ref J1) (pin 17))
      (node (ref J3) (pin 17))
      (node (ref J4) (pin 17)))
    (net (code 19) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3)))
    (net (code 20) (name /D3)
      (node (ref J4) (pin 30))
      (node (ref J1) (pin 30))
      (node (ref J6) (pin 30))
      (node (ref J3) (pin 30))
      (node (ref J5) (pin 30)))
    (net (code 21) (name /RESET)
      (node (ref J4) (pin 20))
      (node (ref J3) (pin 20))
      (node (ref J1) (pin 20))
      (node (ref J6) (pin 20))
      (node (ref J5) (pin 20)))
    (net (code 22) (name /PHI2)
      (node (ref J1) (pin 19))
      (node (ref J4) (pin 19))
      (node (ref J5) (pin 19))
      (node (ref J6) (pin 19))
      (node (ref J3) (pin 19)))
    (net (code 23) (name /PHI0)
      (node (ref J6) (pin 21))
      (node (ref J5) (pin 21))
      (node (ref J4) (pin 21))
      (node (ref J3) (pin 21))
      (node (ref J1) (pin 21)))
    (net (code 24) (name /IRQ)
      (node (ref J6) (pin 22))
      (node (ref J5) (pin 22))
      (node (ref J3) (pin 22))
      (node (ref J1) (pin 22))
      (node (ref J4) (pin 22)))
    (net (code 25) (name /R/~W)
      (node (ref J1) (pin 24))
      (node (ref J5) (pin 24))
      (node (ref J3) (pin 24))
      (node (ref J4) (pin 24))
      (node (ref J6) (pin 24)))
    (net (code 26) (name /RDY)
      (node (ref J4) (pin 25))
      (node (ref J5) (pin 25))
      (node (ref J6) (pin 25))
      (node (ref J1) (pin 25))
      (node (ref J3) (pin 25)))
    (net (code 27) (name /SYNC)
      (node (ref J5) (pin 26))
      (node (ref J4) (pin 26))
      (node (ref J1) (pin 26))
      (node (ref J3) (pin 26))
      (node (ref J6) (pin 26)))
    (net (code 28) (name /D0)
      (node (ref J3) (pin 27))
      (node (ref J4) (pin 27))
      (node (ref J5) (pin 27))
      (node (ref J1) (pin 27))
      (node (ref J6) (pin 27)))
    (net (code 29) (name /D1)
      (node (ref J5) (pin 28))
      (node (ref J1) (pin 28))
      (node (ref J4) (pin 28))
      (node (ref J3) (pin 28))
      (node (ref J6) (pin 28)))
    (net (code 30) (name /D2)
      (node (ref J4) (pin 29))
      (node (ref J1) (pin 29))
      (node (ref J5) (pin 29))
      (node (ref J3) (pin 29))
      (node (ref J6) (pin 29)))
    (net (code 31) (name /D4)
      (node (ref J5) (pin 31))
      (node (ref J4) (pin 31))
      (node (ref J6) (pin 31))
      (node (ref J3) (pin 31))
      (node (ref J1) (pin 31)))
    (net (code 32) (name /D5)
      (node (ref J4) (pin 32))
      (node (ref J3) (pin 32))
      (node (ref J1) (pin 32))
      (node (ref J5) (pin 32))
      (node (ref J6) (pin 32)))
    (net (code 33) (name /D6)
      (node (ref J4) (pin 33))
      (node (ref J1) (pin 33))
      (node (ref J5) (pin 33))
      (node (ref J6) (pin 33))
      (node (ref J3) (pin 33)))
    (net (code 34) (name /D7)
      (node (ref J4) (pin 34))
      (node (ref J3) (pin 34))
      (node (ref J5) (pin 34))
      (node (ref J6) (pin 34))
      (node (ref J1) (pin 34)))
    (net (code 35) (name /TX)
      (node (ref J4) (pin 35))
      (node (ref J6) (pin 35))
      (node (ref J3) (pin 35))
      (node (ref J1) (pin 35))
      (node (ref J5) (pin 35)))
    (net (code 36) (name /RX)
      (node (ref J1) (pin 36))
      (node (ref J4) (pin 36))
      (node (ref J6) (pin 36))
      (node (ref J3) (pin 36))
      (node (ref J5) (pin 36)))
    (net (code 37) (name /NMI)
      (node (ref J6) (pin 37))
      (node (ref J3) (pin 37))
      (node (ref J5) (pin 37))
      (node (ref J4) (pin 37))
      (node (ref J1) (pin 37)))
    (net (code 38) (name /SPARE1)
      (node (ref J1) (pin 38))
      (node (ref J5) (pin 38))
      (node (ref J3) (pin 38))
      (node (ref J6) (pin 38))
      (node (ref J4) (pin 38)))
    (net (code 39) (name /SPARE2)
      (node (ref J3) (pin 39))
      (node (ref J1) (pin 39))
      (node (ref J4) (pin 39))
      (node (ref J6) (pin 39))
      (node (ref J5) (pin 39)))
    (net (code 40) (name /SPARE0)
      (node (ref J6) (pin 23))
      (node (ref J4) (pin 23))
      (node (ref J1) (pin 23))
      (node (ref J3) (pin 23))
      (node (ref J5) (pin 23)))
    (net (code 41) (name "Net-(C1-Pad1)")
      (node (ref JP1) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 42) (name "Net-(J7-Pad1)")
      (node (ref J7) (pin 1)))
    (net (code 43) (name "Net-(J8-Pad1)")
      (node (ref J8) (pin 1)))
    (net (code 44) (name "Net-(J9-Pad1)")
      (node (ref J9) (pin 1)))
    (net (code 45) (name "Net-(J10-Pad1)")
      (node (ref J10) (pin 1)))))