(export (version D)
  (design
    (source "C:/Users/Stache/Documents/KiCad Projects/6502Computer/rev1.a/6502Computer.sch")
    (date "5/25/2016 8:58:05 PM")
    (tool "Eeschema 4.0.2-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 6502Computer.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name "/page 1/") (tstamps /56D50E2C/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source page1.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/page 2/") (tstamps /56D50EEB/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source page2.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name "/page 3/") (tstamps /56D50F54/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source page3.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name "/page 4/") (tstamps /56D665EF/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source page4.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref LED1)
      (value LED)
      (footprint 6502Library:WP1503CB_LED)
      (libsource (lib device) (part LED))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56D512BB))
    (comp (ref R1)
      (value 330)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56D512BD))
    (comp (ref J1)
      (value BARREL_JACK)
      (footprint 6502Library:Barrel_Jack_PJ002A)
      (libsource (lib 6502) (part BARREL_JACK_NEW))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56D512C3))
    (comp (ref C3)
      (value .33uf)
      (footprint 6502Library:C_Disc_D6_P5)
      (libsource (lib device) (part C))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56D512C4))
    (comp (ref U4)
      (value AddressDecoderModule)
      (footprint 6502Library:Address_Decoder_CPLD2)
      (libsource (lib propeller) (part AddressDecoderModule))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E51955))
    (comp (ref C10)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E51F5E))
    (comp (ref C11)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E524A7))
    (comp (ref C4)
      (value 47uf)
      (footprint Capacitors_ThroughHole:C_Radial_D5_L11_P2)
      (libsource (lib device) (part CP1))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E6E633))
    (comp (ref R2)
      (value 422k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E6FF2F))
    (comp (ref R3)
      (value 53.6k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E70138))
    (comp (ref C5)
      (value 1000uf)
      (footprint Capacitors_ThroughHole:C_Radial_D12.5_L25_P5)
      (libsource (lib device) (part CP1))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E712A4))
    (comp (ref C6)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E71BA5))
    (comp (ref U1)
      (value MIC29150-5.0WT)
      (footprint mod_to:to220-horiz_5772)
      (libsource (lib propeller) (part MIC29300-5.0WT))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E73B6A))
    (comp (ref C1)
      (value 1000uf)
      (footprint Capacitors_ThroughHole:C_Radial_D10_L16_P5)
      (libsource (lib device) (part CP1))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E743F1))
    (comp (ref C2)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E745E0))
    (comp (ref U3)
      (value MIC29150-3.3WT)
      (footprint mod_to:to220-horiz-notab)
      (libsource (lib propeller) (part MIC29300-5.0WT))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E7582A))
    (comp (ref C7)
      (value 47uf)
      (footprint Capacitors_ThroughHole:C_Radial_D5_L11_P2)
      (libsource (lib device) (part CP1))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E7583C))
    (comp (ref C8)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E75842))
    (comp (ref C9)
      (value .33uf)
      (footprint 6502Library:C_Disc_D6_P5)
      (libsource (lib device) (part C))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E75B8C))
    (comp (ref U2)
      (value MIC29152WT)
      (footprint mod_to:to220-5-horiz-notab)
      (libsource (lib propeller) (part MIC29302))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 56E9A048))
    (comp (ref JP1)
      (value DECODER_JUMPERS)
      (footprint 6502Library:Pin_Header_Straight_3x05)
      (libsource (lib 6502) (part DECODER_JUMPERS))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 570B77B3))
    (comp (ref SW1)
      (value SPST2)
      (footprint 6502Library:SW_Micro_Right_Angle_SPST)
      (libsource (lib 6502) (part SPST2))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 57142567))
    (comp (ref P16)
      (value CONN_01X12)
      (footprint 6502Library:Socket_Strip_Straight_1x12)
      (libsource (lib conn) (part CONN_01X12))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 5723B0F7))
    (comp (ref P1)
      (value CONN_01X07)
      (footprint 6502Library:Socket_Strip_Straight_1x07)
      (libsource (lib conn) (part CONN_01X07))
      (sheetpath (names "/page 1/") (tstamps /56D50E2C/))
      (tstamp 57296FE0))
    (comp (ref U6)
      (value 65C02)
      (footprint mod_pth_circuits:dil_40-600_socket)
      (libsource (lib 6502) (part 65C02))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56D5154B))
    (comp (ref U7)
      (value AT28C256_EEPROM)
      (footprint 6502Library:28-526-11-SOCKET)
      (libsource (lib 6502) (part AT28C256_EEPROM))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56D5154C))
    (comp (ref U8)
      (value 62256_SRAM)
      (footprint mod_pth_circuits:dil_28-600_socket)
      (libsource (lib 6502) (part 62256_SRAM))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56D5154D))
    (comp (ref Y1)
      (value ECS-2100X-1MHZ)
      (footprint 6502Library:ECS-2100AX)
      (libsource (lib 6502) (part ECS-2100X-1MHZ))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56D51555))
    (comp (ref SW2)
      (value SW_PUSH_SAFE)
      (footprint 6502Library:1-1825027-1-TACTILE_SWITCH)
      (libsource (lib 6502) (part SW_PUSH_SAFE))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56D51558))
    (comp (ref P3)
      (value CONN_01X20)
      (footprint 6502Library:Socket_Strip_Straight_1x20)
      (libsource (lib conn) (part CONN_01X20))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E033B9))
    (comp (ref P4)
      (value CONN_01X20)
      (footprint 6502Library:Socket_Strip_Straight_1x20)
      (libsource (lib conn) (part CONN_01X20))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E03703))
    (comp (ref U5)
      (value DS1813_EconoReset)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib propeller) (part DS1813_EconoReset))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E04919))
    (comp (ref C12)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E1ED84))
    (comp (ref C15)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E1FD22))
    (comp (ref C16)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E2079B))
    (comp (ref C14)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E20E0A))
    (comp (ref C13)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 56E22E50))
    (comp (ref RR1)
      (value RR7)
      (footprint 6502Library:7_pin_resistor_network)
      (libsource (lib 6502) (part RR7))
      (sheetpath (names "/page 2/") (tstamps /56D50EEB/))
      (tstamp 57228700))
    (comp (ref U10)
      (value 6551)
      (footprint mod_pth_circuits:dil_28-600_socket)
      (libsource (lib 6502) (part 6551))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56D5C1F8))
    (comp (ref Y2)
      (value 1.8432MHZ_OSC)
      (footprint 6502Library:ECS-2100AX)
      (libsource (lib 6502) (part 1.8432MHZ_OSC))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56D5C574))
    (comp (ref U12)
      (value 6551)
      (footprint mod_pth_circuits:dil_28-600_socket)
      (libsource (lib 6502) (part 6551))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56D5CB6F))
    (comp (ref U9)
      (value 6522)
      (footprint mod_pth_circuits:dil_40-600_socket)
      (libsource (lib 6502) (part 6522))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56D653D3))
    (comp (ref U11)
      (value 6522)
      (footprint mod_pth_circuits:dil_40-600_socket)
      (libsource (lib 6502) (part 6522))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56D6549A))
    (comp (ref U13)
      (value 6581_SID)
      (footprint mod_pth_circuits:dil_28-600_socket)
      (libsource (lib 6502) (part 6581_SID))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56D65B1D))
    (comp (ref C26)
      (value 2.2nf)
      (footprint 6502Library:C_Axial_D6_L11_P18)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DA3E33))
    (comp (ref C25)
      (value 2.2nf)
      (footprint 6502Library:C_Axial_D6_L11_P18)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DA3E6F))
    (comp (ref R10)
      (value 1k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DA44A4))
    (comp (ref JP4)
      (value JUMPER3)
      (footprint 6502Library:Pin_Header_Straight_1x03)
      (libsource (lib device) (part JUMPER3))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DDCC04))
    (comp (ref JP5)
      (value JUMPER3)
      (footprint 6502Library:Pin_Header_Straight_1x03)
      (libsource (lib device) (part JUMPER3))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DDD716))
    (comp (ref JP6)
      (value JUMPER3)
      (footprint 6502Library:Pin_Header_Straight_1x03)
      (libsource (lib device) (part JUMPER3))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DDDC75))
    (comp (ref JP7)
      (value JUMPER3)
      (footprint 6502Library:Pin_Header_Straight_1x03)
      (libsource (lib device) (part JUMPER3))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DDE4FB))
    (comp (ref R11)
      (value 10k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DE5D5D))
    (comp (ref C33)
      (value 1nf)
      (footprint 6502Library:C_Disc_D6_P3.5_Skinny)
      (libsource (lib device) (part C))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DE5E4D))
    (comp (ref Q1)
      (value 2N2222A)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib 6502Computer-rescue) (part PN2222A-RESCUE-6502Computer))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DE656A))
    (comp (ref R12)
      (value 1k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DE6601))
    (comp (ref C38)
      (value 10uf)
      (footprint Capacitors_ThroughHole:C_Radial_D12.5_L25_P5)
      (libsource (lib device) (part CP1_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DE79B1))
    (comp (ref C28)
      (value 1nf)
      (footprint 6502Library:C_Disc_D6_P3.5_Skinny)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DF153A))
    (comp (ref C30)
      (value 1nf)
      (footprint 6502Library:C_Disc_D6_P3.5_Skinny)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DF1700))
    (comp (ref C27)
      (value 1nf)
      (footprint 6502Library:C_Disc_D6_P3.5_Skinny)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DF3BED))
    (comp (ref U15)
      (value BQ3285E_RTC)
      (footprint mod_pth_circuits:dil_24-600_socket)
      (libsource (lib propeller) (part BQ3285E_RTC))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DF95CE))
    (comp (ref Y3)
      (value 32.768kHz)
      (footprint 6502Library:crystal_tc-38_horiz)
      (libsource (lib device) (part Crystal_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DF9769))
    (comp (ref BT1)
      (value "CR2032 3V")
      (footprint 6502Library:BU2032SM)
      (libsource (lib device) (part Battery))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56DFBFC2))
    (comp (ref JP8)
      (value JUMPER3)
      (footprint 6502Library:Pin_Header_Straight_1x03)
      (libsource (lib device) (part JUMPER3))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E0273F))
    (comp (ref P11)
      (value CONN_01X03)
      (footprint 6502Library:Socket_Strip_Straight_1x03)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E05604))
    (comp (ref P7)
      (value CONN_01X05)
      (footprint 6502Library:Socket_Strip_Straight_1x05)
      (libsource (lib conn) (part CONN_01X05))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E17E0D))
    (comp (ref C18)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E25602))
    (comp (ref C21)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E25DD4))
    (comp (ref C19)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E28688))
    (comp (ref C17)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E29AC9))
    (comp (ref C37)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E2A1D2))
    (comp (ref C20)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E2B91C))
    (comp (ref C31)
      (value .47uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E2F8D5))
    (comp (ref C34)
      (value .47nf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E2F9DE))
    (comp (ref C29)
      (value .22uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E2FF36))
    (comp (ref C36)
      (value 10uf)
      (footprint Capacitors_ThroughHole:C_Radial_D5_L11_P2)
      (libsource (lib device) (part CP1_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E3002E))
    (comp (ref C32)
      (value .47nf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E3447B))
    (comp (ref C35)
      (value 10uf)
      (footprint Capacitors_ThroughHole:C_Radial_D5_L11_P2)
      (libsource (lib device) (part CP1_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E345B9))
    (comp (ref D1)
      (value 1N5817)
      (footprint 6502Library:diode_do41)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E31250))
    (comp (ref D2)
      (value 1N5817)
      (footprint 6502Library:diode_do41)
      (libsource (lib device) (part D_Schottky_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E322AF))
    (comp (ref J3)
      (value AUDIO_OUT)
      (footprint 6502Library:RCJ013AUDIO)
      (libsource (lib propeller) (part TV_OUT))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E4365B))
    (comp (ref J2)
      (value JACK_2P)
      (footprint 6502Library:SJ13525NHeadphone)
      (libsource (lib device) (part JACK_2P))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E52F89))
    (comp (ref P12)
      (value CONN_01X02)
      (footprint 6502Library:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E53740))
    (comp (ref P5)
      (value CONN_01X05)
      (footprint 6502Library:Socket_Strip_Straight_1x05)
      (libsource (lib conn) (part CONN_01X05))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E579C0))
    (comp (ref P6)
      (value CONN_02X09)
      (footprint 6502Library:Socket_Strip_Angled_2x09)
      (libsource (lib conn) (part CONN_02X09))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E7FC3B))
    (comp (ref P8)
      (value CONN_02X09)
      (footprint 6502Library:Socket_Strip_Angled_2x09)
      (libsource (lib conn) (part CONN_02X09))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E83283))
    (comp (ref P10)
      (value CONN_02X09)
      (footprint 6502Library:Socket_Strip_Angled_2x09)
      (libsource (lib conn) (part CONN_02X09))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E835AC))
    (comp (ref P9)
      (value CONN_02X09)
      (footprint 6502Library:Socket_Strip_Angled_2x09)
      (libsource (lib conn) (part CONN_02X09))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56E838AF))
    (comp (ref FB1)
      (value FB)
      (footprint 6502Library:Ferrite_Bead_Horizontal_RM10mm)
      (libsource (lib propeller) (part FB))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56EC6D77))
    (comp (ref C23)
      (value 6pf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56ED6EF5))
    (comp (ref U14)
      (value 74LS138N)
      (footprint mod_pth_circuits:dil_16-300_socket)
      (libsource (lib addressdecoder) (part 74LS138N))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56F1BE38))
    (comp (ref C22)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56F2C229))
    (comp (ref C39)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56F2ED86))
    (comp (ref FB2)
      (value FB)
      (footprint 6502Library:Ferrite_Bead_Horizontal_RM10mm)
      (libsource (lib propeller) (part FB))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 57045729))
    (comp (ref FB3)
      (value FB)
      (footprint 6502Library:Ferrite_Bead_Horizontal_RM10mm)
      (libsource (lib propeller) (part FB))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 57047EB5))
    (comp (ref U16)
      (value 7400)
      (footprint mod_pth_circuits:dil_14-300_socket)
      (libsource (lib 6502) (part 74LS00_NEW))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 5712E747))
    (comp (ref P15)
      (value CONN_01X05)
      (footprint 6502Library:Pin_Header_Angled_1x05)
      (libsource (lib conn) (part CONN_01X05))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 57204364))
    (comp (ref C24)
      (value 6pf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 3/") (tstamps /56D50F54/))
      (tstamp 56ED7234))
    (comp (ref U18)
      (value 24LC256_EEPROM)
      (footprint mod_pth_circuits:dil_8-300_socket)
      (libsource (lib propeller) (part 24LC256_EEPROM))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D6694A))
    (comp (ref J5)
      (value VGA)
      (footprint 6502Library:117343442VGA)
      (libsource (lib vga) (part VGA))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D66D62))
    (comp (ref K1)
      (value PS2_KEYBOARD)
      (footprint 6502Library:MD60SM)
      (libsource (lib keyboard_parts) (part PS2_FEMALE))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D67A23))
    (comp (ref U17)
      (value Prop_P8X32A)
      (footprint mod_pth_circuits:dil_40-600_socket)
      (libsource (lib propeller) (part Prop_P8X32A))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D8535A))
    (comp (ref R29)
      (value 10k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9A5EA))
    (comp (ref Y4)
      (value "5MHz 20pf")
      (footprint mod_crystal:crystal_hc-49s)
      (libsource (lib device) (part Crystal_Small))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9AABF))
    (comp (ref P14)
      (value PROP_PLUG)
      (footprint 6502Library:PROP_PLUG)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9B3B1))
    (comp (ref R18)
      (value 240)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9CA26))
    (comp (ref R17)
      (value 240)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9D386))
    (comp (ref R26)
      (value 470)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9D9EF))
    (comp (ref R25)
      (value 240)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9DACF))
    (comp (ref R21)
      (value 240)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9E7D5))
    (comp (ref R22)
      (value 470)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9E858))
    (comp (ref R23)
      (value 240)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9EDC0))
    (comp (ref R24)
      (value 470)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56D9EE2A))
    (comp (ref R28)
      (value 10K)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56DA1233))
    (comp (ref R19)
      (value 100)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56DA1AF9))
    (comp (ref R20)
      (value 100)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56DA203A))
    (comp (ref R30)
      (value 10K)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56DA24F7))
    (comp (ref CON1)
      (value SD_Card_SPI)
      (footprint 6502Library:DM1AASFPEJ_SDCARD)
      (libsource (lib propeller) (part SD_Card_SPI))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56DC7BDC))
    (comp (ref P13)
      (value CONN_01X12)
      (footprint 6502Library:Socket_Strip_Straight_1x12)
      (libsource (lib conn) (part CONN_01X12))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E07EB2))
    (comp (ref C41)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E39A3D))
    (comp (ref C42)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E3ADD9))
    (comp (ref C43)
      (value 1uf)
      (footprint 6502Library:C_Disc_D6_P5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E418A5))
    (comp (ref R27)
      (value 10k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E42757))
    (comp (ref R16)
      (value 10k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E4461E))
    (comp (ref J4)
      (value TV_OUT)
      (footprint 6502Library:RCJ014VIDEO)
      (libsource (lib propeller) (part TV_OUT))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E3D9FF))
    (comp (ref R13)
      (value 1.1k)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E3F87E))
    (comp (ref R14)
      (value 560)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E411C3))
    (comp (ref R15)
      (value 270)
      (footprint 6502Library:Resistor_Horizontal_RM10mm)
      (libsource (lib device) (part R))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56E41F6D))
    (comp (ref C40)
      (value .1uf)
      (footprint 6502Library:C_Disc_D3_P2.5)
      (libsource (lib device) (part C_Small))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 56F3C5ED))
    (comp (ref JP9)
      (value PROP_JUMPERS)
      (footprint 6502Library:Pin_Header_Straight_2x06)
      (libsource (lib 6502) (part PROP_JUMPERS))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 570B67CB))
    (comp (ref SW3)
      (value SW_PUSH_SAFE)
      (footprint 6502Library:1-1825027-1-TACTILE_SWITCH)
      (libsource (lib 6502) (part SW_PUSH_SAFE))
      (sheetpath (names "/page 4/") (tstamps /56D665EF/))
      (tstamp 571FDFD2)))
  (libparts
    (libpart (lib 6502) (part 1.8432MHZ_OSC)
      (fields
        (field (name Reference) Y)
        (field (name Value) 1.8432MHZ_OSC))
      (pins
        (pin (num 1) (name GND) (type passive))
        (pin (num 4) (name GND) (type input))
        (pin (num 5) (name OUTPUT) (type output))
        (pin (num 8) (name +5V) (type input))))
    (libpart (lib propeller) (part 24LC256_EEPROM)
      (fields
        (field (name Reference) U)
        (field (name Value) 24LC256_EEPROM))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SDA) (type input))
        (pin (num 6) (name SCL) (type input))
        (pin (num 7) (name WP) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib 6502) (part 62256_SRAM)
      (fields
        (field (name Reference) U)
        (field (name Value) 62256_SRAM))
      (pins
        (pin (num 1) (name A14) (type input))
        (pin (num 2) (name A12) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A6) (type input))
        (pin (num 5) (name A5) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A1) (type input))
        (pin (num 10) (name A0) (type input))
        (pin (num 11) (name 1/O0) (type input))
        (pin (num 12) (name I/O1) (type input))
        (pin (num 13) (name I/O2) (type input))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name I/O3) (type input))
        (pin (num 16) (name I/O4) (type input))
        (pin (num 17) (name I/O5) (type input))
        (pin (num 18) (name I/O6) (type input))
        (pin (num 19) (name I/O7) (type input))
        (pin (num 20) (name ~CE) (type input))
        (pin (num 21) (name A10) (type input))
        (pin (num 22) (name ~OE) (type input))
        (pin (num 23) (name A11) (type input))
        (pin (num 24) (name A9) (type input))
        (pin (num 25) (name A8) (type input))
        (pin (num 26) (name A13) (type input))
        (pin (num 27) (name ~WE) (type input))
        (pin (num 28) (name VCC) (type power_in))))
    (libpart (lib 6502) (part 6522)
      (fields
        (field (name Reference) U)
        (field (name Value) 6522))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name PA0) (type input))
        (pin (num 3) (name PA1) (type input))
        (pin (num 4) (name PA2) (type input))
        (pin (num 5) (name PA3) (type input))
        (pin (num 6) (name PA4) (type input))
        (pin (num 7) (name PA5) (type input))
        (pin (num 8) (name PA6) (type input))
        (pin (num 9) (name PA7) (type input))
        (pin (num 10) (name PB0) (type input))
        (pin (num 11) (name PB1) (type input))
        (pin (num 12) (name PB2) (type input))
        (pin (num 13) (name PB3) (type input))
        (pin (num 14) (name PB4) (type input))
        (pin (num 15) (name PB5) (type input))
        (pin (num 16) (name PB6) (type input))
        (pin (num 17) (name PB7) (type input))
        (pin (num 18) (name CB1) (type input))
        (pin (num 19) (name CB2) (type input))
        (pin (num 20) (name VCC) (type power_in))
        (pin (num 21) (name IRQ) (type input))
        (pin (num 22) (name RW) (type input))
        (pin (num 23) (name CS2) (type input))
        (pin (num 24) (name CS1) (type input))
        (pin (num 25) (name PHI2) (type input))
        (pin (num 26) (name D7) (type input))
        (pin (num 27) (name D6) (type input))
        (pin (num 28) (name D5) (type input))
        (pin (num 29) (name D4) (type input))
        (pin (num 30) (name D3) (type input))
        (pin (num 31) (name D2) (type input))
        (pin (num 32) (name D1) (type input))
        (pin (num 33) (name D0) (type input))
        (pin (num 34) (name RES) (type input))
        (pin (num 35) (name RS3) (type input))
        (pin (num 36) (name RS2) (type input))
        (pin (num 37) (name RS1) (type input))
        (pin (num 38) (name RS0) (type input))
        (pin (num 39) (name CA2) (type input))
        (pin (num 40) (name CA1) (type input))))
    (libpart (lib 6502) (part 6551)
      (fields
        (field (name Reference) U)
        (field (name Value) 6551))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name CS0) (type input))
        (pin (num 3) (name CS1) (type input))
        (pin (num 4) (name RES) (type input))
        (pin (num 5) (name RXC) (type input))
        (pin (num 6) (name XTAL1) (type input))
        (pin (num 7) (name XTAL2) (type input))
        (pin (num 8) (name RTS) (type input))
        (pin (num 9) (name CTS) (type input))
        (pin (num 10) (name TXD) (type input))
        (pin (num 11) (name DTR) (type input))
        (pin (num 12) (name RXD) (type input))
        (pin (num 13) (name RS0) (type input))
        (pin (num 14) (name RS1) (type input))
        (pin (num 15) (name VCC) (type power_in))
        (pin (num 16) (name DCD) (type input))
        (pin (num 17) (name DSR) (type input))
        (pin (num 18) (name D0) (type input))
        (pin (num 19) (name D1) (type input))
        (pin (num 20) (name D2) (type input))
        (pin (num 21) (name D3) (type input))
        (pin (num 22) (name D4) (type input))
        (pin (num 23) (name D5) (type input))
        (pin (num 24) (name D6) (type input))
        (pin (num 25) (name D7) (type input))
        (pin (num 26) (name IRQ) (type input))
        (pin (num 27) (name PHI2) (type input))
        (pin (num 28) (name RW) (type input))))
    (libpart (lib 6502) (part 6581_SID)
      (fields
        (field (name Reference) U)
        (field (name Value) 6581_SID))
      (pins
        (pin (num 1) (name CAP1A) (type input))
        (pin (num 2) (name CAP1B) (type input))
        (pin (num 3) (name CAP2A) (type input))
        (pin (num 4) (name CAP2B) (type input))
        (pin (num 5) (name RES) (type input))
        (pin (num 6) (name PHI2) (type input))
        (pin (num 7) (name RW) (type input))
        (pin (num 8) (name CS) (type input))
        (pin (num 9) (name A0) (type input))
        (pin (num 10) (name A1) (type input))
        (pin (num 11) (name A2) (type input))
        (pin (num 12) (name A3) (type input))
        (pin (num 13) (name A4) (type input))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name D0) (type input))
        (pin (num 16) (name D1) (type input))
        (pin (num 17) (name D2) (type input))
        (pin (num 18) (name D3) (type input))
        (pin (num 19) (name D4) (type input))
        (pin (num 20) (name D5) (type input))
        (pin (num 21) (name D6) (type input))
        (pin (num 22) (name D7) (type input))
        (pin (num 23) (name POTY) (type input))
        (pin (num 24) (name POTX) (type input))
        (pin (num 25) (name VCC) (type input))
        (pin (num 26) (name EXT-IN) (type input))
        (pin (num 27) (name AUDIO-OUT) (type input))
        (pin (num 28) (name VDD) (type input))))
    (libpart (lib 6502) (part 65C02)
      (fields
        (field (name Reference) U)
        (field (name Value) 65C02))
      (pins
        (pin (num 1) (name VPB) (type input))
        (pin (num 2) (name RDY) (type input))
        (pin (num 3) (name PHI1O) (type input))
        (pin (num 4) (name IRQB) (type input))
        (pin (num 5) (name MLB) (type input))
        (pin (num 6) (name NMIB) (type input))
        (pin (num 7) (name SYNC) (type input))
        (pin (num 8) (name VDD) (type power_in))
        (pin (num 9) (name A0) (type input))
        (pin (num 10) (name A1) (type input))
        (pin (num 11) (name A2) (type input))
        (pin (num 12) (name A3) (type input))
        (pin (num 13) (name A4) (type input))
        (pin (num 14) (name A5) (type input))
        (pin (num 15) (name A6) (type input))
        (pin (num 16) (name A7) (type input))
        (pin (num 17) (name A8) (type input))
        (pin (num 18) (name A9) (type input))
        (pin (num 19) (name A10) (type input))
        (pin (num 20) (name A11) (type input))
        (pin (num 21) (name VSS) (type power_in))
        (pin (num 22) (name A12) (type input))
        (pin (num 23) (name A13) (type input))
        (pin (num 24) (name A14) (type input))
        (pin (num 25) (name A15) (type input))
        (pin (num 26) (name D7) (type input))
        (pin (num 27) (name D6) (type input))
        (pin (num 28) (name D5) (type input))
        (pin (num 29) (name D4) (type input))
        (pin (num 30) (name D3) (type input))
        (pin (num 31) (name D2) (type input))
        (pin (num 32) (name D1) (type input))
        (pin (num 33) (name D0) (type input))
        (pin (num 34) (name RWB) (type input))
        (pin (num 35) (name NC) (type BiDi))
        (pin (num 36) (name BE) (type input))
        (pin (num 37) (name PHI2) (type input))
        (pin (num 38) (name SOB) (type output))
        (pin (num 39) (name PHI2O) (type input))
        (pin (num 40) (name RESB) (type input))))
    (libpart (lib 6502) (part 74LS00_NEW)
      (description "Quad nand2")
      (footprints
        (fp 14DIP300*)
        (fp SO14*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS00_NEW))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib addressdecoder) (part 74LS138N)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS138N))
      (pins
        (pin (num 1) (name A) (type output))
        (pin (num 2) (name B) (type output))
        (pin (num 3) (name C) (type output))
        (pin (num 4) (name ~G2A) (type input))
        (pin (num 5) (name ~G2B) (type input))
        (pin (num 6) (name G1) (type input))
        (pin (num 7) (name Y7) (type output))
        (pin (num 8) (name GND) (type input))
        (pin (num 9) (name Y6) (type passive))
        (pin (num 10) (name Y5) (type output))
        (pin (num 11) (name Y4) (type passive))
        (pin (num 12) (name Y3) (type passive))
        (pin (num 13) (name Y2) (type passive))
        (pin (num 14) (name Y1) (type output))
        (pin (num 15) (name Y0) (type passive))
        (pin (num 16) (name VCC) (type input))))
    (libpart (lib 6502) (part AT28C256_EEPROM)
      (fields
        (field (name Reference) U)
        (field (name Value) AT28C256_EEPROM))
      (pins
        (pin (num 1) (name A14) (type input))
        (pin (num 2) (name A12) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A6) (type input))
        (pin (num 5) (name A5) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A1) (type input))
        (pin (num 10) (name A0) (type input))
        (pin (num 11) (name 1/O0) (type input))
        (pin (num 12) (name I/O1) (type input))
        (pin (num 13) (name I/O2) (type input))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name I/O3) (type input))
        (pin (num 16) (name I/O4) (type input))
        (pin (num 17) (name I/O5) (type input))
        (pin (num 18) (name I/O6) (type input))
        (pin (num 19) (name I/O7) (type input))
        (pin (num 20) (name ~CE) (type input))
        (pin (num 21) (name A10) (type input))
        (pin (num 22) (name ~OE) (type input))
        (pin (num 23) (name A11) (type input))
        (pin (num 24) (name A9) (type input))
        (pin (num 25) (name A8) (type input))
        (pin (num 26) (name A13) (type input))
        (pin (num 27) (name ~WE) (type input))
        (pin (num 28) (name VCC) (type power_in))))
    (libpart (lib propeller) (part AddressDecoderModule)
      (fields
        (field (name Reference) U)
        (field (name Value) AddressDecoderModule))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name PHI2) (type input))
        (pin (num 3) (name SE1) (type input))
        (pin (num 4) (name SE2) (type input))
        (pin (num 5) (name SE3) (type input))
        (pin (num 6) (name SE4) (type input))
        (pin (num 7) (name SE5) (type input))
        (pin (num 8) (name RW) (type input))
        (pin (num 12) (name A4) (type input))
        (pin (num 13) (name A5) (type input))
        (pin (num 14) (name A6) (type input))
        (pin (num 15) (name A7) (type input))
        (pin (num 16) (name A8) (type input))
        (pin (num 17) (name A9) (type input))
        (pin (num 18) (name A10) (type input))
        (pin (num 19) (name A11) (type input))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name VCC) (type power_in))
        (pin (num 22) (name A12) (type input))
        (pin (num 23) (name A13) (type input))
        (pin (num 24) (name A14) (type input))
        (pin (num 25) (name A15) (type input))
        (pin (num 26) (name RAM_CE) (type output))
        (pin (num 27) (name ROM_CE) (type output))
        (pin (num 28) (name WE) (type output))
        (pin (num 29) (name OE) (type output))
        (pin (num 33) (name CS1) (type output))
        (pin (num 34) (name CS2) (type output))
        (pin (num 35) (name CS3) (type output))
        (pin (num 36) (name CS4) (type output))
        (pin (num 37) (name CS5) (type output))
        (pin (num 38) (name CS6) (type output))
        (pin (num 39) (name CS7) (type output))
        (pin (num 40) (name CS8) (type output))))
    (libpart (lib 6502) (part BARREL_JACK_NEW)
      (description "DC Barrel Jack")
      (fields
        (field (name Reference) CON)
        (field (name Value) BARREL_JACK_NEW))
      (pins
        (pin (num 1) (name ~) (type power_out))
        (pin (num 2) (name ~) (type power_out))
        (pin (num 3) (name ~) (type NotConnected))))
    (libpart (lib propeller) (part BQ3285E_RTC)
      (fields
        (field (name Reference) U)
        (field (name Value) BQ3285E_RTC))
      (pins
        (pin (num 1) (name MOT) (type input))
        (pin (num 2) (name X1) (type input))
        (pin (num 3) (name X2) (type input))
        (pin (num 4) (name AD0) (type input))
        (pin (num 5) (name AD1) (type input))
        (pin (num 6) (name AD2) (type input))
        (pin (num 7) (name AD3) (type input))
        (pin (num 8) (name AD4) (type input))
        (pin (num 9) (name AD5) (type input))
        (pin (num 10) (name AD6) (type input))
        (pin (num 11) (name AD7) (type input))
        (pin (num 12) (name VSS) (type power_in))
        (pin (num 13) (name ~CS) (type input))
        (pin (num 14) (name AS) (type input))
        (pin (num 15) (name R/~W) (type input))
        (pin (num 16) (name VSS) (type input))
        (pin (num 17) (name DS) (type input))
        (pin (num 18) (name ~RST) (type input))
        (pin (num 19) (name ~INT) (type input))
        (pin (num 20) (name BC) (type input))
        (pin (num 21) (name ~RCL) (type input))
        (pin (num 22) (name EXTRAM) (type input))
        (pin (num 23) (name SQW) (type input))
        (pin (num 24) (name VCC) (type power_in))))
    (libpart (lib device) (part Battery)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (description "Connector 01x05")
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib conn) (part CONN_01X07)
      (description "Connector 01x07")
      (footprints
        (fp Pin_Header_Straight_1X07)
        (fp Pin_Header_Angled_1X07)
        (fp Socket_Strip_Straight_1X07)
        (fp Socket_Strip_Angled_1X07))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X07))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib conn) (part CONN_01X12)
      (description "Connector 01x12")
      (footprints
        (fp Pin_Header_Straight_1X12)
        (fp Pin_Header_Angled_1X12)
        (fp Socket_Strip_Straight_1X12)
        (fp Socket_Strip_Angled_1X12))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X12))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))))
    (libpart (lib conn) (part CONN_01X20)
      (description "Connector 01x20")
      (footprints
        (fp Pin_Header_Straight_1X20)
        (fp Pin_Header_Angled_1X20)
        (fp Socket_Strip_Straight_1X20)
        (fp Socket_Strip_Angled_1X20))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X20))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))))
    (libpart (lib conn) (part CONN_02X09)
      (description "Connector 02x09")
      (footprints
        (fp Pin_Header_Straight_2X09)
        (fp Pin_Header_Angled_2X09)
        (fp Socket_Strip_Straight_2X09)
        (fp Socket_Strip_Angled_2X09))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X09))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Polarised capacitor")
      (footprints
        (fp SMD*_Pol)
        (fp c_elec*)
        (fp C*elec)
        (fp TantalC*)
        (fp Elko*)
        (fp CP*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1_Small)
      (description "Polarised capacitor")
      (footprints
        (fp CP*)
        (fp Elko*)
        (fp TantalC*)
        (fp C*elec)
        (fp c_elec*)
        (fp SMD*_Pol))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal_Small)
      (description "Two pin crystal")
      (footprints
        (fp Crystal_))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib 6502) (part DECODER_JUMPERS)
      (fields
        (field (name Reference) JP)
        (field (name Value) DECODER_JUMPERS))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type input))
        (pin (num 7) (name ~) (type input))
        (pin (num 8) (name ~) (type input))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name ~) (type input))
        (pin (num 15) (name ~) (type input))))
    (libpart (lib propeller) (part DS1813_EconoReset)
      (fields
        (field (name Reference) U)
        (field (name Value) DS1813_EconoReset))
      (pins
        (pin (num 1) (name RST) (type input))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name GND) (type power_in))))
    (libpart (lib device) (part D_Schottky_Small)
      (description "Diode Schottky")
      (footprints
        (fp Diode_*)
        (fp D-Pak_TO252AA)
        (fp *SingleDiode)
        (fp *SingleDiode*)
        (fp *_Diode_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib 6502) (part ECS-2100X-1MHZ)
      (fields
        (field (name Reference) Y)
        (field (name Value) ECS-2100X-1MHZ))
      (pins
        (pin (num 1) (name GND) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name OUTPUT) (type output))
        (pin (num 8) (name +5V) (type power_in))))
    (libpart (lib propeller) (part FB)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) FB)
        (field (name Value) FB))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part JACK_2P)
      (fields
        (field (name Reference) J)
        (field (name Value) JACK_2P))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib device) (part JUMPER3)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER3))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib propeller) (part MIC29300-5.0WT)
      (fields
        (field (name Reference) U)
        (field (name Value) MIC29300-5.0WT))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type power_out))))
    (libpart (lib propeller) (part MIC29302)
      (fields
        (field (name Reference) U)
        (field (name Value) MIC29302))
      (pins
        (pin (num 1) (name EN) (type passive))
        (pin (num 2) (name IN) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name OUT) (type power_out))
        (pin (num 5) (name ADJ) (type passive))))
    (libpart (lib 6502Computer-rescue) (part PN2222A-RESCUE-6502Computer)
      (footprints
        (fp TO-92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) PN2222A-RESCUE-6502Computer)
        (field (name Footprint) TO-92))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib 6502) (part PROP_JUMPERS)
      (fields
        (field (name Reference) JP)
        (field (name Value) PROP_JUMPERS))
      (pins
        (pin (num 1) (name JP1) (type input))
        (pin (num 2) (name JP2) (type input))
        (pin (num 3) (name JP3) (type input))
        (pin (num 4) (name JP4) (type input))
        (pin (num 5) (name JP5) (type input))
        (pin (num 6) (name JP6) (type input))
        (pin (num 7) (name JP7) (type input))
        (pin (num 8) (name JP8) (type input))
        (pin (num 9) (name JP9) (type input))
        (pin (num 10) (name JP10) (type input))
        (pin (num 11) (name JP11) (type passive))
        (pin (num 12) (name JP12) (type passive))))
    (libpart (lib keyboard_parts) (part PS2_FEMALE)
      (fields
        (field (name Reference) K)
        (field (name Value) PS2_FEMALE))
      (pins
        (pin (num 1) (name DATA) (type input))
        (pin (num 3) (name GND) (type input))
        (pin (num 4) (name +5V) (type power_in))
        (pin (num 5) (name CLK) (type input))))
    (libpart (lib propeller) (part Prop_P8X32A)
      (fields
        (field (name Reference) U)
        (field (name Value) Prop_P8X32A))
      (pins
        (pin (num 1) (name P0) (type BiDi))
        (pin (num 2) (name P1) (type BiDi))
        (pin (num 3) (name P2) (type BiDi))
        (pin (num 4) (name P3) (type output))
        (pin (num 5) (name P4) (type input))
        (pin (num 6) (name P5) (type input))
        (pin (num 7) (name P6) (type input))
        (pin (num 8) (name P7) (type input))
        (pin (num 9) (name VSS) (type power_in))
        (pin (num 10) (name BOEn) (type input))
        (pin (num 11) (name RESn) (type input))
        (pin (num 12) (name VDD) (type power_in))
        (pin (num 13) (name P8) (type input))
        (pin (num 14) (name P9) (type input))
        (pin (num 15) (name P10) (type input))
        (pin (num 16) (name P11) (type input))
        (pin (num 17) (name P12) (type input))
        (pin (num 18) (name P13) (type input))
        (pin (num 19) (name P14) (type input))
        (pin (num 20) (name P15) (type input))
        (pin (num 21) (name P16) (type input))
        (pin (num 22) (name P17) (type input))
        (pin (num 23) (name P18) (type input))
        (pin (num 24) (name P19) (type input))
        (pin (num 25) (name P20) (type input))
        (pin (num 26) (name P21) (type input))
        (pin (num 27) (name P22) (type input))
        (pin (num 28) (name P23) (type input))
        (pin (num 29) (name VSS) (type power_in))
        (pin (num 30) (name XI) (type input))
        (pin (num 31) (name XO) (type input))
        (pin (num 32) (name VDD) (type power_in))
        (pin (num 33) (name P24) (type input))
        (pin (num 34) (name P25) (type input))
        (pin (num 35) (name P26) (type input))
        (pin (num 36) (name P27) (type input))
        (pin (num 37) (name P28) (type input))
        (pin (num 38) (name P29) (type input))
        (pin (num 39) (name P30) (type input))
        (pin (num 40) (name P31) (type input))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib 6502) (part RR7)
      (description "8 resistors")
      (fields
        (field (name Reference) RR)
        (field (name Value) RR7))
      (pins
        (pin (num 1) (name COM) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))))
    (libpart (lib propeller) (part SD_Card_SPI)
      (description "SD Card Reader")
      (docs http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf)
      (footprints
        (fp SD_Card_Receptacle))
      (fields
        (field (name Reference) CON)
        (field (name Value) SD_Card_SPI)
        (field (name Footprint) 10067847-001))
      (pins
        (pin (num 1) (name CS) (type input))
        (pin (num 2) (name DI) (type input))
        (pin (num 3) (name VSS) (type input))
        (pin (num 4) (name VDD) (type input))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type input))
        (pin (num 7) (name DO) (type input))
        (pin (num 8) (name DAT1) (type input))
        (pin (num 9) (name DAT2) (type input))))
    (libpart (lib 6502) (part SPST2)
      (description "Interrupteur simple")
      (fields
        (field (name Reference) SW)
        (field (name Value) SPST2))
      (pins
        (pin (num 2) (name 2) (type power_in))
        (pin (num 3) (name 3) (type power_out))))
    (libpart (lib 6502) (part SW_PUSH_SAFE)
      (description Button)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH_SAFE))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib propeller) (part TV_OUT)
      (fields
        (field (name Reference) J)
        (field (name Value) TV_OUT))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name IN) (type input))))
    (libpart (lib vga) (part VGA)
      (fields
        (field (name Reference) J)
        (field (name Value) VGA))
      (pins
        (pin (num 1) (name RED) (type input))
        (pin (num 2) (name GREEN) (type input))
        (pin (num 3) (name BLUE) (type input))
        (pin (num 4) (name ID2/RES) (type input))
        (pin (num 5) (name GND_HSYNC) (type input))
        (pin (num 6) (name RED_RTN) (type input))
        (pin (num 7) (name GREEN_RTN) (type input))
        (pin (num 8) (name BLUE_RTN) (type input))
        (pin (num 9) (name KEY/PWR) (type input))
        (pin (num 10) (name GND_VSYNC) (type input))
        (pin (num 11) (name ID0/RES) (type input))
        (pin (num 12) (name ID1/SDA) (type input))
        (pin (num 13) (name HSYNC) (type input))
        (pin (num 14) (name VSYNC) (type input))
        (pin (num 15) (name ID3/SCL) (type input)))))
  (libraries
    (library (logical 6502Computer-rescue)
      (uri "C:\\Users\\Stache\\Documents\\KiCad Projects\\6502Computer\\rev1.a\\6502Computer-rescue.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical propeller)
      (uri "C:\\Users\\Stache\\Documents\\KiCad Projects\\6502Computer\\rev1.a\\propeller.lib"))
    (library (logical vga)
      (uri "C:\\Users\\Stache\\Documents\\KiCad Projects\\6502Computer\\rev1.a\\vga.lib"))
    (library (logical keyboard_parts)
      (uri "C:\\Users\\Stache\\Documents\\KiCad Projects\\6502Computer\\rev1.a\\keyboard_parts.lib"))
    (library (logical addressdecoder)
      (uri "C:\\Users\\Stache\\Documents\\KiCad Projects\\AddressDecoderModule\\rev1.a\\addressdecoder.lib"))
    (library (logical 6502)
      (uri "C:\\Users\\Stache\\Documents\\KiCad Projects\\6502ioPrototypingBoardv1.2\\6502.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name +5V)
      (node (ref P16) (pin 6))
      (node (ref P16) (pin 5))
      (node (ref U14) (pin 6))
      (node (ref R30) (pin 1))
      (node (ref R28) (pin 2))
      (node (ref P16) (pin 4))
      (node (ref P10) (pin 2))
      (node (ref J5) (pin 9))
      (node (ref C16) (pin 2))
      (node (ref C32) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref U10) (pin 15))
      (node (ref U15) (pin 24))
      (node (ref U9) (pin 24))
      (node (ref U9) (pin 20))
      (node (ref U6) (pin 8))
      (node (ref LED1) (pin 2))
      (node (ref U11) (pin 24))
      (node (ref U11) (pin 20))
      (node (ref U8) (pin 28))
      (node (ref U3) (pin 1))
      (node (ref Y1) (pin 8))
      (node (ref U10) (pin 2))
      (node (ref U7) (pin 27))
      (node (ref U4) (pin 21))
      (node (ref U1) (pin 3))
      (node (ref U7) (pin 28))
      (node (ref U12) (pin 2))
      (node (ref Y2) (pin 8))
      (node (ref C2) (pin 1))
      (node (ref U12) (pin 15))
      (node (ref C1) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref P15) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref JP1) (pin 15))
      (node (ref U5) (pin 2))
      (node (ref P8) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref U14) (pin 16))
      (node (ref C37) (pin 1))
      (node (ref U16) (pin 14))
      (node (ref P9) (pin 2))
      (node (ref P8) (pin 17))
      (node (ref K1) (pin 4))
      (node (ref C17) (pin 1))
      (node (ref P6) (pin 17))
      (node (ref C19) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref FB2) (pin 1))
      (node (ref P10) (pin 17))
      (node (ref P6) (pin 2))
      (node (ref C39) (pin 1))
      (node (ref C22) (pin 2))
      (node (ref JP1) (pin 12))
      (node (ref JP1) (pin 9))
      (node (ref RR1) (pin 1))
      (node (ref JP1) (pin 6))
      (node (ref JP1) (pin 3))
      (node (ref P9) (pin 17))
      (node (ref C35) (pin 1))
      (node (ref P3) (pin 13))
      (node (ref C20) (pin 2)))
    (net (code 2) (name GND)
      (node (ref C20) (pin 1))
      (node (ref U10) (pin 9))
      (node (ref Y2) (pin 1))
      (node (ref U10) (pin 17))
      (node (ref C17) (pin 2))
      (node (ref Y2) (pin 4))
      (node (ref U10) (pin 16))
      (node (ref R12) (pin 2))
      (node (ref U10) (pin 1))
      (node (ref C37) (pin 2))
      (node (ref U9) (pin 1))
      (node (ref U8) (pin 14))
      (node (ref U12) (pin 17))
      (node (ref C33) (pin 2))
      (node (ref U11) (pin 1))
      (node (ref U15) (pin 12))
      (node (ref U15) (pin 16))
      (node (ref C13) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref U16) (pin 7))
      (node (ref P8) (pin 18))
      (node (ref P9) (pin 4))
      (node (ref P9) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref P10) (pin 4))
      (node (ref P10) (pin 1))
      (node (ref C23) (pin 2))
      (node (ref U14) (pin 8))
      (node (ref P9) (pin 15))
      (node (ref P9) (pin 18))
      (node (ref P6) (pin 18))
      (node (ref P8) (pin 1))
      (node (ref P8) (pin 4))
      (node (ref P10) (pin 15))
      (node (ref P6) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref P12) (pin 1))
      (node (ref P8) (pin 15))
      (node (ref C39) (pin 2))
      (node (ref P6) (pin 15))
      (node (ref P10) (pin 18))
      (node (ref P6) (pin 4))
      (node (ref U6) (pin 21))
      (node (ref U13) (pin 14))
      (node (ref U7) (pin 14))
      (node (ref R10) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U12) (pin 9))
      (node (ref U12) (pin 1))
      (node (ref Y1) (pin 4))
      (node (ref C24) (pin 2))
      (node (ref P15) (pin 5))
      (node (ref U12) (pin 16))
      (node (ref U4) (pin 20))
      (node (ref C9) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref SW3) (pin 1))
      (node (ref J5) (pin 5))
      (node (ref J5) (pin 6))
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref K1) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U18) (pin 2))
      (node (ref U18) (pin 3))
      (node (ref U3) (pin 2))
      (node (ref U18) (pin 4))
      (node (ref U18) (pin 7))
      (node (ref C7) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref J5) (pin 10))
      (node (ref J5) (pin 8))
      (node (ref J5) (pin 7))
      (node (ref JP1) (pin 10))
      (node (ref P16) (pin 11))
      (node (ref P16) (pin 12))
      (node (ref U2) (pin 3))
      (node (ref JP1) (pin 7))
      (node (ref JP1) (pin 4))
      (node (ref JP1) (pin 13))
      (node (ref JP1) (pin 1))
      (node (ref C43) (pin 1))
      (node (ref C40) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref P16) (pin 7))
      (node (ref P16) (pin 8))
      (node (ref P16) (pin 9))
      (node (ref P16) (pin 10))
      (node (ref U17) (pin 29))
      (node (ref C28) (pin 2))
      (node (ref U15) (pin 1))
      (node (ref C27) (pin 2))
      (node (ref P14) (pin 1))
      (node (ref CON1) (pin 6))
      (node (ref C41) (pin 1))
      (node (ref P4) (pin 20))
      (node (ref U17) (pin 9))
      (node (ref R3) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref C42) (pin 1))
      (node (ref CON1) (pin 3))
      (node (ref U18) (pin 1)))
    (net (code 3) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 5))
      (node (ref R2) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 4) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref SW1) (pin 2)))
    (net (code 5) (name CS7)
      (node (ref U4) (pin 39))
      (node (ref P1) (pin 1)))
    (net (code 6) (name OE)
      (node (ref U7) (pin 22))
      (node (ref U4) (pin 29))
      (node (ref U8) (pin 22)))
    (net (code 7) (name CS_RTC)
      (node (ref U14) (pin 5))
      (node (ref U14) (pin 4))
      (node (ref U15) (pin 13))
      (node (ref U4) (pin 38)))
    (net (code 8) (name WE)
      (node (ref U8) (pin 27))
      (node (ref U4) (pin 28)))
    (net (code 9) (name CS_SID)
      (node (ref U4) (pin 37))
      (node (ref U13) (pin 8)))
    (net (code 10) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 11) (name "Net-(JP1-Pad5)")
      (node (ref U4) (pin 6))
      (node (ref P1) (pin 4))
      (node (ref JP1) (pin 5)))
    (net (code 12) (name "Net-(JP1-Pad8)")
      (node (ref U4) (pin 5))
      (node (ref P1) (pin 5))
      (node (ref JP1) (pin 8)))
    (net (code 13) (name "Net-(JP1-Pad11)")
      (node (ref P1) (pin 6))
      (node (ref U4) (pin 4))
      (node (ref JP1) (pin 11)))
    (net (code 14) (name "Net-(JP1-Pad14)")
      (node (ref U4) (pin 3))
      (node (ref P1) (pin 7))
      (node (ref JP1) (pin 14)))
    (net (code 15) (name PHI2)
      (node (ref U6) (pin 39))
      (node (ref U4) (pin 2))
      (node (ref U14) (pin 1))
      (node (ref U13) (pin 6))
      (node (ref P4) (pin 2))
      (node (ref U9) (pin 25))
      (node (ref U11) (pin 25))
      (node (ref U10) (pin 27))
      (node (ref U12) (pin 27)))
    (net (code 16) (name "Net-(JP1-Pad2)")
      (node (ref JP1) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref U4) (pin 7)))
    (net (code 17) (name "Net-(LED1-Pad1)")
      (node (ref LED1) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 18) (name ROM_CE)
      (node (ref U4) (pin 27))
      (node (ref U7) (pin 20)))
    (net (code 19) (name CS_VIA2)
      (node (ref U11) (pin 23))
      (node (ref U4) (pin 36)))
    (net (code 20) (name RAM_CE)
      (node (ref U8) (pin 20))
      (node (ref U4) (pin 26)))
    (net (code 21) (name CS_VIA1)
      (node (ref U4) (pin 35))
      (node (ref U9) (pin 23)))
    (net (code 22) (name CS_ACIA2)
      (node (ref U4) (pin 34))
      (node (ref U12) (pin 3)))
    (net (code 23) (name CS_ACIA1)
      (node (ref U10) (pin 3))
      (node (ref U4) (pin 33)))
    (net (code 24) (name CS8)
      (node (ref P1) (pin 2))
      (node (ref U4) (pin 40)))
    (net (code 25) (name RW)
      (node (ref U10) (pin 28))
      (node (ref U14) (pin 2))
      (node (ref U9) (pin 22))
      (node (ref U12) (pin 28))
      (node (ref U11) (pin 22))
      (node (ref U6) (pin 34))
      (node (ref P4) (pin 7))
      (node (ref U4) (pin 8))
      (node (ref U13) (pin 7)))
    (net (code 26) (name +12V)
      (node (ref C6) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref C5) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref C36) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref FB3) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 27) (name +3V3)
      (node (ref P9) (pin 3))
      (node (ref CON1) (pin 4))
      (node (ref U3) (pin 3))
      (node (ref U18) (pin 8))
      (node (ref P8) (pin 16))
      (node (ref P6) (pin 3))
      (node (ref P10) (pin 3))
      (node (ref C42) (pin 2))
      (node (ref P6) (pin 16))
      (node (ref C9) (pin 1))
      (node (ref U17) (pin 10))
      (node (ref U17) (pin 32))
      (node (ref C43) (pin 2))
      (node (ref U17) (pin 12))
      (node (ref P16) (pin 3))
      (node (ref P16) (pin 2))
      (node (ref P16) (pin 1))
      (node (ref P9) (pin 16))
      (node (ref C8) (pin 1))
      (node (ref P15) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref P10) (pin 16))
      (node (ref P8) (pin 3))
      (node (ref C41) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref R27) (pin 1)))
    (net (code 28) (name "Net-(C3-Pad1)")
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref SW1) (pin 3)))
    (net (code 29) (name VPB)
      (node (ref P3) (pin 20))
      (node (ref U6) (pin 1)))
    (net (code 30) (name SYNC)
      (node (ref U6) (pin 7))
      (node (ref P3) (pin 14)))
    (net (code 31) (name NMI)
      (node (ref JP6) (pin 3))
      (node (ref JP5) (pin 3))
      (node (ref JP7) (pin 3))
      (node (ref RR1) (pin 6))
      (node (ref U6) (pin 6))
      (node (ref P3) (pin 15))
      (node (ref JP8) (pin 3))
      (node (ref JP4) (pin 3)))
    (net (code 32) (name MLB)
      (node (ref U6) (pin 5))
      (node (ref P3) (pin 16)))
    (net (code 33) (name IRQ)
      (node (ref P3) (pin 17))
      (node (ref JP8) (pin 1))
      (node (ref JP7) (pin 1))
      (node (ref U6) (pin 4))
      (node (ref JP6) (pin 1))
      (node (ref JP4) (pin 1))
      (node (ref JP5) (pin 1))
      (node (ref RR1) (pin 5)))
    (net (code 34) (name PHI1O)
      (node (ref U6) (pin 3))
      (node (ref P3) (pin 18)))
    (net (code 35) (name NC)
      (node (ref U6) (pin 35))
      (node (ref P4) (pin 6)))
    (net (code 36) (name BE)
      (node (ref U6) (pin 36))
      (node (ref P4) (pin 5))
      (node (ref RR1) (pin 3)))
    (net (code 37) (name CLOCK)
      (node (ref P4) (pin 4))
      (node (ref U6) (pin 37))
      (node (ref Y1) (pin 5)))
    (net (code 38) (name SOB)
      (node (ref P4) (pin 3))
      (node (ref RR1) (pin 2))
      (node (ref U6) (pin 38)))
    (net (code 39) (name RES)
      (node (ref U12) (pin 4))
      (node (ref U10) (pin 4))
      (node (ref RR1) (pin 7))
      (node (ref U11) (pin 34))
      (node (ref U15) (pin 18))
      (node (ref JP9) (pin 2))
      (node (ref U9) (pin 34))
      (node (ref SW2) (pin 4))
      (node (ref U5) (pin 1))
      (node (ref P4) (pin 1))
      (node (ref U6) (pin 40))
      (node (ref U13) (pin 5)))
    (net (code 40) (name RDY)
      (node (ref RR1) (pin 4))
      (node (ref U6) (pin 2))
      (node (ref P3) (pin 19)))
    (net (code 41) (name "Net-(FB1-Pad1)")
      (node (ref R11) (pin 2))
      (node (ref FB1) (pin 1)))
    (net (code 42) (name AUDIO_OUT)
      (node (ref J3) (pin 2))
      (node (ref J2) (pin 3))
      (node (ref J2) (pin 2))
      (node (ref P12) (pin 2))
      (node (ref C38) (pin 2)))
    (net (code 43) (name "Net-(U14-Pad7)")
      (node (ref U14) (pin 7))
      (node (ref U15) (pin 17)))
    (net (code 44) (name "Net-(U14-Pad9)")
      (node (ref U14) (pin 9)))
    (net (code 45) (name "Net-(U14-Pad10)")
      (node (ref U14) (pin 10))
      (node (ref U15) (pin 15)))
    (net (code 46) (name "Net-(U14-Pad11)")
      (node (ref U14) (pin 11)))
    (net (code 47) (name "Net-(U14-Pad12)")
      (node (ref U14) (pin 12)))
    (net (code 48) (name "Net-(U15-Pad14)")
      (node (ref U15) (pin 14))
      (node (ref U16) (pin 3)))
    (net (code 49) (name "Net-(U14-Pad15)")
      (node (ref U14) (pin 15)))
    (net (code 50) (name "Net-(U14-Pad13)")
      (node (ref U14) (pin 13)))
    (net (code 51) (name "Net-(U10-Pad7)")
      (node (ref U10) (pin 7)))
    (net (code 52) (name "Net-(U12-Pad7)")
      (node (ref U12) (pin 7)))
    (net (code 53) (name "Net-(P5-Pad5)")
      (node (ref U10) (pin 8))
      (node (ref P5) (pin 5)))
    (net (code 54) (name "Net-(P5-Pad2)")
      (node (ref P5) (pin 2))
      (node (ref U10) (pin 5)))
    (net (code 55) (name "Net-(P5-Pad4)")
      (node (ref P5) (pin 4))
      (node (ref U10) (pin 11)))
    (net (code 56) (name "Net-(P7-Pad2)")
      (node (ref U12) (pin 5))
      (node (ref P7) (pin 2)))
    (net (code 57) (name "Net-(P7-Pad4)")
      (node (ref U12) (pin 11))
      (node (ref P7) (pin 4)))
    (net (code 58) (name "Net-(P7-Pad5)")
      (node (ref U12) (pin 8))
      (node (ref P7) (pin 5)))
    (net (code 59) (name "Net-(P11-Pad3)")
      (node (ref P11) (pin 3))
      (node (ref U15) (pin 21)))
    (net (code 60) (name "Net-(P11-Pad2)")
      (node (ref P11) (pin 2))
      (node (ref U15) (pin 22)))
    (net (code 61) (name "Net-(P11-Pad1)")
      (node (ref P11) (pin 1))
      (node (ref U15) (pin 23)))
    (net (code 62) (name "Net-(JP8-Pad2)")
      (node (ref U15) (pin 19))
      (node (ref JP8) (pin 2)))
    (net (code 63) (name "Net-(D1-Pad1)")
      (node (ref U9) (pin 21))
      (node (ref D1) (pin 1)))
    (net (code 64) (name "Net-(D2-Pad1)")
      (node (ref U11) (pin 21))
      (node (ref D2) (pin 1)))
    (net (code 65) (name "Net-(BT1-Pad1)")
      (node (ref BT1) (pin 1))
      (node (ref U15) (pin 20)))
    (net (code 66) (name "Net-(C27-Pad1)")
      (node (ref C27) (pin 1))
      (node (ref U13) (pin 26)))
    (net (code 67) (name "Net-(C28-Pad1)")
      (node (ref C28) (pin 1))
      (node (ref U13) (pin 24)))
    (net (code 68) (name "Net-(C30-Pad1)")
      (node (ref U13) (pin 23))
      (node (ref C30) (pin 1)))
    (net (code 69) (name "Net-(C23-Pad1)")
      (node (ref C23) (pin 1))
      (node (ref U15) (pin 2))
      (node (ref Y3) (pin 1)))
    (net (code 70) (name "Net-(C24-Pad1)")
      (node (ref Y3) (pin 2))
      (node (ref U15) (pin 3))
      (node (ref C24) (pin 1)))
    (net (code 71) (name ACIA2_RX)
      (node (ref P7) (pin 3))
      (node (ref JP9) (pin 12))
      (node (ref P15) (pin 3))
      (node (ref U12) (pin 12)))
    (net (code 72) (name ACIA2_TX)
      (node (ref JP9) (pin 10))
      (node (ref P7) (pin 1))
      (node (ref P15) (pin 4))
      (node (ref U12) (pin 10)))
    (net (code 73) (name ACIA1_TX)
      (node (ref U10) (pin 10))
      (node (ref P5) (pin 1))
      (node (ref U17) (pin 34)))
    (net (code 74) (name ACIA1_RX)
      (node (ref U10) (pin 12))
      (node (ref P5) (pin 3))
      (node (ref U17) (pin 33)))
    (net (code 75) (name "Net-(C38-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref C38) (pin 1)))
    (net (code 76) (name "Net-(U14-Pad14)")
      (node (ref U14) (pin 14))
      (node (ref U16) (pin 2))
      (node (ref U16) (pin 1)))
    (net (code 77) (name "Net-(C26-Pad2)")
      (node (ref U13) (pin 4))
      (node (ref C26) (pin 2)))
    (net (code 78) (name "Net-(C26-Pad1)")
      (node (ref U13) (pin 3))
      (node (ref C26) (pin 1)))
    (net (code 79) (name "Net-(C25-Pad2)")
      (node (ref U13) (pin 2))
      (node (ref C25) (pin 2)))
    (net (code 80) (name "Net-(C25-Pad1)")
      (node (ref C25) (pin 1))
      (node (ref U13) (pin 1)))
    (net (code 81) (name "Net-(U10-Pad6)")
      (node (ref U10) (pin 6))
      (node (ref Y2) (pin 5))
      (node (ref U12) (pin 6)))
    (net (code 82) (name "Net-(JP4-Pad2)")
      (node (ref U10) (pin 26))
      (node (ref JP4) (pin 2)))
    (net (code 83) (name "Net-(JP6-Pad2)")
      (node (ref U12) (pin 26))
      (node (ref JP6) (pin 2)))
    (net (code 84) (name "Net-(C33-Pad1)")
      (node (ref C33) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 85) (name "Net-(FB1-Pad2)")
      (node (ref R10) (pin 2))
      (node (ref FB1) (pin 2))
      (node (ref U13) (pin 27)))
    (net (code 86) (name VIA2_PB6)
      (node (ref U11) (pin 16))
      (node (ref P9) (pin 13)))
    (net (code 87) (name VIA2_PB7)
      (node (ref P9) (pin 14))
      (node (ref U11) (pin 17)))
    (net (code 88) (name VIA2_CB1)
      (node (ref P9) (pin 5))
      (node (ref U11) (pin 18)))
    (net (code 89) (name VIA2_CB2)
      (node (ref P9) (pin 6))
      (node (ref U11) (pin 19)))
    (net (code 90) (name VIA2_CA2)
      (node (ref U11) (pin 39))
      (node (ref P10) (pin 6)))
    (net (code 91) (name VIA1_PA0)
      (node (ref P6) (pin 7))
      (node (ref U9) (pin 2)))
    (net (code 92) (name VIA1_PA1)
      (node (ref P6) (pin 8))
      (node (ref U9) (pin 3)))
    (net (code 93) (name VIA1_PA2)
      (node (ref U9) (pin 4))
      (node (ref P6) (pin 9)))
    (net (code 94) (name VIA1_CB2)
      (node (ref P8) (pin 6))
      (node (ref U9) (pin 19)))
    (net (code 95) (name VIA1_CA2)
      (node (ref P6) (pin 6))
      (node (ref U9) (pin 39)))
    (net (code 96) (name VIA2_PA0)
      (node (ref U11) (pin 2))
      (node (ref P10) (pin 7)))
    (net (code 97) (name VIA2_PA1)
      (node (ref U11) (pin 3))
      (node (ref P10) (pin 8)))
    (net (code 98) (name VIA2_PA2)
      (node (ref U11) (pin 4))
      (node (ref P10) (pin 9)))
    (net (code 99) (name VIA2_PA3)
      (node (ref U11) (pin 5))
      (node (ref P10) (pin 10)))
    (net (code 100) (name VIA2_PA4)
      (node (ref P10) (pin 11))
      (node (ref U11) (pin 6)))
    (net (code 101) (name VIA2_PA5)
      (node (ref U11) (pin 7))
      (node (ref P10) (pin 12)))
    (net (code 102) (name VIA2_PA6)
      (node (ref U11) (pin 8))
      (node (ref P10) (pin 13)))
    (net (code 103) (name VIA2_PA7)
      (node (ref U11) (pin 9))
      (node (ref P10) (pin 14)))
    (net (code 104) (name VIA2_PB0)
      (node (ref U11) (pin 10))
      (node (ref P9) (pin 7)))
    (net (code 105) (name VIA2_CA1)
      (node (ref U11) (pin 40))
      (node (ref P10) (pin 5)))
    (net (code 106) (name VIA2_PB1)
      (node (ref P9) (pin 8))
      (node (ref U11) (pin 11)))
    (net (code 107) (name VIA2_PB2)
      (node (ref P9) (pin 9))
      (node (ref U11) (pin 12)))
    (net (code 108) (name VIA2_PB3)
      (node (ref U11) (pin 13))
      (node (ref P9) (pin 10)))
    (net (code 109) (name VIA2_PB4)
      (node (ref U11) (pin 14))
      (node (ref P9) (pin 11)))
    (net (code 110) (name VIA2_PB5)
      (node (ref U11) (pin 15))
      (node (ref P9) (pin 12)))
    (net (code 111) (name VIA1_PB3)
      (node (ref P8) (pin 10))
      (node (ref U9) (pin 13)))
    (net (code 112) (name VIA1_PA3)
      (node (ref U9) (pin 5))
      (node (ref P6) (pin 10)))
    (net (code 113) (name VIA1_PA4)
      (node (ref U9) (pin 6))
      (node (ref P6) (pin 11)))
    (net (code 114) (name VIA1_PA5)
      (node (ref P6) (pin 12))
      (node (ref U9) (pin 7)))
    (net (code 115) (name VIA1_PA6)
      (node (ref U9) (pin 8))
      (node (ref P6) (pin 13)))
    (net (code 116) (name VIA1_PA7)
      (node (ref P6) (pin 14))
      (node (ref U9) (pin 9)))
    (net (code 117) (name VIA1_PB0)
      (node (ref U9) (pin 10))
      (node (ref P8) (pin 7)))
    (net (code 118) (name VIA1_CA1)
      (node (ref P6) (pin 5))
      (node (ref U9) (pin 40)))
    (net (code 119) (name VIA1_PB1)
      (node (ref P8) (pin 8))
      (node (ref U9) (pin 11)))
    (net (code 120) (name VIA1_PB2)
      (node (ref P8) (pin 9))
      (node (ref U9) (pin 12)))
    (net (code 121) (name "Net-(D2-Pad2)")
      (node (ref JP7) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 122) (name VIA1_PB4)
      (node (ref P8) (pin 11))
      (node (ref U9) (pin 14)))
    (net (code 123) (name VIA1_PB5)
      (node (ref U9) (pin 15))
      (node (ref P8) (pin 12)))
    (net (code 124) (name VIA1_PB6)
      (node (ref U9) (pin 16))
      (node (ref P8) (pin 13)))
    (net (code 125) (name VIA1_PB7)
      (node (ref U9) (pin 17))
      (node (ref P8) (pin 14)))
    (net (code 126) (name VIA1_CB1)
      (node (ref U9) (pin 18))
      (node (ref P8) (pin 5)))
    (net (code 127) (name "Net-(C31-Pad1)")
      (node (ref U13) (pin 28))
      (node (ref C31) (pin 1))
      (node (ref FB3) (pin 2)))
    (net (code 128) (name "Net-(C29-Pad1)")
      (node (ref U13) (pin 25))
      (node (ref FB2) (pin 2))
      (node (ref C29) (pin 1)))
    (net (code 129) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref JP5) (pin 2)))
    (net (code 130) (name "Net-(P13-Pad5)")
      (node (ref U17) (pin 16))
      (node (ref P13) (pin 5)))
    (net (code 131) (name "Net-(P13-Pad11)")
      (node (ref U17) (pin 6))
      (node (ref P13) (pin 11)))
    (net (code 132) (name "Net-(P13-Pad1)")
      (node (ref P13) (pin 1))
      (node (ref U17) (pin 20)))
    (net (code 133) (name "Net-(P13-Pad2)")
      (node (ref U17) (pin 19))
      (node (ref P13) (pin 2)))
    (net (code 134) (name "Net-(P13-Pad3)")
      (node (ref U17) (pin 18))
      (node (ref P13) (pin 3)))
    (net (code 135) (name "Net-(P13-Pad4)")
      (node (ref U17) (pin 17))
      (node (ref P13) (pin 4)))
    (net (code 136) (name "Net-(R20-Pad2)")
      (node (ref R20) (pin 2))
      (node (ref U17) (pin 35)))
    (net (code 137) (name "Net-(R19-Pad2)")
      (node (ref U17) (pin 36))
      (node (ref R19) (pin 2)))
    (net (code 138) (name "Net-(R24-Pad2)")
      (node (ref R24) (pin 2))
      (node (ref U17) (pin 27)))
    (net (code 139) (name "Net-(R23-Pad2)")
      (node (ref R23) (pin 2))
      (node (ref U17) (pin 28)))
    (net (code 140) (name "Net-(R22-Pad2)")
      (node (ref U17) (pin 25))
      (node (ref R22) (pin 2)))
    (net (code 141) (name "Net-(CON1-Pad7)")
      (node (ref U17) (pin 1))
      (node (ref CON1) (pin 7)))
    (net (code 142) (name "Net-(CON1-Pad1)")
      (node (ref U17) (pin 4))
      (node (ref CON1) (pin 1)))
    (net (code 143) (name "Net-(CON1-Pad2)")
      (node (ref U17) (pin 3))
      (node (ref CON1) (pin 2)))
    (net (code 144) (name "Net-(CON1-Pad5)")
      (node (ref CON1) (pin 5))
      (node (ref U17) (pin 2)))
    (net (code 145) (name "Net-(CON1-Pad9)")
      (node (ref CON1) (pin 9)))
    (net (code 146) (name "Net-(CON1-Pad8)")
      (node (ref CON1) (pin 8)))
    (net (code 147) (name "Net-(JP9-Pad4)")
      (node (ref JP9) (pin 4))
      (node (ref R13) (pin 1)))
    (net (code 148) (name "Net-(JP9-Pad5)")
      (node (ref JP9) (pin 5))
      (node (ref U17) (pin 8))
      (node (ref P13) (pin 9)))
    (net (code 149) (name "Net-(JP9-Pad3)")
      (node (ref JP9) (pin 3))
      (node (ref P13) (pin 10))
      (node (ref U17) (pin 7)))
    (net (code 150) (name "Net-(JP9-Pad8)")
      (node (ref R15) (pin 1))
      (node (ref JP9) (pin 8)))
    (net (code 151) (name "Net-(JP9-Pad7)")
      (node (ref U17) (pin 13))
      (node (ref JP9) (pin 7))
      (node (ref P13) (pin 8)))
    (net (code 152) (name "Net-(JP9-Pad6)")
      (node (ref JP9) (pin 6))
      (node (ref R14) (pin 1)))
    (net (code 153) (name "Net-(JP9-Pad1)")
      (node (ref P13) (pin 12))
      (node (ref JP9) (pin 1))
      (node (ref U17) (pin 5)))
    (net (code 154) (name "Net-(J5-Pad11)")
      (node (ref J5) (pin 11)))
    (net (code 155) (name "Net-(J5-Pad12)")
      (node (ref J5) (pin 12)))
    (net (code 156) (name "Net-(J5-Pad15)")
      (node (ref J5) (pin 15)))
    (net (code 157) (name "Net-(J5-Pad4)")
      (node (ref J5) (pin 4)))
    (net (code 158) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R14) (pin 2)))
    (net (code 159) (name "Net-(JP9-Pad11)")
      (node (ref P13) (pin 6))
      (node (ref JP9) (pin 11))
      (node (ref U17) (pin 15)))
    (net (code 160) (name "Net-(JP9-Pad9)")
      (node (ref U17) (pin 14))
      (node (ref JP9) (pin 9))
      (node (ref P13) (pin 7)))
    (net (code 161) (name "Net-(R29-Pad2)")
      (node (ref R29) (pin 2))
      (node (ref U18) (pin 5))
      (node (ref U17) (pin 38)))
    (net (code 162) (name "Net-(R27-Pad2)")
      (node (ref U18) (pin 6))
      (node (ref U17) (pin 37))
      (node (ref R27) (pin 2)))
    (net (code 163) (name "Net-(P14-Pad4)")
      (node (ref P14) (pin 4))
      (node (ref U17) (pin 39)))
    (net (code 164) (name "Net-(R21-Pad2)")
      (node (ref R21) (pin 2))
      (node (ref U17) (pin 26)))
    (net (code 165) (name "Net-(U17-Pad30)")
      (node (ref U17) (pin 30))
      (node (ref Y4) (pin 1)))
    (net (code 166) (name "Net-(U17-Pad31)")
      (node (ref U17) (pin 31))
      (node (ref Y4) (pin 2)))
    (net (code 167) (name "Net-(K1-Pad1)")
      (node (ref K1) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref R30) (pin 2)))
    (net (code 168) (name "Net-(J5-Pad2)")
      (node (ref J5) (pin 2))
      (node (ref R21) (pin 1))
      (node (ref R22) (pin 1)))
    (net (code 169) (name "Net-(J5-Pad1)")
      (node (ref R23) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref R24) (pin 1)))
    (net (code 170) (name "Net-(R18-Pad1)")
      (node (ref U17) (pin 21))
      (node (ref R18) (pin 1)))
    (net (code 171) (name "Net-(K1-Pad5)")
      (node (ref K1) (pin 5))
      (node (ref R28) (pin 1))
      (node (ref R19) (pin 1)))
    (net (code 172) (name "Net-(R26-Pad2)")
      (node (ref R26) (pin 2))
      (node (ref U17) (pin 23)))
    (net (code 173) (name "Net-(R25-Pad2)")
      (node (ref R25) (pin 2))
      (node (ref U17) (pin 24)))
    (net (code 174) (name "Net-(J5-Pad3)")
      (node (ref R26) (pin 1))
      (node (ref J5) (pin 3))
      (node (ref R25) (pin 1)))
    (net (code 175) (name "Net-(R17-Pad1)")
      (node (ref U17) (pin 22))
      (node (ref R17) (pin 1)))
    (net (code 176) (name "Net-(J5-Pad13)")
      (node (ref R17) (pin 2))
      (node (ref J5) (pin 13)))
    (net (code 177) (name "Net-(P14-Pad3)")
      (node (ref P14) (pin 3))
      (node (ref U17) (pin 40)))
    (net (code 178) (name "Net-(P14-Pad2)")
      (node (ref R16) (pin 2))
      (node (ref P14) (pin 2))
      (node (ref U17) (pin 11))
      (node (ref SW3) (pin 4)))
    (net (code 179) (name "Net-(J5-Pad14)")
      (node (ref J5) (pin 14))
      (node (ref R18) (pin 2)))
    (net (code 180) (name "/page 2/D6")
      (node (ref U15) (pin 10))
      (node (ref U12) (pin 24))
      (node (ref U8) (pin 18))
      (node (ref U11) (pin 27))
      (node (ref U10) (pin 24))
      (node (ref U13) (pin 21))
      (node (ref U6) (pin 27))
      (node (ref P4) (pin 14))
      (node (ref U7) (pin 18))
      (node (ref U9) (pin 27)))
    (net (code 181) (name "/page 1/A10")
      (node (ref P3) (pin 2))
      (node (ref U4) (pin 18))
      (node (ref U7) (pin 21))
      (node (ref U8) (pin 21))
      (node (ref U6) (pin 19)))
    (net (code 182) (name "/page 1/A11")
      (node (ref U8) (pin 23))
      (node (ref U7) (pin 23))
      (node (ref U6) (pin 20))
      (node (ref P3) (pin 1))
      (node (ref U4) (pin 19)))
    (net (code 183) (name "/page 1/A12")
      (node (ref U7) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref U4) (pin 22))
      (node (ref U6) (pin 22))
      (node (ref P4) (pin 19)))
    (net (code 184) (name "/page 1/A13")
      (node (ref U8) (pin 26))
      (node (ref U7) (pin 26))
      (node (ref U4) (pin 23))
      (node (ref P4) (pin 18))
      (node (ref U6) (pin 23)))
    (net (code 185) (name "/page 1/A14")
      (node (ref U6) (pin 24))
      (node (ref U8) (pin 1))
      (node (ref U4) (pin 24))
      (node (ref P4) (pin 17))
      (node (ref U7) (pin 1)))
    (net (code 186) (name "/page 1/A15")
      (node (ref P4) (pin 16))
      (node (ref U6) (pin 25))
      (node (ref U4) (pin 25)))
    (net (code 187) (name "/page 2/D0")
      (node (ref P4) (pin 8))
      (node (ref U8) (pin 11))
      (node (ref U13) (pin 15))
      (node (ref U7) (pin 11))
      (node (ref U12) (pin 18))
      (node (ref U10) (pin 18))
      (node (ref U9) (pin 33))
      (node (ref U15) (pin 4))
      (node (ref U6) (pin 33))
      (node (ref U11) (pin 33)))
    (net (code 188) (name "/page 2/D1")
      (node (ref U11) (pin 32))
      (node (ref P4) (pin 9))
      (node (ref U6) (pin 32))
      (node (ref U12) (pin 19))
      (node (ref U15) (pin 5))
      (node (ref U9) (pin 32))
      (node (ref U8) (pin 12))
      (node (ref U10) (pin 19))
      (node (ref U7) (pin 12))
      (node (ref U13) (pin 16)))
    (net (code 189) (name "/page 2/D2")
      (node (ref U11) (pin 31))
      (node (ref U13) (pin 17))
      (node (ref U6) (pin 31))
      (node (ref U7) (pin 13))
      (node (ref U8) (pin 13))
      (node (ref U9) (pin 31))
      (node (ref U15) (pin 6))
      (node (ref P4) (pin 10))
      (node (ref U12) (pin 20))
      (node (ref U10) (pin 20)))
    (net (code 190) (name "/page 2/D3")
      (node (ref U13) (pin 18))
      (node (ref U6) (pin 30))
      (node (ref U7) (pin 15))
      (node (ref U9) (pin 30))
      (node (ref U12) (pin 21))
      (node (ref U8) (pin 15))
      (node (ref U11) (pin 30))
      (node (ref U15) (pin 7))
      (node (ref P4) (pin 11))
      (node (ref U10) (pin 21)))
    (net (code 191) (name "/page 2/D4")
      (node (ref U10) (pin 22))
      (node (ref U11) (pin 29))
      (node (ref U7) (pin 16))
      (node (ref U9) (pin 29))
      (node (ref U8) (pin 16))
      (node (ref U13) (pin 19))
      (node (ref U15) (pin 8))
      (node (ref U6) (pin 29))
      (node (ref P4) (pin 12))
      (node (ref U12) (pin 22)))
    (net (code 192) (name "/page 2/D5")
      (node (ref U9) (pin 28))
      (node (ref U12) (pin 23))
      (node (ref U15) (pin 9))
      (node (ref P4) (pin 13))
      (node (ref U10) (pin 23))
      (node (ref U11) (pin 28))
      (node (ref U7) (pin 17))
      (node (ref U8) (pin 17))
      (node (ref U6) (pin 28))
      (node (ref U13) (pin 20)))
    (net (code 193) (name A1)
      (node (ref U8) (pin 9))
      (node (ref U7) (pin 9))
      (node (ref U6) (pin 10))
      (node (ref U10) (pin 14))
      (node (ref U9) (pin 37))
      (node (ref U13) (pin 10))
      (node (ref P3) (pin 11))
      (node (ref U12) (pin 14))
      (node (ref U11) (pin 37)))
    (net (code 194) (name "/page 2/D7")
      (node (ref U9) (pin 26))
      (node (ref U15) (pin 11))
      (node (ref P4) (pin 15))
      (node (ref U13) (pin 22))
      (node (ref U10) (pin 25))
      (node (ref U8) (pin 19))
      (node (ref U11) (pin 26))
      (node (ref U6) (pin 26))
      (node (ref U7) (pin 19))
      (node (ref U12) (pin 25)))
    (net (code 195) (name A0)
      (node (ref U14) (pin 3))
      (node (ref U11) (pin 38))
      (node (ref U6) (pin 9))
      (node (ref U13) (pin 9))
      (node (ref U7) (pin 10))
      (node (ref P3) (pin 12))
      (node (ref U12) (pin 13))
      (node (ref U10) (pin 13))
      (node (ref U8) (pin 10))
      (node (ref U9) (pin 38)))
    (net (code 196) (name "/page 1/A8")
      (node (ref U6) (pin 17))
      (node (ref U7) (pin 25))
      (node (ref P3) (pin 4))
      (node (ref U4) (pin 16))
      (node (ref U8) (pin 25)))
    (net (code 197) (name "/page 1/A9")
      (node (ref U8) (pin 24))
      (node (ref U4) (pin 17))
      (node (ref U6) (pin 18))
      (node (ref U7) (pin 24))
      (node (ref P3) (pin 3)))
    (net (code 198) (name A2)
      (node (ref P3) (pin 10))
      (node (ref U7) (pin 8))
      (node (ref U9) (pin 36))
      (node (ref U8) (pin 8))
      (node (ref U11) (pin 36))
      (node (ref U6) (pin 11))
      (node (ref U13) (pin 11)))
    (net (code 199) (name A3)
      (node (ref U9) (pin 35))
      (node (ref U11) (pin 35))
      (node (ref U8) (pin 7))
      (node (ref U13) (pin 12))
      (node (ref U6) (pin 12))
      (node (ref P3) (pin 9))
      (node (ref U7) (pin 7)))
    (net (code 200) (name A4)
      (node (ref U8) (pin 6))
      (node (ref U6) (pin 13))
      (node (ref U7) (pin 6))
      (node (ref U4) (pin 12))
      (node (ref P3) (pin 8))
      (node (ref U13) (pin 13)))
    (net (code 201) (name "/page 1/A5")
      (node (ref U4) (pin 13))
      (node (ref U8) (pin 5))
      (node (ref U6) (pin 14))
      (node (ref U7) (pin 5))
      (node (ref P3) (pin 7)))
    (net (code 202) (name "/page 1/A6")
      (node (ref U8) (pin 4))
      (node (ref U6) (pin 15))
      (node (ref P3) (pin 6))
      (node (ref U7) (pin 4))
      (node (ref U4) (pin 14)))
    (net (code 203) (name "/page 1/A7")
      (node (ref U6) (pin 16))
      (node (ref P3) (pin 5))
      (node (ref U7) (pin 3))
      (node (ref U4) (pin 15))
      (node (ref U8) (pin 3)))))