(module crystal_tc-38 (layer F.Cu)
  (descr "Crystal, TC-38")
  (tags QUARTZ)
  (autoplace_cost180 10)
  (clearance 0.2)
  (fp_text reference TC-38 (at 0 -2.6) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_text value X*** (at 0 2.5) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_circle (center 0 0) (end -1.6 0) (layer F.SilkS) (width 0.254))
  (pad 1 thru_hole circle (at -0.55 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 0.55 0) (size 0.7 0.7) (drill 0.35) (layers *.Cu *.Mask F.SilkS))
  (model walter/crystal/crystal_tc-38.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
