(module crystal_tc-26_horiz (layer F.Cu)
  (descr "Crystal, TC-26, horizontal")
  (tags QUARTZ)
  (autoplace_cost180 10)
  (clearance 0.2)
  (fp_text reference TC-26_Horiz (at 0 -4.3) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_text value X*** (at 0 5.3) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.2)))
  )
  (fp_line (start -1 -2.7) (end -1 3.3) (layer F.SilkS) (width 0.254))
  (fp_line (start -1 -2.7) (end 1 -2.7) (layer F.SilkS) (width 0.254))
  (fp_line (start 1 -2.7) (end 1 3.3) (layer F.SilkS) (width 0.254))
  (fp_line (start -1 3.3) (end 1 3.3) (layer F.SilkS) (width 0.254))
  (pad 1 thru_hole oval (at -0.35 -3.17) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 0.35 -3.17) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask F.SilkS))
  (pad "" smd rect (at 0 3.3) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (model walter/crystal/crystal_tc-26_horiz.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
