(edif REFB
  (edifVersion 2 0 0)
  (edifLevel 0)
  (keywordMap (keywordLevel 0))
  (status
    (written
      (timestamp 2023 9 20 4 45 58)
      (program "SCUBA" (version "Diamond (64-bit) 3.12.1.454"))))
      (comment "C:\lscc\diamond\3.12\ispfpga\bin\nt64\scuba.exe -w -n REFB -lang verilog -synth synplify -bus_exp 7 -bb -type efb -arch xo2c00 -freq 14.4 -ufm -ufm_ebr 190 -mem_size 321 -memfile ../RAM2E-LCMXO2.mem -memformat hex -wb -dev 1200 ")
  (library ORCLIB
    (edifLevel 0)
    (technology
      (numberDefinition))
    (cell VHI
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port Z
            (direction OUTPUT)))))
    (cell VLO
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port Z
            (direction OUTPUT)))))
    (cell EFB
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port WBCLKI
            (direction INPUT))
          (port WBRSTI
            (direction INPUT))
          (port WBCYCI
            (direction INPUT))
          (port WBSTBI
            (direction INPUT))
          (port WBWEI
            (direction INPUT))
          (port WBADRI7
            (direction INPUT))
          (port WBADRI6
            (direction INPUT))
          (port WBADRI5
            (direction INPUT))
          (port WBADRI4
            (direction INPUT))
          (port WBADRI3
            (direction INPUT))
          (port WBADRI2
            (direction INPUT))
          (port WBADRI1
            (direction INPUT))
          (port WBADRI0
            (direction INPUT))
          (port WBDATI7
            (direction INPUT))
          (port WBDATI6
            (direction INPUT))
          (port WBDATI5
            (direction INPUT))
          (port WBDATI4
            (direction INPUT))
          (port WBDATI3
            (direction INPUT))
          (port WBDATI2
            (direction INPUT))
          (port WBDATI1
            (direction INPUT))
          (port WBDATI0
            (direction INPUT))
          (port PLL0DATI7
            (direction INPUT))
          (port PLL0DATI6
            (direction INPUT))
          (port PLL0DATI5
            (direction INPUT))
          (port PLL0DATI4
            (direction INPUT))
          (port PLL0DATI3
            (direction INPUT))
          (port PLL0DATI2
            (direction INPUT))
          (port PLL0DATI1
            (direction INPUT))
          (port PLL0DATI0
            (direction INPUT))
          (port PLL0ACKI
            (direction INPUT))
          (port PLL1DATI7
            (direction INPUT))
          (port PLL1DATI6
            (direction INPUT))
          (port PLL1DATI5
            (direction INPUT))
          (port PLL1DATI4
            (direction INPUT))
          (port PLL1DATI3
            (direction INPUT))
          (port PLL1DATI2
            (direction INPUT))
          (port PLL1DATI1
            (direction INPUT))
          (port PLL1DATI0
            (direction INPUT))
          (port PLL1ACKI
            (direction INPUT))
          (port I2C1SCLI
            (direction INPUT))
          (port I2C1SDAI
            (direction INPUT))
          (port I2C2SCLI
            (direction INPUT))
          (port I2C2SDAI
            (direction INPUT))
          (port SPISCKI
            (direction INPUT))
          (port SPIMISOI
            (direction INPUT))
          (port SPIMOSII
            (direction INPUT))
          (port SPISCSN
            (direction INPUT))
          (port TCCLKI
            (direction INPUT))
          (port TCRSTN
            (direction INPUT))
          (port TCIC
            (direction INPUT))
          (port UFMSN
            (direction INPUT))
          (port WBDATO7
            (direction OUTPUT))
          (port WBDATO6
            (direction OUTPUT))
          (port WBDATO5
            (direction OUTPUT))
          (port WBDATO4
            (direction OUTPUT))
          (port WBDATO3
            (direction OUTPUT))
          (port WBDATO2
            (direction OUTPUT))
          (port WBDATO1
            (direction OUTPUT))
          (port WBDATO0
            (direction OUTPUT))
          (port WBACKO
            (direction OUTPUT))
          (port PLLCLKO
            (direction OUTPUT))
          (port PLLRSTO
            (direction OUTPUT))
          (port PLL0STBO
            (direction OUTPUT))
          (port PLL1STBO
            (direction OUTPUT))
          (port PLLWEO
            (direction OUTPUT))
          (port PLLADRO4
            (direction OUTPUT))
          (port PLLADRO3
            (direction OUTPUT))
          (port PLLADRO2
            (direction OUTPUT))
          (port PLLADRO1
            (direction OUTPUT))
          (port PLLADRO0
            (direction OUTPUT))
          (port PLLDATO7
            (direction OUTPUT))
          (port PLLDATO6
            (direction OUTPUT))
          (port PLLDATO5
            (direction OUTPUT))
          (port PLLDATO4
            (direction OUTPUT))
          (port PLLDATO3
            (direction OUTPUT))
          (port PLLDATO2
            (direction OUTPUT))
          (port PLLDATO1
            (direction OUTPUT))
          (port PLLDATO0
            (direction OUTPUT))
          (port I2C1SCLO
            (direction OUTPUT))
          (port I2C1SCLOEN
            (direction OUTPUT))
          (port I2C1SDAO
            (direction OUTPUT))
          (port I2C1SDAOEN
            (direction OUTPUT))
          (port I2C2SCLO
            (direction OUTPUT))
          (port I2C2SCLOEN
            (direction OUTPUT))
          (port I2C2SDAO
            (direction OUTPUT))
          (port I2C2SDAOEN
            (direction OUTPUT))
          (port I2C1IRQO
            (direction OUTPUT))
          (port I2C2IRQO
            (direction OUTPUT))
          (port SPISCKO
            (direction OUTPUT))
          (port SPISCKEN
            (direction OUTPUT))
          (port SPIMISOO
            (direction OUTPUT))
          (port SPIMISOEN
            (direction OUTPUT))
          (port SPIMOSIO
            (direction OUTPUT))
          (port SPIMOSIEN
            (direction OUTPUT))
          (port SPIMCSN7
            (direction OUTPUT))
          (port SPIMCSN6
            (direction OUTPUT))
          (port SPIMCSN5
            (direction OUTPUT))
          (port SPIMCSN4
            (direction OUTPUT))
          (port SPIMCSN3
            (direction OUTPUT))
          (port SPIMCSN2
            (direction OUTPUT))
          (port SPIMCSN1
            (direction OUTPUT))
          (port SPIMCSN0
            (direction OUTPUT))
          (port SPICSNEN
            (direction OUTPUT))
          (port SPIIRQO
            (direction OUTPUT))
          (port TCINT
            (direction OUTPUT))
          (port TCOC
            (direction OUTPUT))
          (port WBCUFMIRQ
            (direction OUTPUT))
          (port CFGWAKE
            (direction OUTPUT))
          (port CFGSTDBY
            (direction OUTPUT)))))
    (cell REFB
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port wb_clk_i
            (direction INPUT))
          (port wb_rst_i
            (direction INPUT))
          (port wb_cyc_i
            (direction INPUT))
          (port wb_stb_i
            (direction INPUT))
          (port wb_we_i
            (direction INPUT))
          (port (array (rename wb_adr_i "wb_adr_i(7:0)") 8)
            (direction INPUT))
          (port (array (rename wb_dat_i "wb_dat_i(7:0)") 8)
            (direction INPUT))
          (port (array (rename wb_dat_o "wb_dat_o(7:0)") 8)
            (direction OUTPUT))
          (port wb_ack_o
            (direction OUTPUT))
          (port wbc_ufm_irq
            (direction OUTPUT)))
        (property NGD_DRC_MASK (integer 1))
        (contents
          (instance scuba_vhi_inst
            (viewRef view1 
              (cellRef VHI)))
          (instance scuba_vlo_inst
            (viewRef view1 
              (cellRef VLO)))
          (instance EFBInst_0
            (viewRef view1 
              (cellRef EFB))
            (property UFM_INIT_FILE_FORMAT
              (string "HEX"))
            (property UFM_INIT_FILE_NAME
              (string "../RAM2E-LCMXO2.mem"))
            (property UFM_INIT_ALL_ZEROS
              (string "DISABLED"))
            (property UFM_INIT_START_PAGE
              (string "190"))
            (property UFM_INIT_PAGES
              (string "321"))
            (property DEV_DENSITY
              (string "1200L"))
            (property EFB_UFM
              (string "ENABLED"))
            (property TC_ICAPTURE
              (string "DISABLED"))
            (property TC_OVERFLOW
              (string "DISABLED"))
            (property TC_ICR_INT
              (string "OFF"))
            (property TC_OCR_INT
              (string "OFF"))
            (property TC_OV_INT
              (string "OFF"))
            (property TC_TOP_SEL
              (string "OFF"))
            (property TC_RESETN
              (string "ENABLED"))
            (property TC_OC_MODE
              (string "TOGGLE"))
            (property TC_OCR_SET
              (string "32767"))
            (property TC_TOP_SET
              (string "65535"))
            (property GSR
              (string "ENABLED"))
            (property TC_CCLK_SEL
              (string "1"))
            (property TC_MODE
              (string "CTCM"))
            (property TC_SCLK_SEL
              (string "PCLOCK"))
            (property EFB_TC_PORTMODE
              (string "WB"))
            (property EFB_TC
              (string "DISABLED"))
            (property SPI_WAKEUP
              (string "DISABLED"))
            (property SPI_INTR_RXOVR
              (string "DISABLED"))
            (property SPI_INTR_TXOVR
              (string "DISABLED"))
            (property SPI_INTR_RXRDY
              (string "DISABLED"))
            (property SPI_INTR_TXRDY
              (string "DISABLED"))
            (property SPI_SLAVE_HANDSHAKE
              (string "DISABLED"))
            (property SPI_PHASE_ADJ
              (string "DISABLED"))
            (property SPI_CLK_INV
              (string "DISABLED"))
            (property SPI_LSB_FIRST
              (string "DISABLED"))
            (property SPI_CLK_DIVIDER
              (string "1"))
            (property SPI_MODE
              (string "MASTER"))
            (property EFB_SPI
              (string "DISABLED"))
            (property I2C2_WAKEUP
              (string "DISABLED"))
            (property I2C2_GEN_CALL
              (string "DISABLED"))
            (property I2C2_CLK_DIVIDER
              (string "1"))
            (property I2C2_BUS_PERF
              (string "100kHz"))
            (property I2C2_SLAVE_ADDR
              (string "0b1000010"))
            (property I2C2_ADDRESSING
              (string "7BIT"))
            (property EFB_I2C2
              (string "DISABLED"))
            (property I2C1_WAKEUP
              (string "DISABLED"))
            (property I2C1_GEN_CALL
              (string "DISABLED"))
            (property I2C1_CLK_DIVIDER
              (string "1"))
            (property I2C1_BUS_PERF
              (string "100kHz"))
            (property I2C1_SLAVE_ADDR
              (string "0b1000001"))
            (property I2C1_ADDRESSING
              (string "7BIT"))
            (property EFB_I2C1
              (string "DISABLED"))
            (property EFB_WB_CLK_FREQ
              (string "14.4")))
          (net scuba_vhi
            (joined
              (portRef Z (instanceRef scuba_vhi_inst))
              (portRef UFMSN (instanceRef EFBInst_0))))
          (net scuba_vlo
            (joined
              (portRef Z (instanceRef scuba_vlo_inst))
              (portRef PLL1DATI7 (instanceRef EFBInst_0))
              (portRef PLL1DATI6 (instanceRef EFBInst_0))
              (portRef PLL1DATI5 (instanceRef EFBInst_0))
              (portRef PLL1DATI4 (instanceRef EFBInst_0))
              (portRef PLL1DATI3 (instanceRef EFBInst_0))
              (portRef PLL1DATI2 (instanceRef EFBInst_0))
              (portRef PLL1DATI1 (instanceRef EFBInst_0))
              (portRef PLL1DATI0 (instanceRef EFBInst_0))
              (portRef PLL1ACKI (instanceRef EFBInst_0))
              (portRef PLL0DATI7 (instanceRef EFBInst_0))
              (portRef PLL0DATI6 (instanceRef EFBInst_0))
              (portRef PLL0DATI5 (instanceRef EFBInst_0))
              (portRef PLL0DATI4 (instanceRef EFBInst_0))
              (portRef PLL0DATI3 (instanceRef EFBInst_0))
              (portRef PLL0DATI2 (instanceRef EFBInst_0))
              (portRef PLL0DATI1 (instanceRef EFBInst_0))
              (portRef PLL0DATI0 (instanceRef EFBInst_0))
              (portRef PLL0ACKI (instanceRef EFBInst_0))
              (portRef TCIC (instanceRef EFBInst_0))
              (portRef TCRSTN (instanceRef EFBInst_0))
              (portRef TCCLKI (instanceRef EFBInst_0))
              (portRef SPISCSN (instanceRef EFBInst_0))
              (portRef SPIMOSII (instanceRef EFBInst_0))
              (portRef SPIMISOI (instanceRef EFBInst_0))
              (portRef SPISCKI (instanceRef EFBInst_0))
              (portRef I2C2SDAI (instanceRef EFBInst_0))
              (portRef I2C2SCLI (instanceRef EFBInst_0))
              (portRef I2C1SDAI (instanceRef EFBInst_0))
              (portRef I2C1SCLI (instanceRef EFBInst_0))))
          (net wbc_ufm_irq
            (joined
              (portRef wbc_ufm_irq)
              (portRef WBCUFMIRQ (instanceRef EFBInst_0))))
          (net wb_ack_o
            (joined
              (portRef wb_ack_o)
              (portRef WBACKO (instanceRef EFBInst_0))))
          (net wb_dat_o7
            (joined
              (portRef (member wb_dat_o 0))
              (portRef WBDATO7 (instanceRef EFBInst_0))))
          (net wb_dat_o6
            (joined
              (portRef (member wb_dat_o 1))
              (portRef WBDATO6 (instanceRef EFBInst_0))))
          (net wb_dat_o5
            (joined
              (portRef (member wb_dat_o 2))
              (portRef WBDATO5 (instanceRef EFBInst_0))))
          (net wb_dat_o4
            (joined
              (portRef (member wb_dat_o 3))
              (portRef WBDATO4 (instanceRef EFBInst_0))))
          (net wb_dat_o3
            (joined
              (portRef (member wb_dat_o 4))
              (portRef WBDATO3 (instanceRef EFBInst_0))))
          (net wb_dat_o2
            (joined
              (portRef (member wb_dat_o 5))
              (portRef WBDATO2 (instanceRef EFBInst_0))))
          (net wb_dat_o1
            (joined
              (portRef (member wb_dat_o 6))
              (portRef WBDATO1 (instanceRef EFBInst_0))))
          (net wb_dat_o0
            (joined
              (portRef (member wb_dat_o 7))
              (portRef WBDATO0 (instanceRef EFBInst_0))))
          (net wb_dat_i7
            (joined
              (portRef (member wb_dat_i 0))
              (portRef WBDATI7 (instanceRef EFBInst_0))))
          (net wb_dat_i6
            (joined
              (portRef (member wb_dat_i 1))
              (portRef WBDATI6 (instanceRef EFBInst_0))))
          (net wb_dat_i5
            (joined
              (portRef (member wb_dat_i 2))
              (portRef WBDATI5 (instanceRef EFBInst_0))))
          (net wb_dat_i4
            (joined
              (portRef (member wb_dat_i 3))
              (portRef WBDATI4 (instanceRef EFBInst_0))))
          (net wb_dat_i3
            (joined
              (portRef (member wb_dat_i 4))
              (portRef WBDATI3 (instanceRef EFBInst_0))))
          (net wb_dat_i2
            (joined
              (portRef (member wb_dat_i 5))
              (portRef WBDATI2 (instanceRef EFBInst_0))))
          (net wb_dat_i1
            (joined
              (portRef (member wb_dat_i 6))
              (portRef WBDATI1 (instanceRef EFBInst_0))))
          (net wb_dat_i0
            (joined
              (portRef (member wb_dat_i 7))
              (portRef WBDATI0 (instanceRef EFBInst_0))))
          (net wb_adr_i7
            (joined
              (portRef (member wb_adr_i 0))
              (portRef WBADRI7 (instanceRef EFBInst_0))))
          (net wb_adr_i6
            (joined
              (portRef (member wb_adr_i 1))
              (portRef WBADRI6 (instanceRef EFBInst_0))))
          (net wb_adr_i5
            (joined
              (portRef (member wb_adr_i 2))
              (portRef WBADRI5 (instanceRef EFBInst_0))))
          (net wb_adr_i4
            (joined
              (portRef (member wb_adr_i 3))
              (portRef WBADRI4 (instanceRef EFBInst_0))))
          (net wb_adr_i3
            (joined
              (portRef (member wb_adr_i 4))
              (portRef WBADRI3 (instanceRef EFBInst_0))))
          (net wb_adr_i2
            (joined
              (portRef (member wb_adr_i 5))
              (portRef WBADRI2 (instanceRef EFBInst_0))))
          (net wb_adr_i1
            (joined
              (portRef (member wb_adr_i 6))
              (portRef WBADRI1 (instanceRef EFBInst_0))))
          (net wb_adr_i0
            (joined
              (portRef (member wb_adr_i 7))
              (portRef WBADRI0 (instanceRef EFBInst_0))))
          (net wb_we_i
            (joined
              (portRef wb_we_i)
              (portRef WBWEI (instanceRef EFBInst_0))))
          (net wb_stb_i
            (joined
              (portRef wb_stb_i)
              (portRef WBSTBI (instanceRef EFBInst_0))))
          (net wb_cyc_i
            (joined
              (portRef wb_cyc_i)
              (portRef WBCYCI (instanceRef EFBInst_0))))
          (net wb_rst_i
            (joined
              (portRef wb_rst_i)
              (portRef WBRSTI (instanceRef EFBInst_0))))
          (net wb_clk_i
            (joined
              (portRef wb_clk_i)
              (portRef WBCLKI (instanceRef EFBInst_0))))))))
  (design REFB
    (cellRef REFB
      (libraryRef ORCLIB)))
)
