;                     
; Template INF for a USB Remote NDIS Device
; Copyright (c) Microsoft Corporation
;

[Version]
Signature           = "$Windows NT$"
Class               = Net
ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider            = %Atmel%
DriverVer           = 06/20/2008,0.0.0.3
;CatalogFile         = Atmel.cat

[Manufacturer]
%Atmel%          = AtmelDevices,NT.5.1

[AtmelDevices]
%AtmelDevice%    = RNDIS, USB\VID_03EB&PID_2021&MI_00

[AtmelDevices.NT.5.1]
%AtmelDevice%    = RNDIS.NT.5.1, USB\VID_03EB&PID_2021&MI_00

[ControlFlags]
ExcludeFromSelect=*

; Windows 2000 specific sections ---------------------------------

[RNDIS.NT]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15
DriverVer       = 06/20/2008,0.0.0.2
AddReg          = RNDIS_AddReg_NT, RNDIS_AddReg_WIN2K,RNDIS_AddReg_Vista
CopyFiles       = RNDIS_CopyFiles_NT

; DO NOT MODIFY THE SERVICE NAME
[RNDIS.NT.Services]
AddService = USB_RNDISY, 2, RNDIS_ServiceInst_NT, RNDIS_EventLog

[RNDIS_CopyFiles_NT]
; no rename of files on Windows 2000, use the 'y' names as is
usb8023y.sys, , , 0 
rndismpy.sys, , , 0 

[RNDIS_ServiceInst_NT]
DisplayName     = %ServiceDisplayName%
ServiceType     = 1 
StartType       = 3 
ErrorControl    = 1 
ServiceBinary   = %12%\usb8023y.sys    
LoadOrderGroup  = NDIS
AddReg          = RNDIS_WMI_AddReg_NT

[RNDIS_WMI_AddReg_NT]
HKR, , MofImagePath, 0x00020000, "System32\drivers\rndismpy.sys"

; Windows XP specific sections -----------------------------------

[RNDIS.NT.5.1]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15
DriverVer       = 06/20/2008,0.0.0.2
AddReg          = RNDIS_AddReg_XP
include         = netrndis.inf
needs           = Usb_Rndis.ndi

; no copyfiles - the files are already in place

[RNDIS.NT.5.1.Services]
include     = netrndis.inf
needs       = Usb_Rndis.ndi.Services

; Windows 2000 sections 

; DO NOT MODIFY ServiceName
[RNDIS_AddReg_NT]
HKR, Ndi,               Service,        0, "USB_RNDISY"
HKR, Ndi\Interfaces,    UpperRange,     0, "ndis5" 
HKR, Ndi\Interfaces,    LowerRange,     0, "ethernet"

[RNDIS_AddReg_WIN2K]
HKR, ,                  ReclaimRecv,    0x00010001, 1
HKR, NDI\params\NetworkAddress, ParamDesc,  0, %NetworkAddress%
HKR, NDI\params\NetworkAddress, type,       0, "edit"
HKR, NDI\params\NetworkAddress, LimitText,  0, "12"
HKR, NDI\params\NetworkAddress, UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress, default,    0, " "
HKR, NDI\params\NetworkAddress, optional,   0, "1"

[RNDIS_EventLog]
AddReg = RNDIS_EventLog_AddReg

[RNDIS_EventLog_AddReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[RNDIS_AddReg_XP]
[RNDIS_AddReg_XP]
HKR, NDI\params\rawmode,      ParamDesc,  0, %RAWMODE%
HKR, NDI\params\rawmode,      base,       0, "10"
HKR, NDI\params\rawmode,      type,       0, "enum"
HKR, NDI\params\rawmode,      default,    0, "0"
HKR, NDI\params\rawmode\enum, "0",        0, "Off"
HKR, NDI\params\rawmode\enum, "1",        0, "On"


[SourceDisksNames]
1=%SourceDisk%,,1

[SourceDisksFiles]
usb8023y.sys=1
rndismpy.sys=1

[DestinationDirs]
RNDIS_CopyFiles_NT    = 12

; DO NOT CHANGE ServiceDisplayName
[Strings]
ServiceDisplayName    = "USB Remote NDIS Y Network Device Driver"
NetworkAddress        = "Network Address"
Atmel                  = "Atmel Corporation"
AtmelDevice            = "Atmel RAVEN USB Stick"
SourceDisk            = "Atmel USB Network Driver Install Disk"
RAWMODE               = "Raw 802.15.4 Mode"
