<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="92.8932" y2="-0.1524" width="0" layer="20"/>
<wire x1="92.8932" y1="-0.1524" x2="92.8932" y2="99.8476" width="0" layer="20"/>
<wire x1="92.8932" y1="99.8476" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<text>TOP</text>
<text>Bot</text>
<text>a1k.org 68030-TK v0.9d
(c) 2014 Matthias Heinrichs
thx BukoCharly, Georg Braun, Herzi</text>
<text>a1k.org 68030-TK V0.9
(c)2013 Matthias Heinrichs
Free for non commercial
reproduction</text>
<text>JTAG</text>
</plain>
<libraries>
<library name="micro-mc68000">
<description>&lt;b&gt;Motorola MC68000 Processors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MPGA128">
<description>&lt;b&gt;micro Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="DIL64">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14S">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-vg">
<description>&lt;b&gt;VG Connectors (DIN 41612/DIN 41617)&lt;/b&gt;&lt;p&gt;
The library contains devices which allow to place the contacts individually or 
in one or several blocks.&lt;p&gt;
This behavior is indicated by the key words &lt;i&gt;single&lt;/i&gt; and &lt;i&gt;block&lt;/i&gt; in
the respective device descriptions.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FABC96R">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
female, 96 pins, type R, rows ABC, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="resistor-dil">
<description>&lt;b&gt;Resistors in DIL Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EXBV8V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.20 mm x 1.60 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
</packages>
</library>
<library name="amd-mach-Small-pad">
<description>&lt;b&gt;AMD MACH4/MACH5 Family (Vantis)&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP100">
<description>&lt;b&gt;THIN QUAD FLAT PACK&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="micro-mc68000" package="MPGA128" value="">
<attribute name="OC_NEWARK" value="52F3269"/>
<attribute name="MPN" value="MC68030RC50C"/>
<attribute name="MF" value="MOTOROLA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="micro-mc68000" package="DIL64" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="micro-mc68000" package="PLCC68" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C4" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C5" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C6" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C12" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C13" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C14" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C16" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C17" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="SV1" library="con-harting-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="QG1" library="crystal" package="DIL14S" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805K" value="15pF">
<attribute name="NAME"/>
</element>
<element name="R1" library="rcl" package="R0805" value="10">
<attribute name="NAME"/>
</element>
<element name="IC5" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="IC6" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R12" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R13" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R15" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R18" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R19" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R20" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R21" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="RN2" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="RN1" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="rcl" package="C1210" value="10µF"/>
<element name="IC7" library="amd-mach-Small-pad" package="TQFP100" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C9" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="L1" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C11" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C15" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R4" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R5" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R7" library="rcl" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C18" library="rcl" package="C1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C19" library="rcl" package="C1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C21" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C22" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C23" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R8" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="X1" library="con-vg" package="FABC96R" value="FABC96R"/>
<element name="IC4" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="IC8" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="IC9" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="IC10" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="IC11" library="74xx-eu" package="SO20W" value="74HCT245DW">
<attribute name="NAME"/>
</element>
<element name="C24" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C25" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C26" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C27" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C28" library="rcl" package="C0603K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R10" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="RN3" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="RN4" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="RN5" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="RN6" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="RN7" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="RN8" library="resistor-dil" package="EXBV8V" value="4,7k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R9" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R22" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R23" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R24" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R25" library="rcl" package="R0603" value="4,7k">
<attribute name="NAME"/>
</element>
<element name="R26" library="rcl" package="R0603" value="4,7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0603" value="4,7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D0">
<contactref element="IC1" pad="K13"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC5" pad="2"/>
<contactref element="X1" pad="B16"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="K12"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="X1" pad="C16"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="L13"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="X1" pad="B15"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="M13"/>
<contactref element="IC3" pad="68"/>
<contactref element="IC5" pad="5"/>
<contactref element="X1" pad="C15"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="L12"/>
<contactref element="IC3" pad="67"/>
<contactref element="IC5" pad="6"/>
<contactref element="X1" pad="B14"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="K11"/>
<contactref element="IC3" pad="66"/>
<contactref element="IC5" pad="7"/>
<contactref element="X1" pad="C14"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="M12"/>
<contactref element="IC3" pad="65"/>
<contactref element="IC5" pad="8"/>
<contactref element="X1" pad="B13"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="L11"/>
<contactref element="IC3" pad="64"/>
<contactref element="IC5" pad="9"/>
<contactref element="X1" pad="C13"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="N13"/>
<contactref element="IC3" pad="62"/>
<contactref element="IC6" pad="2"/>
<contactref element="X1" pad="B12"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="M11"/>
<contactref element="IC3" pad="60"/>
<contactref element="IC6" pad="3"/>
<contactref element="X1" pad="C12"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="L10"/>
<contactref element="IC3" pad="59"/>
<contactref element="IC6" pad="4"/>
<contactref element="X1" pad="B11"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="N12"/>
<contactref element="IC3" pad="58"/>
<contactref element="IC6" pad="5"/>
<contactref element="X1" pad="C11"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="M10"/>
<contactref element="IC3" pad="57"/>
<contactref element="IC6" pad="6"/>
<contactref element="X1" pad="B10"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="N11"/>
<contactref element="IC3" pad="56"/>
<contactref element="IC6" pad="7"/>
<contactref element="X1" pad="C10"/>
</signal>
<signal name="D14">
<contactref element="IC1" pad="M09"/>
<contactref element="IC3" pad="55"/>
<contactref element="IC6" pad="8"/>
<contactref element="X1" pad="B9"/>
</signal>
<signal name="D15">
<contactref element="IC1" pad="N10"/>
<contactref element="IC3" pad="54"/>
<contactref element="IC6" pad="9"/>
<contactref element="X1" pad="C9"/>
</signal>
<signal name="D16">
<contactref element="IC1" pad="N09"/>
<contactref element="IC3" pad="50"/>
<contactref element="X1" pad="B8"/>
<contactref element="IC11" pad="9"/>
</signal>
<signal name="D17">
<contactref element="IC1" pad="M08"/>
<contactref element="IC3" pad="49"/>
<contactref element="X1" pad="C8"/>
<contactref element="IC11" pad="8"/>
</signal>
<signal name="D18">
<contactref element="IC1" pad="N08"/>
<contactref element="IC3" pad="48"/>
<contactref element="X1" pad="B7"/>
<contactref element="IC11" pad="7"/>
</signal>
<signal name="D19">
<contactref element="IC1" pad="N07"/>
<contactref element="IC3" pad="47"/>
<contactref element="X1" pad="C7"/>
<contactref element="IC11" pad="6"/>
</signal>
<signal name="D20">
<contactref element="IC1" pad="M07"/>
<contactref element="IC3" pad="46"/>
<contactref element="X1" pad="B6"/>
<contactref element="IC11" pad="5"/>
</signal>
<signal name="D21">
<contactref element="IC1" pad="N06"/>
<contactref element="IC3" pad="45"/>
<contactref element="X1" pad="C6"/>
<contactref element="IC11" pad="2"/>
</signal>
<signal name="D22">
<contactref element="IC1" pad="M06"/>
<contactref element="IC3" pad="44"/>
<contactref element="X1" pad="B5"/>
<contactref element="IC11" pad="3"/>
</signal>
<signal name="D23">
<contactref element="IC1" pad="N05"/>
<contactref element="IC3" pad="42"/>
<contactref element="X1" pad="C5"/>
<contactref element="IC11" pad="4"/>
</signal>
<signal name="D24">
<contactref element="IC1" pad="M05"/>
<contactref element="IC3" pad="40"/>
<contactref element="X1" pad="B4"/>
<contactref element="IC10" pad="2"/>
</signal>
<signal name="D25">
<contactref element="IC1" pad="N04"/>
<contactref element="IC3" pad="39"/>
<contactref element="X1" pad="C4"/>
<contactref element="IC10" pad="3"/>
</signal>
<signal name="D26">
<contactref element="IC1" pad="N03"/>
<contactref element="IC3" pad="38"/>
<contactref element="X1" pad="B3"/>
<contactref element="IC10" pad="4"/>
</signal>
<signal name="D27">
<contactref element="IC1" pad="M04"/>
<contactref element="IC3" pad="37"/>
<contactref element="X1" pad="C3"/>
<contactref element="IC10" pad="5"/>
</signal>
<signal name="D28">
<contactref element="IC1" pad="N02"/>
<contactref element="IC3" pad="36"/>
<contactref element="X1" pad="B2"/>
<contactref element="IC7" pad="55"/>
<contactref element="IC10" pad="6"/>
</signal>
<signal name="D29">
<contactref element="IC1" pad="M03"/>
<contactref element="IC3" pad="35"/>
<contactref element="X1" pad="C2"/>
<contactref element="IC7" pad="54"/>
<contactref element="IC10" pad="7"/>
</signal>
<signal name="D30">
<contactref element="IC1" pad="L04"/>
<contactref element="IC3" pad="34"/>
<contactref element="IC7" pad="72"/>
<contactref element="X1" pad="B1"/>
<contactref element="IC10" pad="8"/>
</signal>
<signal name="D31">
<contactref element="IC1" pad="N01"/>
<contactref element="IC3" pad="33"/>
<contactref element="X1" pad="C1"/>
<contactref element="IC7" pad="53"/>
<contactref element="IC10" pad="9"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="C04"/>
<contactref element="IC3" pad="25"/>
<contactref element="IC7" pad="60"/>
<contactref element="X1" pad="B32"/>
<contactref element="IC4" pad="2"/>
<contactref element="RN8" pad="2"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="D13"/>
<contactref element="IC3" pad="24"/>
<contactref element="IC7" pad="43"/>
<contactref element="X1" pad="A32"/>
<contactref element="IC4" pad="3"/>
<contactref element="RN8" pad="4"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="D12"/>
<contactref element="IC3" pad="23"/>
<contactref element="IC7" pad="44"/>
<contactref element="X1" pad="C31"/>
<contactref element="IC4" pad="4"/>
<contactref element="RN7" pad="3"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="C13"/>
<contactref element="IC3" pad="22"/>
<contactref element="X1" pad="B31"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC7" pad="46"/>
<contactref element="RN7" pad="4"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="C12"/>
<contactref element="X1" pad="A31"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC7" pad="45"/>
<contactref element="RN8" pad="3"/>
</signal>
<signal name="A6">
<contactref element="IC1" pad="D11"/>
<contactref element="X1" pad="C30"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC7" pad="22"/>
<contactref element="RN6" pad="4"/>
</signal>
<signal name="A7">
<contactref element="IC1" pad="B13"/>
<contactref element="X1" pad="B30"/>
<contactref element="IC4" pad="7"/>
<contactref element="RN7" pad="1"/>
</signal>
<signal name="A8">
<contactref element="IC1" pad="B12"/>
<contactref element="X1" pad="A30"/>
<contactref element="IC4" pad="6"/>
<contactref element="RN7" pad="2"/>
</signal>
<signal name="A9">
<contactref element="IC1" pad="C11"/>
<contactref element="X1" pad="C29"/>
<contactref element="IC8" pad="9"/>
<contactref element="RN6" pad="1"/>
</signal>
<signal name="A10">
<contactref element="IC1" pad="A13"/>
<contactref element="X1" pad="B29"/>
<contactref element="IC8" pad="8"/>
<contactref element="RN6" pad="2"/>
</signal>
<signal name="A11">
<contactref element="IC1" pad="C10"/>
<contactref element="X1" pad="A29"/>
<contactref element="IC8" pad="7"/>
<contactref element="RN6" pad="3"/>
</signal>
<signal name="A12">
<contactref element="IC1" pad="B11"/>
<contactref element="X1" pad="C28"/>
<contactref element="IC8" pad="6"/>
<contactref element="RN5" pad="2"/>
</signal>
<signal name="A13">
<contactref element="IC1" pad="A12"/>
<contactref element="X1" pad="B28"/>
<contactref element="IC8" pad="5"/>
<contactref element="RN5" pad="3"/>
</signal>
<signal name="A14">
<contactref element="IC1" pad="B10"/>
<contactref element="X1" pad="A28"/>
<contactref element="IC8" pad="4"/>
<contactref element="RN5" pad="4"/>
</signal>
<signal name="A15">
<contactref element="IC1" pad="A11"/>
<contactref element="X1" pad="C27"/>
<contactref element="IC8" pad="3"/>
<contactref element="RN4" pad="3"/>
</signal>
<signal name="A16">
<contactref element="IC1" pad="B09"/>
<contactref element="IC7" pad="96"/>
<contactref element="X1" pad="B27"/>
<contactref element="IC8" pad="2"/>
<contactref element="RN4" pad="4"/>
</signal>
<signal name="A17">
<contactref element="IC1" pad="A10"/>
<contactref element="X1" pad="A27"/>
<contactref element="IC7" pad="59"/>
<contactref element="IC9" pad="9"/>
<contactref element="RN5" pad="1"/>
</signal>
<signal name="A18">
<contactref element="IC1" pad="C08"/>
<contactref element="IC7" pad="95"/>
<contactref element="X1" pad="C26"/>
<contactref element="IC9" pad="8"/>
<contactref element="RN3" pad="4"/>
</signal>
<signal name="A19">
<contactref element="IC1" pad="A09"/>
<contactref element="IC7" pad="97"/>
<contactref element="X1" pad="B26"/>
<contactref element="IC9" pad="7"/>
<contactref element="RN4" pad="1"/>
</signal>
<signal name="A20">
<contactref element="IC1" pad="B08"/>
<contactref element="IC7" pad="93"/>
<contactref element="X1" pad="A26"/>
<contactref element="IC9" pad="6"/>
<contactref element="RN4" pad="2"/>
</signal>
<signal name="A21">
<contactref element="IC1" pad="A08"/>
<contactref element="IC7" pad="94"/>
<contactref element="X1" pad="C25"/>
<contactref element="IC9" pad="5"/>
<contactref element="RN3" pad="1"/>
</signal>
<signal name="A22">
<contactref element="IC1" pad="B07"/>
<contactref element="X1" pad="B25"/>
<contactref element="IC9" pad="4"/>
<contactref element="IC7" pad="84"/>
<contactref element="RN3" pad="2"/>
</signal>
<signal name="A23">
<contactref element="IC1" pad="A07"/>
<contactref element="X1" pad="A25"/>
<contactref element="IC9" pad="3"/>
<contactref element="IC7" pad="85"/>
<contactref element="RN3" pad="3"/>
</signal>
<signal name="FC0">
<contactref element="IC2" pad="28"/>
<contactref element="IC1" pad="D02"/>
<contactref element="X1" pad="C19"/>
<contactref element="IC7" pad="57"/>
</signal>
<signal name="FC1">
<contactref element="IC2" pad="27"/>
<contactref element="IC1" pad="C01"/>
<contactref element="X1" pad="B19"/>
<contactref element="IC7" pad="58"/>
</signal>
<signal name="FC2">
<contactref element="IC2" pad="26"/>
<contactref element="IC1" pad="D01"/>
<contactref element="X1" pad="A19"/>
</signal>
<signal name="E_00">
<contactref element="IC2" pad="20"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="VMA_00">
<contactref element="IC2" pad="19"/>
<contactref element="IC7" pad="35"/>
</signal>
<signal name="BG_00">
<contactref element="IC2" pad="11"/>
<contactref element="IC7" pad="29"/>
</signal>
<signal name="AS_00">
<contactref element="IC2" pad="6"/>
<contactref element="IC7" pad="42"/>
</signal>
<signal name="R/W">
<contactref element="IC1" pad="L03"/>
<contactref element="IC3" pad="28"/>
<contactref element="X1" pad="B18"/>
<contactref element="IC7" pad="71"/>
</signal>
<signal name="UDS_00">
<contactref element="IC2" pad="7"/>
<contactref element="IC7" pad="32"/>
</signal>
<signal name="LDS_00">
<contactref element="IC2" pad="8"/>
<contactref element="IC7" pad="31"/>
</signal>
<signal name="CLK_00">
<contactref element="IC2" pad="15"/>
<contactref element="IC7" pad="11"/>
</signal>
<signal name="BERR">
<contactref element="IC2" pad="22"/>
<contactref element="IC1" pad="H01"/>
<contactref element="X1" pad="C17"/>
<contactref element="IC7" pad="41"/>
</signal>
<signal name="RST">
<contactref element="IC2" pad="18"/>
<contactref element="IC7" pad="86"/>
</signal>
<signal name="HLT">
<contactref element="IC2" pad="17"/>
<contactref element="IC1" pad="H02"/>
</signal>
<signal name="VPA_00">
<contactref element="IC2" pad="21"/>
<contactref element="IC7" pad="36"/>
</signal>
<signal name="BGACK_00">
<contactref element="IC2" pad="12"/>
<contactref element="IC7" pad="28"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC9" pad="1"/>
</signal>
<signal name="DTACK_00">
<contactref element="IC2" pad="10"/>
<contactref element="IC7" pad="30"/>
</signal>
<signal name="IPL0">
<contactref element="IC2" pad="25"/>
<contactref element="IC7" pad="67"/>
</signal>
<signal name="IPL1">
<contactref element="IC2" pad="24"/>
<contactref element="IC7" pad="56"/>
</signal>
<signal name="IPL2">
<contactref element="IC2" pad="23"/>
<contactref element="IC7" pad="68"/>
</signal>
<signal name="CLK_30">
<contactref element="IC1" pad="E01"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="F12"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC7" pad="3"/>
<contactref element="X1" pad="A18"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="BG_30">
<contactref element="R19" pad="2"/>
<contactref element="IC7" pad="21"/>
<contactref element="X1" pad="A12"/>
<contactref element="IC1" pad="B02"/>
</signal>
<signal name="BR_30">
<contactref element="IC1" pad="A01"/>
<contactref element="IC2" pad="13"/>
<contactref element="X1" pad="A11"/>
</signal>
<signal name="BGACK_30">
<contactref element="IC1" pad="C03"/>
<contactref element="IC7" pad="83"/>
<contactref element="X1" pad="C20"/>
</signal>
<signal name="IPEND">
<contactref element="IC1" pad="E13"/>
</signal>
<signal name="AVEC">
<contactref element="IC1" pad="E02"/>
<contactref element="X1" pad="A13"/>
<contactref element="R17" pad="2"/>
<contactref element="IC7" pad="92"/>
</signal>
<signal name="CIIN">
<contactref element="IC1" pad="L01"/>
<contactref element="IC7" pad="47"/>
<contactref element="R8" pad="2"/>
<contactref element="X1" pad="A6"/>
</signal>
<signal name="CIOUT">
<contactref element="IC1" pad="C02"/>
</signal>
<signal name="CBREQ">
<contactref element="IC1" pad="K01"/>
<contactref element="R13" pad="1"/>
<contactref element="X1" pad="A8"/>
</signal>
<signal name="CBACK">
<contactref element="IC1" pad="J01"/>
<contactref element="R20" pad="1"/>
<contactref element="X1" pad="A7"/>
</signal>
<signal name="STERM">
<contactref element="IC1" pad="G01"/>
<contactref element="R15" pad="1"/>
<contactref element="X1" pad="A22"/>
</signal>
<signal name="MMUDIS">
<contactref element="IC1" pad="F13"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="CDIS">
<contactref element="IC1" pad="H12"/>
<contactref element="R12" pad="1"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="STATUS">
<contactref element="IC1" pad="J12"/>
</signal>
<signal name="REFILL">
<contactref element="IC1" pad="J13"/>
</signal>
<signal name="DSACK1">
<contactref element="IC1" pad="G02"/>
<contactref element="IC3" pad="32"/>
<contactref element="IC7" pad="81"/>
<contactref element="X1" pad="A15"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="DSACK0">
<contactref element="IC1" pad="F01"/>
<contactref element="IC3" pad="31"/>
<contactref element="X1" pad="A9"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="SIZ0">
<contactref element="IC1" pad="L02"/>
<contactref element="X1" pad="A21"/>
<contactref element="IC7" pad="70"/>
</signal>
<signal name="SIZ1">
<contactref element="IC1" pad="K03"/>
<contactref element="X1" pad="B21"/>
<contactref element="IC7" pad="79"/>
</signal>
<signal name="ECS">
<contactref element="IC1" pad="M02"/>
<contactref element="R18" pad="2"/>
<contactref element="X1" pad="B20"/>
</signal>
<signal name="OCS">
<contactref element="IC1" pad="D03"/>
</signal>
<signal name="RMC">
<contactref element="IC1" pad="B01"/>
</signal>
<signal name="AS_30">
<contactref element="IC1" pad="J02"/>
<contactref element="IC3" pad="21"/>
<contactref element="IC7" pad="82"/>
<contactref element="X1" pad="C21"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="DS_30">
<contactref element="IC1" pad="K02"/>
<contactref element="IC3" pad="20"/>
<contactref element="IC7" pad="98"/>
<contactref element="X1" pad="A10"/>
<contactref element="X1" pad="A20"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="DBEN">
<contactref element="IC1" pad="M01"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="A02"/>
<contactref element="X1" pad="C32"/>
<contactref element="IC7" pad="69"/>
<contactref element="RN8" pad="1"/>
</signal>
<signal name="A24">
<contactref element="IC1" pad="A06"/>
<contactref element="IC7" pad="19"/>
<contactref element="X1" pad="C24"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="A25">
<contactref element="IC1" pad="B06"/>
<contactref element="IC7" pad="18"/>
<contactref element="X1" pad="B24"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="A26">
<contactref element="IC1" pad="A05"/>
<contactref element="IC7" pad="17"/>
<contactref element="X1" pad="A24"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="A28">
<contactref element="IC1" pad="A04"/>
<contactref element="IC7" pad="15"/>
<contactref element="X1" pad="B23"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="A29">
<contactref element="IC1" pad="B04"/>
<contactref element="IC7" pad="6"/>
<contactref element="X1" pad="A23"/>
<contactref element="RN2" pad="1"/>
</signal>
<signal name="A30">
<contactref element="IC1" pad="A03"/>
<contactref element="IC7" pad="5"/>
<contactref element="X1" pad="C22"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="A31">
<contactref element="IC1" pad="B03"/>
<contactref element="IC7" pad="4"/>
<contactref element="X1" pad="B22"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="CS_FPU">
<contactref element="IC3" pad="29"/>
<contactref element="IC7" pad="78"/>
</signal>
<signal name="VCC">
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="26"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC2" pad="49"/>
<contactref element="IC1" pad="C06"/>
<contactref element="IC1" pad="D04"/>
<contactref element="IC1" pad="D10"/>
<contactref element="IC1" pad="F02"/>
<contactref element="IC1" pad="F11"/>
<contactref element="IC1" pad="H03"/>
<contactref element="IC1" pad="H11"/>
<contactref element="IC1" pad="K04"/>
<contactref element="IC1" pad="K10"/>
<contactref element="IC1" pad="L06"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC3" pad="27"/>
<contactref element="IC3" pad="43"/>
<contactref element="IC3" pad="52"/>
<contactref element="IC3" pad="53"/>
<contactref element="IC3" pad="61"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC6" pad="20"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC6" pad="20"/>
<contactref element="SV1" pad="4"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC7" pad="87"/>
<contactref element="IC7" pad="90"/>
<contactref element="IC7" pad="12"/>
<contactref element="IC7" pad="37"/>
<contactref element="IC7" pad="40"/>
<contactref element="IC7" pad="62"/>
<contactref element="IC7" pad="73"/>
<contactref element="L1" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="X1" pad="A3"/>
<contactref element="X1" pad="A4"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC8" pad="20"/>
<contactref element="IC9" pad="20"/>
<contactref element="IC10" pad="20"/>
<contactref element="IC11" pad="20"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC8" pad="20"/>
<contactref element="IC9" pad="20"/>
<contactref element="IC11" pad="20"/>
<contactref element="IC10" pad="20"/>
<contactref element="C28" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="X1" pad="A5"/>
<contactref element="R2" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="53"/>
<contactref element="IC1" pad="C05"/>
<contactref element="IC1" pad="C07"/>
<contactref element="IC1" pad="C09"/>
<contactref element="IC1" pad="E03"/>
<contactref element="IC1" pad="E11"/>
<contactref element="IC1" pad="F03"/>
<contactref element="IC1" pad="G03"/>
<contactref element="IC1" pad="G11"/>
<contactref element="IC1" pad="J03"/>
<contactref element="IC1" pad="J11"/>
<contactref element="IC1" pad="L05"/>
<contactref element="IC1" pad="L07"/>
<contactref element="IC1" pad="L08"/>
<contactref element="IC1" pad="L09"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC3" pad="12"/>
<contactref element="IC3" pad="14"/>
<contactref element="IC3" pad="19"/>
<contactref element="IC3" pad="30"/>
<contactref element="IC3" pad="41"/>
<contactref element="IC3" pad="51"/>
<contactref element="IC3" pad="63"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="QG1" pad="7"/>
<contactref element="C7" pad="2"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC6" pad="10"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC6" pad="10"/>
<contactref element="SV1" pad="2"/>
<contactref element="SV1" pad="10"/>
<contactref element="RN2" pad="8"/>
<contactref element="RN2" pad="7"/>
<contactref element="RN2" pad="6"/>
<contactref element="RN2" pad="5"/>
<contactref element="RN1" pad="8"/>
<contactref element="RN1" pad="7"/>
<contactref element="RN1" pad="6"/>
<contactref element="RN1" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="IC7" pad="89"/>
<contactref element="IC7" pad="88"/>
<contactref element="IC7" pad="77"/>
<contactref element="IC7" pad="76"/>
<contactref element="IC7" pad="100"/>
<contactref element="IC7" pad="99"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC7" pad="13"/>
<contactref element="IC7" pad="25"/>
<contactref element="IC7" pad="26"/>
<contactref element="IC7" pad="27"/>
<contactref element="IC7" pad="38"/>
<contactref element="IC7" pad="39"/>
<contactref element="IC7" pad="49"/>
<contactref element="IC7" pad="50"/>
<contactref element="IC7" pad="51"/>
<contactref element="IC7" pad="75"/>
<contactref element="IC7" pad="52"/>
<contactref element="IC7" pad="63"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="X1" pad="A1"/>
<contactref element="X1" pad="A2"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC9" pad="10"/>
<contactref element="IC10" pad="10"/>
<contactref element="IC11" pad="10"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC9" pad="10"/>
<contactref element="IC11" pad="10"/>
<contactref element="IC10" pad="10"/>
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="RN3" pad="5"/>
<contactref element="RN3" pad="6"/>
<contactref element="RN3" pad="7"/>
<contactref element="RN3" pad="8"/>
<contactref element="RN6" pad="8"/>
<contactref element="RN6" pad="7"/>
<contactref element="RN6" pad="6"/>
<contactref element="RN6" pad="5"/>
<contactref element="RN5" pad="8"/>
<contactref element="RN5" pad="7"/>
<contactref element="RN5" pad="6"/>
<contactref element="RN5" pad="5"/>
<contactref element="RN4" pad="8"/>
<contactref element="RN4" pad="7"/>
<contactref element="RN4" pad="6"/>
<contactref element="RN4" pad="5"/>
<contactref element="RN7" pad="5"/>
<contactref element="RN7" pad="6"/>
<contactref element="RN7" pad="7"/>
<contactref element="RN7" pad="8"/>
<contactref element="RN8" pad="5"/>
<contactref element="RN8" pad="6"/>
<contactref element="RN8" pad="7"/>
<contactref element="RN8" pad="8"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="A27">
<contactref element="IC1" pad="B05"/>
<contactref element="IC7" pad="16"/>
<contactref element="X1" pad="C23"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="OSZI_OUT">
<contactref element="QG1" pad="8"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="AMIGA_BUS_EN_LOW">
<contactref element="IC6" pad="19"/>
<contactref element="IC5" pad="19"/>
<contactref element="IC7" pad="20"/>
</signal>
<signal name="TCK">
<contactref element="SV1" pad="1"/>
<contactref element="IC7" pad="24"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="TMS">
<contactref element="SV1" pad="5"/>
<contactref element="IC7" pad="23"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="TDO">
<contactref element="IC7" pad="74"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="TDI">
<contactref element="SV1" pad="9"/>
<contactref element="IC7" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="CLK_OSZI">
<contactref element="R1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="IC7" pad="61"/>
</signal>
<signal name="VCC_OSZI">
<contactref element="L1" pad="2"/>
<contactref element="QG1" pad="14"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="IPL0_30">
<contactref element="IC1" pad="H13"/>
<contactref element="IC7" pad="8"/>
<contactref element="X1" pad="B17"/>
</signal>
<signal name="IPL1_30">
<contactref element="IC1" pad="G13"/>
<contactref element="IC7" pad="7"/>
<contactref element="X1" pad="A17"/>
</signal>
<signal name="IPL2_30">
<contactref element="IC1" pad="G12"/>
<contactref element="IC7" pad="9"/>
<contactref element="X1" pad="C18"/>
</signal>
<signal name="CLK_EXP">
<contactref element="X1" pad="A14"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="TDO-PIN">
<contactref element="SV1" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="IO_EXP">
<contactref element="R2" pad="1"/>
<contactref element="IC7" pad="14"/>
<contactref element="X1" pad="A16"/>
</signal>
<signal name="AMIGA_BUS_ENABLE_HIGH">
<contactref element="IC7" pad="34"/>
<contactref element="IC11" pad="19"/>
<contactref element="IC10" pad="19"/>
</signal>
<signal name="AMIGA_DATA_DIR">
<contactref element="IC7" pad="48"/>
<contactref element="IC11" pad="1"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="R/W_00">
<contactref element="IC2" pad="9"/>
<contactref element="IC7" pad="80"/>
</signal>
<signal name="AMIGA_A1">
<contactref element="IC2" pad="29"/>
<contactref element="IC4" pad="18"/>
</signal>
<signal name="AMIGA_A2">
<contactref element="IC2" pad="30"/>
<contactref element="IC4" pad="17"/>
</signal>
<signal name="AMIGA_A3">
<contactref element="IC2" pad="31"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="AMIGA_A4">
<contactref element="IC2" pad="32"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="AMIGA_A5">
<contactref element="IC2" pad="33"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="AMIGA_A6">
<contactref element="IC2" pad="34"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="AMIGA_A7">
<contactref element="IC2" pad="35"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="AMIGA_A8">
<contactref element="IC2" pad="36"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="AMIGA_A9">
<contactref element="IC2" pad="37"/>
<contactref element="IC8" pad="11"/>
</signal>
<signal name="AMIGA_A10">
<contactref element="IC2" pad="38"/>
<contactref element="IC8" pad="12"/>
</signal>
<signal name="AMIGA_A11">
<contactref element="IC2" pad="39"/>
<contactref element="IC8" pad="13"/>
</signal>
<signal name="AMIGA_A12">
<contactref element="IC2" pad="40"/>
<contactref element="IC8" pad="14"/>
</signal>
<signal name="AMIGA_A13">
<contactref element="IC2" pad="41"/>
<contactref element="IC8" pad="15"/>
</signal>
<signal name="AMIGA_A14">
<contactref element="IC2" pad="42"/>
<contactref element="IC8" pad="16"/>
</signal>
<signal name="AMIGA_A15">
<contactref element="IC2" pad="43"/>
<contactref element="IC8" pad="17"/>
</signal>
<signal name="AMIGA_A16">
<contactref element="IC2" pad="44"/>
<contactref element="IC8" pad="18"/>
</signal>
<signal name="AMIGA_A17">
<contactref element="IC2" pad="45"/>
<contactref element="IC9" pad="11"/>
</signal>
<signal name="AMIGA_A18">
<contactref element="IC2" pad="46"/>
<contactref element="IC9" pad="12"/>
</signal>
<signal name="AMIGA_A19">
<contactref element="IC2" pad="47"/>
<contactref element="IC9" pad="13"/>
</signal>
<signal name="AMIGA_A20">
<contactref element="IC2" pad="48"/>
<contactref element="IC9" pad="14"/>
</signal>
<signal name="AMIGA_A21">
<contactref element="IC2" pad="50"/>
<contactref element="IC9" pad="15"/>
</signal>
<signal name="AMIGA_A22">
<contactref element="IC2" pad="51"/>
<contactref element="IC9" pad="16"/>
</signal>
<signal name="AMIGA_A23">
<contactref element="IC2" pad="52"/>
<contactref element="IC9" pad="17"/>
</signal>
<signal name="AMIGA_D0">
<contactref element="IC2" pad="5"/>
<contactref element="IC11" pad="11"/>
<contactref element="IC5" pad="18"/>
</signal>
<signal name="AMIGA_D1">
<contactref element="IC2" pad="4"/>
<contactref element="IC11" pad="12"/>
<contactref element="IC5" pad="17"/>
</signal>
<signal name="AMIGA_D2">
<contactref element="IC2" pad="3"/>
<contactref element="IC11" pad="13"/>
<contactref element="IC5" pad="16"/>
</signal>
<signal name="AMIGA_D3">
<contactref element="IC2" pad="2"/>
<contactref element="IC11" pad="14"/>
<contactref element="IC5" pad="15"/>
</signal>
<signal name="AMIGA_D4">
<contactref element="IC2" pad="1"/>
<contactref element="IC11" pad="15"/>
<contactref element="IC5" pad="14"/>
</signal>
<signal name="AMIGA_D5">
<contactref element="IC2" pad="64"/>
<contactref element="IC11" pad="18"/>
<contactref element="IC5" pad="13"/>
</signal>
<signal name="AMIGA_D6">
<contactref element="IC2" pad="63"/>
<contactref element="IC11" pad="17"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="AMIGA_D7">
<contactref element="IC2" pad="62"/>
<contactref element="IC11" pad="16"/>
<contactref element="IC5" pad="11"/>
</signal>
<signal name="AMIGA_D8">
<contactref element="IC2" pad="61"/>
<contactref element="IC10" pad="18"/>
<contactref element="IC6" pad="18"/>
</signal>
<signal name="AMIGA_D9">
<contactref element="IC2" pad="60"/>
<contactref element="IC10" pad="17"/>
<contactref element="IC6" pad="17"/>
</signal>
<signal name="AMIGA_D10">
<contactref element="IC2" pad="59"/>
<contactref element="IC10" pad="16"/>
<contactref element="IC6" pad="16"/>
</signal>
<signal name="AMIGA_D11">
<contactref element="IC2" pad="58"/>
<contactref element="IC10" pad="15"/>
<contactref element="IC6" pad="15"/>
</signal>
<signal name="AMIGA_D12">
<contactref element="IC2" pad="57"/>
<contactref element="IC10" pad="14"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="AMIGA_D13">
<contactref element="IC2" pad="56"/>
<contactref element="IC10" pad="13"/>
<contactref element="IC6" pad="13"/>
</signal>
<signal name="AMIGA_D14">
<contactref element="IC2" pad="55"/>
<contactref element="IC10" pad="12"/>
<contactref element="IC6" pad="12"/>
</signal>
<signal name="AMIGA_D15">
<contactref element="IC2" pad="54"/>
<contactref element="IC10" pad="11"/>
<contactref element="IC6" pad="11"/>
</signal>
<signal name="CLK_30_CPLD">
<contactref element="IC7" pad="64"/>
<contactref element="IC7" pad="65"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="CLK_30_FPU">
<contactref element="R11" pad="2"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="R14" pad="2"/>
<contactref element="IC7" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="IC7" pad="66"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="!FPU_SENSE">
<contactref element="IC3" pad="4"/>
<contactref element="IC7" pad="91"/>
</signal>
<signal name="AMIGA_ADR_ENABLE">
<contactref element="IC4" pad="19"/>
<contactref element="IC8" pad="19"/>
<contactref element="IC9" pad="19"/>
<contactref element="IC7" pad="33"/>
</signal>
<signal name="N$3">
<contactref element="IC9" pad="18"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R27" pad="2"/>
<contactref element="IC9" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
