(export (version D)
  (design
    (source C:\Users\Steve\Documents\AppleIIeCardYCable\AppleIIeCardYCable.sch)
    (date "7/21/2020 7:08:56 PM")
    (tool "Eeschema (5.1.6)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Apple IIe Card Y Cable")
        (company "Steve Maves")
        (rev)
        (date)
        (source AppleIIeCardYCable.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J3)
      (value Conn_02x10_Odd_Even)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x10_Odd_Even) (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0FE758))
    (comp (ref J1)
      (value 10090926-P264XLF)
      (footprint 10090926P264XLF)
      (datasheet http://portal.fciconnect.com/Comergent//fci/drawing/10090926.pdf)
      (fields
        (field (name "Arrow Part Number") 10090926-P264XLF)
        (field (name "Arrow Price/Stock") https://www.arrow.com/en/products/10090926-p264xlf/amphenol-fci)
        (field (name Description) "D Sub HD right angle male 26 way TMT Amphenol FCI 10090926 Series, 26 Way Right Angle Through Hole mount PCB D-sub Connector Plug, 2.29mm Pitch")
        (field (name Height) 12.8)
        (field (name Manufacturer_Name) Amphenol)
        (field (name Manufacturer_Part_Number) 10090926-P264XLF)
        (field (name "Mouser Part Number") 649-10090926-P264XLF)
        (field (name "Mouser Price/Stock") https://www.mouser.com/Search/Refine.aspx?Keyword=649-10090926-P264XLF))
      (libsource (lib 10090926-P264XLF) (part 10090926-P264XLF) (description "D Sub HD right angle male 26 way TMT Amphenol FCI 10090926 Series, 26 Way Right Angle Through Hole mount PCB D-sub Connector Plug, 2.29mm Pitch"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0FD231))
    (comp (ref J2)
      (value A-DF_09_A_KG-T2S)
      (footprint A-DF-09-AKG-T2S_1)
      (datasheet http://assmann.us/specs/A-DF-xx-A_KG-T2x.pdf)
      (fields
        (field (name "Arrow Part Number") "A-DF 09 A/KG-T2S")
        (field (name "Arrow Price/Stock") https://www.arrow.com/en/products/a-df09akg-t2s/assmann-wsw-components-inc)
        (field (name Description) "DSub connector - R/A Shrouded, Hex Stand-off, Female 9 pin")
        (field (name Manufacturer_Name) "ASSMANN WSW components GmbH")
        (field (name Manufacturer_Part_Number) "A-DF 09 A/KG-T2S"))
      (libsource (lib A-DF_09_A_KG-T2S) (part A-DF_09_A_KG-T2S) (description "DSub connector - R/A Shrouded, Hex Stand-off, Female 9 pin"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F18FA61)))
  (libparts
    (libpart (lib 10090926-P264XLF) (part 10090926-P264XLF)
      (description "D Sub HD right angle male 26 way TMT Amphenol FCI 10090926 Series, 26 Way Right Angle Through Hole mount PCB D-sub Connector Plug, 2.29mm Pitch")
      (docs http://portal.fciconnect.com/Comergent//fci/drawing/10090926.pdf)
      (fields
        (field (name Reference) J)
        (field (name Value) 10090926-P264XLF)
        (field (name Footprint) 10090926P264XLF)
        (field (name Datasheet) http://portal.fciconnect.com/Comergent//fci/drawing/10090926.pdf)
        (field (name Description) "D Sub HD right angle male 26 way TMT Amphenol FCI 10090926 Series, 26 Way Right Angle Through Hole mount PCB D-sub Connector Plug, 2.29mm Pitch")
        (field (name Height) 12.8)
        (field (name Manufacturer_Name) Amphenol)
        (field (name Manufacturer_Part_Number) 10090926-P264XLF)
        (field (name "Arrow Part Number") 10090926-P264XLF)
        (field (name "Arrow Price/Stock") https://www.arrow.com/en/products/10090926-p264xlf/amphenol-fci)
        (field (name "Mouser Part Number") 649-10090926-P264XLF)
        (field (name "Mouser Price/Stock") https://www.mouser.com/Search/Refine.aspx?Keyword=649-10090926-P264XLF))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name 14) (type passive))
        (pin (num 15) (name 15) (type passive))
        (pin (num 16) (name 16) (type passive))
        (pin (num 17) (name 17) (type passive))
        (pin (num 18) (name 18) (type passive))
        (pin (num 19) (name 19) (type passive))
        (pin (num 20) (name 20) (type passive))
        (pin (num 21) (name 21) (type passive))
        (pin (num 22) (name 22) (type passive))
        (pin (num 23) (name 23) (type passive))
        (pin (num 24) (name 24) (type passive))
        (pin (num 25) (name 25) (type passive))
        (pin (num 26) (name 26) (type passive))
        (pin (num MH1) (name MH1) (type passive))
        (pin (num MH2) (name MH2) (type passive))))
    (libpart (lib A-DF_09_A_KG-T2S) (part A-DF_09_A_KG-T2S)
      (description "DSub connector - R/A Shrouded, Hex Stand-off, Female 9 pin")
      (docs http://assmann.us/specs/A-DF-xx-A_KG-T2x.pdf)
      (fields
        (field (name Reference) J)
        (field (name Value) A-DF_09_A_KG-T2S)
        (field (name Footprint) A-DF-09-AKG-T2S_1)
        (field (name Datasheet) http://assmann.us/specs/A-DF-xx-A_KG-T2x.pdf)
        (field (name Description) "DSub connector - R/A Shrouded, Hex Stand-off, Female 9 pin")
        (field (name Manufacturer_Name) "ASSMANN WSW components GmbH")
        (field (name Manufacturer_Part_Number) "A-DF 09 A/KG-T2S")
        (field (name "Arrow Part Number") "A-DF 09 A/KG-T2S")
        (field (name "Arrow Price/Stock") https://www.arrow.com/en/products/a-df09akg-t2s/assmann-wsw-components-inc))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x10_Odd_Even)
      (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x10_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive)))))
  (libraries
    (library (logical 10090926-P264XLF)
      (uri C:/Users/Steve/Downloads/LIB_10090926-P264XLF/10090926-P264XLF/KiCad/10090926-P264XLF.lib))
    (library (logical A-DF_09_A_KG-T2S)
      (uri C:/Users/Steve/Downloads/LIB_A-DF_09_A_KG-T2S/A-DF_09_A_KG-T2S/KiCad/A-DF_09_A_KG-T2S.lib))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib")))
  (nets
    (net (code 1) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24))
      (node (ref J3) (pin 2)))
    (net (code 2) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7))
      (node (ref J3) (pin 4)))
    (net (code 3) (name "Net-(J1-Pad16)")
      (node (ref J3) (pin 6))
      (node (ref J1) (pin 16)))
    (net (code 4) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25))
      (node (ref J3) (pin 8)))
    (net (code 5) (name "Net-(J1-Pad8)")
      (node (ref J3) (pin 10))
      (node (ref J1) (pin 8)))
    (net (code 6) (name "Net-(J1-Pad3)")
      (node (ref J2) (pin 8))
      (node (ref J1) (pin 3)))
    (net (code 7) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11))
      (node (ref J2) (pin 9)))
    (net (code 8) (name GND)
      (node (ref J1) (pin 14))
      (node (ref J3) (pin 7))
      (node (ref J3) (pin 1))
      (node (ref J2) (pin 3))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref J3) (pin 5))
      (node (ref J3) (pin 3))
      (node (ref J1) (pin 13)))
    (net (code 9) (name +5V)
      (node (ref J1) (pin 5))
      (node (ref J3) (pin 11)))
    (net (code 10) (name "Net-(J3-Pad9)")
      (node (ref J3) (pin 9)))
    (net (code 11) (name "Net-(J3-Pad13)")
      (node (ref J3) (pin 13)))
    (net (code 12) (name "Net-(J3-Pad15)")
      (node (ref J3) (pin 15)))
    (net (code 13) (name "Net-(J3-Pad17)")
      (node (ref J3) (pin 17)))
    (net (code 14) (name "Net-(J3-Pad19)")
      (node (ref J3) (pin 19)))
    (net (code 15) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 16) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 17) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 18) (name "Net-(J1-PadMH1)")
      (node (ref J1) (pin MH1)))
    (net (code 19) (name "Net-(J1-PadMH2)")
      (node (ref J1) (pin MH2)))
    (net (code 20) (name "Net-(J1-Pad9)")
      (node (ref J3) (pin 16))
      (node (ref J1) (pin 9)))
    (net (code 21) (name "Net-(J1-Pad17)")
      (node (ref J3) (pin 12))
      (node (ref J1) (pin 17)))
    (net (code 22) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26))
      (node (ref J3) (pin 14)))
    (net (code 23) (name "Net-(J1-Pad18)")
      (node (ref J3) (pin 18))
      (node (ref J1) (pin 18)))
    (net (code 24) (name "Net-(J1-Pad15)")
      (node (ref J3) (pin 20))
      (node (ref J1) (pin 15)))
    (net (code 25) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12))
      (node (ref J2) (pin 5)))
    (net (code 26) (name "Net-(J1-Pad20)")
      (node (ref J1) (pin 20))
      (node (ref J2) (pin 4)))
    (net (code 27) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19))
      (node (ref J2) (pin 6)))
    (net (code 28) (name "Net-(J1-Pad10)")
      (node (ref J2) (pin 7))
      (node (ref J1) (pin 10)))
    (net (code 29) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 30) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21))
      (node (ref J2) (pin 2)))))