### Summary

Design Name | WarpSE
Fitting Status | Successful
Software Version | P.20131013
Device Used | XC95144XL-10-TQ100
Date | 4- 7-2023, 2:26AM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
121/144 (85%) | 395/720 (55%) | 97/144 (68%) | 71/81 (88%) | 236/432 (55%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 32 | 32
Output | 35 | 35
Bidirectional | 1 | 1
GCK | 3 | 3
GTS | 0 | 0
GSR | 0 | 0

Pin Type | Used | Total
--- | --- | ---
I/O | 65 | 74
GCK/IO | 3 | 3
GTS/IO | 3 | 4
GSR/IO | 0 | 1

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | C16M
Signal mapped onto global clock net (GCK2) | C8M
Signal mapped onto global clock net (GCK3) | FCLK

##### POWER DATA

Macrocells in high performance mode (MCHP) | 121
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 121