### Summary

Design Name | WarpSE
Fitting Status | Successful
Software Version | P.20131013
Device Used | XC95144XL-10-TQ100
Date | 3-26-2023, 4:30AM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
118/144 (82%) | 384/720 (54%) | 93/144 (65%) | 71/81 (88%) | 224/432 (52%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 32 | 32
Output | 35 | 35
Bidirectional | 1 | 1
GCK | 3 | 3
GTS | 0 | 0
GSR | 0 | 0

Pin Type | Used | Total
--- | --- | ---
I/O | 65 | 74
GCK/IO | 3 | 3
GTS/IO | 3 | 4
GSR/IO | 0 | 1

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | C16M
Signal mapped onto global clock net (GCK2) | C8M
Signal mapped onto global clock net (GCK3) | FCLK

##### POWER DATA

Macrocells in high performance mode (MCHP) | 118
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 118