# Hello World Example

Starts a FreeRTOS task to print "Hello World"

See the README.md file in the upper level 'examples' directory for more information about examples.

### LED Error codes

| Color | Status | Description             |
|-------|--------|-------------------------|
| Green | On     | Quack is running        |
| Green | Off    | No power                |
| Green | Fast   | Quack is starting up    |
| Green | Slow   | Mouse battery low       |
| Blue  | Off    | Bluetooth disabled      |
| Blue  | On     | Bluetooth connected     |
| Blue  | Fast   | Bluetooth starting up   |
| Blue  | Slow   | Bluetooth not connected |
| Amber | Pulse  | Mouse activity          |
| Amber | Slow   | ADB mouse not detected  |
| Red   | Off    | No errors detected      |
| Red   | On     | Configuration error     |
| Red   | Pulse  | Invalid mouse data*     |
