(module "Connector:Apple II Expansion Edge Connector" (layer F.Cu) (tedit 5CA41682)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Apple II Expansion Edge Connector" (at 9.652 -5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "26 GND" (at 45.974 10.922 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "27 DMA IN" (at 42.799 11.43 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "28 INT IN" (at 40.386 11.303 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "29 _NMI" (at 38.1 10.922 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "30 _IRQ" (at 35.687 10.922 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "31 _RES" (at 33.02 10.922 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "32 _INH" (at 30.607 10.922 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "33 -12V" (at 27.813 11.176 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "34 -5V" (at 25.527 10.922 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "35 N.C." (at 23.368 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "36 7M" (at 20.701 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "37 Q3" (at 18.161 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "38 @1" (at 15.621 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "39 USER 1" (at 12.192 11.43 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "40 @0" (at 10.414 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "41 _DEVICE SELECT" (at 5.334 13.335 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "42 D7" (at 5.461 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "43 D6" (at 2.921 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "44 D5" (at 0.508 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "45 D4" (at -2.159 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "46 D3" (at -4.699 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "47 D2" (at -7.239 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "48 D1" (at -9.906 10.541 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "25 +5V" (at 48.26 -0.635 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "24 DMA OUT" (at 46.609 -1.524 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "23 INT OUT" (at 43.942 -1.397 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "22 _DMA" (at 40.767 -0.762 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "21 RDY" (at 37.973 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "20 _I/O STROBE" (at 37.084 -2.413 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "19 N.C." (at 32.893 -0.635 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "18 R/W" (at 30.48 -0.635 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "16 A14" (at 25.273 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "17 A15" (at 27.813 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "14 A12" (at 20.193 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "15 A13" (at 22.733 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "13 A11" (at 17.653 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "12 A10" (at 15.113 -0.508 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "11 A9" (at 12.319 -0.254 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "10 A8" (at 9.779 -0.254 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_poly (pts (xy 48.895 8.89) (xy 48.895 1.27) (xy -15.875 1.27) (xy -15.875 8.89)) (layer B.Mask) (width 0.15))
  (fp_poly (pts (xy 48.895 8.89) (xy 48.895 1.27) (xy -15.875 1.27) (xy -15.875 8.89)) (layer F.Mask) (width 0.15))
  (fp_text user "50 +12V" (at -15.494 11.43 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "1 _I/O SELECT" (at -11.303 -2.032 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "3 A1" (at -8.128 -0.127 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "5 A3" (at -3.048 0 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "4 A2" (at -5.588 0.127 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "49 D0" (at -12.446 10.668 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "2 A0" (at -10.668 -0.127 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "8 A6" (at 4.445 0 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "6 A4" (at -0.635 0 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "9 A7" (at 6.985 0 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_text user "7 A5" (at 1.905 0 45) (layer F.Fab)
    (effects (font (size 0.762 0.762) (thickness 0.127)))
  )
  (fp_line (start -15.875 1.27) (end -16.51 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -15.875 7.62) (end -15.875 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start 48.895 1.27) (end 49.53 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start 48.895 7.62) (end 48.895 1.27) (layer F.SilkS) (width 0.15))
  (pad 50 connect roundrect (at -13.97 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 49 connect roundrect (at -11.43 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 48 connect roundrect (at -8.89 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 47 connect roundrect (at -6.35 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 46 connect roundrect (at -3.81 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 45 connect roundrect (at -1.27 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 44 connect roundrect (at 1.27 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 43 connect roundrect (at 3.81 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 42 connect roundrect (at 6.35 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 41 connect roundrect (at 8.89 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 40 connect roundrect (at 11.43 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 39 connect roundrect (at 13.97 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 37 connect roundrect (at 19.05 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 38 connect roundrect (at 16.51 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 36 connect roundrect (at 21.59 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 35 connect roundrect (at 24.13 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 34 connect roundrect (at 26.67 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 33 connect roundrect (at 29.21 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 32 connect roundrect (at 31.75 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 31 connect roundrect (at 34.29 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 30 connect roundrect (at 36.83 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 29 connect roundrect (at 39.37 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 28 connect roundrect (at 41.91 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 27 connect roundrect (at 44.45 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 26 connect roundrect (at 46.99 5.08) (size 1.27 7.62) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
  (pad 25 connect roundrect (at 46.99 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 24 connect roundrect (at 44.45 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 23 connect roundrect (at 41.91 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 22 connect roundrect (at 39.37 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 21 connect roundrect (at 36.83 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 20 connect roundrect (at 34.29 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 19 connect roundrect (at 31.75 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 18 connect roundrect (at 29.21 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 17 connect roundrect (at 26.67 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 16 connect roundrect (at 24.13 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 15 connect roundrect (at 21.59 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 14 connect roundrect (at 19.05 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 13 connect roundrect (at 16.51 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 12 connect roundrect (at 13.97 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 11 connect roundrect (at 11.43 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 10 connect roundrect (at 8.89 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 9 connect roundrect (at 6.35 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 8 connect roundrect (at 3.81 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 7 connect roundrect (at 1.27 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 6 connect roundrect (at -1.27 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 5 connect roundrect (at -3.81 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 4 connect roundrect (at -6.35 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 3 connect roundrect (at -8.89 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 2 connect roundrect (at -11.43 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 1 connect roundrect (at -13.97 5.08) (size 1.27 7.62) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
)
